{"text_format":"3","workbook":"xls","n_sheets":12,"sheets":["封-2_招标控制价","扉-2_招标控制价","表-01_总说明","表-02_建设项目招标控制价汇总表","表-04_单位工程招标控制价汇总表","表-08_分部分项工程和单价措施项目清单与计价表","表-09_工程量清单综合单价分析表","表-11_总价措施项目清单与计价表","表-12_其他项目清单与计价汇总表","表-15_规费、增值税计价表","主要材料及价格表(有信息价)","表-09_工程量清单综合单价分析表(主材)"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"封-2_招标控制价","index":0,"n_rows":12,"n_cols":4,"rows_kept":12,"merged":[[0,1,0,2],[1,1,1,3],[2,2,3,2],[5,2,6,2],[8,1,8,3],[9,1,9,2],[10,0,10,1],[10,2,10,4]],"flags":["formulas_cached_only"]}
[null,"广西中医药大学教师教学发展中心装修工程",null,"工程"]
[null,"招 标 控 制 价"]
[null,null,"广西中医药大学"]
[null,"招  标  人:"]
[null,null,"(单位盖章)"]
[null,null,"广西华寅工程造价咨询有限公司"]
[null,"造价咨询人:"]
[null,null,"(单位盖章)"]
[null,"2021年06月30日"]
[null,"软件名称及版本号：博奥清单计价软件V17（版本号：17.0.01）\r\n工程计价软件测评合格编号：2016J02\r\n"]
[]
[{"$nulls":3},"封-2"]

{"sheet":"扉-2_招标控制价","index":1,"n_rows":46,"n_cols":9,"rows_kept":46,"merged":[[1,1,1,6],[5,1,5,7],[11,0,11,1],[11,3,11,7],[13,3,14,7],[18,2,19,4],[18,6,19,8],[19,0,19,1],[20,2,20,4],[20,6,20,8],[24,0,24,1],[24,2,25,4],[24,6,25,8],[25,0,25,1],[26,2,26,4],[26,6,26,8],[30,2,31,4],[30,6,31,8],[31,0,31,1],[32,2,32,4],[32,6,32,8],[37,0,37,1],[37,2,37,4],[37,6,37,8],[42,2,42,6]],"flags":["formulas_cached_only"]}
[]
[null,"广西中医药大学教师教学发展中心装修工程",{"$nulls":5},"工程"]
[]
[]
[]
[null,"招 标 控 制 价"]
[]
[]
[]
[]
[]
["  招标控制价",null,"(小写):","1964349.3元"]
[]
[{"$nulls":3},"壹佰玖拾陆万肆仟叁佰肆拾玖元叁角整"]
[null,null,"(大写):"]
[]
[]
[]
[null,null,"广西中医药大学",null,null,"工程造价  ","广西华寅工程造价咨询有限公司"]
["  招  标  人:",{"$nulls":4},"咨 询 人："]
[null,null,"（单位盖章）",{"$nulls":3},"（单位资质专用章）"]
[]
[]
[]
["  法定代表人 ",{"$nulls":4},"法定代表人  "]
["或其授权人：",{"$nulls":4},"或其授权人："]
[null,null,"（签字或盖章）",{"$nulls":3},"（签字或盖章）"]
[]
[]
[]
[]
["编  制  人：",{"$nulls":4},"复  核  人："]
["                 ",null,"（造价人员签字）",{"$nulls":3},"(造价工程师签字盖专用章)"]
[]
[]
[]
[]
["  编 制 时 间:",null,"2021年06月30日",null,null,"复 核 时 间："]
{"$rows_empty":7}
[{"$nulls":8},"扉-2"]

{"sheet":"表-01_总说明","index":2,"n_rows":38,"n_cols":3,"rows_kept":38,"merged":[[0,0,0,2],[2,0,36,2]],"flags":["formulas_cached_only"]}
["总  说  明"]
["工程名称:","广西中医药大学教师教学发展中心装修工程","第1页 共1页"]
["一、工程概况：\r\n    工程名称：广西中医药大学教师教学发展中心装修工程\r\n    项目内容：室内装修、水电、消防等\r\n    本项目位于广西壮族自治区首府南宁五合大道13号广西中医药大学（仙葫校区）,校区临近五合大道、仙葫大道。\r\n    二、编制依据：\r\n    （1）施工图设计文件。\r\n    （2）(GB5050-2013)《建设工程工程量清单计价规范》、(GB50500-2013)《建设工程工程量清单计价规范广西壮族自治区实施细则》。\r\n   （3）2013年《广西壮族自治区建筑装修装修工程消耗量定额》、2015年《广西壮族自治区安装工程消耗量定额》、2011年《广西壮族自治区拆除工程消耗量定额》相应费用定额\r\n   （4）桂建标[2016]16号关于颁布2016年《广西壮族自治区建设工程费用定额》的通知。\r\n   （5）桂建标字[2018]19号文《关于调整建设工程定额人工费及有关费率的通知》。\r\n   （6）桂建标[2016]17号《自治区住房城乡建设厅关于建筑业实施营业税改增值税后广西壮族自治区建设工程计价依据调整的通知》。\r\n   （7）《自治区住房城乡建设部办公厅关于重新调整建设工程计价依据增值税税率通知》(建办标函[2019]193号)。\r\n   （8）本工程材料价按《南宁市建设工程造价信息》2021年第3期南宁市信息价确定。信息价中没有的材料价按市场中档价格。\r\n    三、其他说明：\r\n    （1）弃土运距暂按10km计算；\r\n    \r\n"]
{"$rows_empty":34}
[null,"表-01"]

{"sheet":"表-02_建设项目招标控制价汇总表","index":3,"n_rows":35,"n_cols":5,"rows_kept":35,"merged":[[0,0,0,4],[1,0,1,3],[1,4,1,4],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,3,2,4],[3,3,4,3]],"flags":["formulas_cached_only"]}
["建设项目招标控制价汇总表"]
["工程名称:广西中医药大学教师教学发展中心装修工程",{"$nulls":3},"第1页 共1页"]
["序号","单项工程名称","金额(元)","其中:(元)"]
[{"$nulls":3},"暂估价","安全文明"]
[{"$nulls":4},"施工费"]
["1.1","广西中医药大学教师教学发展中心装修工程",{"v":1964349.3,"d":"1964349.30"},null,78506.49]
[null,"        招标控制价合计",{"v":1964349.3,"d":"1964349.30"},null,78506.49]
{"$rows_empty":27}
[{"$nulls":4},"表-02"]

{"sheet":"表-04_单位工程招标控制价汇总表","index":4,"n_rows":84,"n_cols":4,"rows_kept":84,"merged":[[0,0,0,3],[1,0,1,2],[42,0,42,3],[43,0,43,2]],"flags":["formulas_cached_only"]}
["单位工程招标控制价汇总表"]
["工程名称:广西中医药大学教师教学发展中心装修工程",null,null,"第1页 共2页"]
["序号","汇总内容","金额(元)","备注"]
[null,"广西中医药大学教师教学发展中心装修工程-拆除"]
["1","分部分项工程和单价措施项目清单计价合计",4005.36]
[" 1.1","其中:暂估价"]
["2","总价措施项目清单计价合计",82.58]
[" 2.1","其中:安全文明施工费",{"v":73.4,"d":"73.40"}]
["3","其他项目清单计价合计"]
["4","税前项目清单计价合计"]
["5","规费、税金项目清单计价合计",785.36]
[" 5.1","其中:增值税",141.31]
["6","工程总造价=1+2+3+4+5",{"v":4873.3,"d":"4873.30"}]
[null,"广西中医药大学教师教学发展中心装修工程-装饰装修"]
["1","分部分项工程和单价措施项目清单计价合计",1051885.29]
[" 1.1","  其中:暂估价"]
["2","总价措施项目清单计价合计",77286.94]
[" 2.1","  其中:安全文明施工费",70662.35]
["3","其他项目清单计价合计"]
["4","税前项目清单计价合计",317194.12]
["5","规费",80966.04]
["6","增值税",137459.92]
["7","工程总造价=1+2+3+4+5+6",1664792.31]
[null,"广西中医药大学教师教学发展中心装修工程-安装"]
["1","分部分项工程和单价措施项目清单计价合计",94075.32]
[" 1.1","  其中:暂估价"]
["2","总价措施项目清单计价合计",4107.99]
[" 2.1","  其中:安全文明施工费",2316.59]
["3","其他项目清单计价合计"]
["4","税前项目清单计价合计"]
["5","规费",{"v":5935.7,"d":"5935.70"}]
["6","增值税",9370.71]
["7","工程总造价=1+2+3+4+5+6",113489.72]
[null,"广西中医药大学教师教学发展中心装修工程-消防"]
["1","分部分项工程和单价措施项目清单计价合计",{"v":142862.2,"d":"142862.20"}]
[" 1.1","  其中:暂估价"]
["2","总价措施项目清单计价合计",9694.03]
[" 2.1","  其中:安全文明施工费",5454.15]
["3","其他项目清单计价合计"]
["4","税前项目清单计价合计"]
["5","规费",13676.77]
[null,null," ","表-04"]
["单位工程招标控制价汇总表"]
["工程名称:广西中医药大学教师教学发展中心装修工程",null,null,"第2页 共2页"]
["序号","汇总内容","金额(元)","备注"]
["6","增值税",14960.97]
["7","工程总造价=1+2+3+4+5+6",181193.97]
[null,"工程项目汇总"]
["1","分部分项工程和单价措施项目清单计价合计",1292828.17]
["1.1","其中:暂估价"]
["2","总价措施项目清单计价合计",91171.54]
["2.1","其中:安全文明施工费",78506.49]
["3","其他项目清单计价合计"]
["4","税前项目清单计价合计",317194.12]
["5","规费、税金项目清单计价合计",785.36]
["5.1","其中:增值税",141.31]
["6","工程总造价=1+2+3+4+5",{"v":1964349.3,"d":"1964349.30"}]
["5","规费",100578.51]
["6","增值税",{"v":161791.6,"d":"161791.60"}]
{"$rows_empty":24}
[null,null," ","表-04"]

{"sheet":"表-08_分部分项工程和单价措施项目清单与计价表","index":5,"n_rows":689,"n_cols":8,"rows_kept":689,"merged":[[0,0,0,7],[1,0,1,5],[1,6,1,7],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,3,4,3],[2,4,4,4],[2,5,2,7],[3,5,4,5],[3,6,4,6],[41,0,41,7],[42,0,42,5],[42,6,42,7],[43,0,45,0],[43,1,45,1],[43,2,45,2],[43,3,45,3],[43,4,45,4],[43,5,43,7],[44,5,45,5],[44,6,45,6],[83,0,83,7],[84,0,84,5],[84,6,84,7],[85,0,87,0],[85,1,87,1],[85,2,87,2],[85,3,87,3],[85,4,87,4],[85,5,85,7],[86,5,87,5],[86,6,87,6],[124,0,124,7],[125,0,125,5],[125,6,125,7],[126,0,128,0],[126,1,128,1],[126,2,128,2],[126,3,128,3],[126,4,128,4],[126,5,126,7],[127,5,128,5],[127,6,128,6],[163,0,163,7],[164,0,164,5],[164,6,164,7],[165,0,167,0],[165,1,167,1],[165,2,167,2],[165,3,167,3],[165,4,167,4],[165,5,165,7],[166,5,167,5],[166,6,167,6],[201,0,201,7],[202,0,202,5],[202,6,202,7],[203,0,205,0],[203,1,205,1],[203,2,205,2],[203,3,205,3],[203,4,205,4],[203,5,203,7],[204,5,205,5],[204,6,205,6],[239,0,239,7],[240,0,240,5],[240,6,240,7],[241,0,243,0],[241,1,243,1],[241,2,243,2],[241,3,243,3],[241,4,243,4],[241,5,241,7],[242,5,243,5],[242,6,243,6],[279,0,279,7],[280,0,280,5],[280,6,280,7],[281,0,283,0],[281,1,283,1],[281,2,283,2],[281,3,283,3],[281,4,283,4],[281,5,281,7],[282,5,283,5],[282,6,283,6],[318,0,318,7],[319,0,319,5],[319,6,319,7],[320,0,322,0],[320,1,322,1],[320,2,322,2],[320,3,322,3],[320,4,322,4],[320,5,320,7],[321,5,322,5],[321,6,322,6],[361,0,361,7],[362,0,362,5],[362,6,362,7],[363,0,365,0],[363,1,365,1],[363,2,365,2],[363,3,365,3],[363,4,365,4],[363,5,363,7],[364,5,365,5],[364,6,365,6],[402,0,402,7],[403,0,403,5],[403,6,403,7],[404,0,406,0],[404,1,406,1],[404,2,406,2],[404,3,406,3],[404,4,406,4],[404,5,404,7],[405,5,406,5],[405,6,406,6],[440,0,440,7],[441,0,441,5],[441,6,441,7],[442,0,444,0],[442,1,444,1],[442,2,444,2],[442,3,444,3],[442,4,444,4],[442,5,442,7],[443,5,444,5],[443,6,444,6],[481,0,481,7],[482,0,482,5],[482,6,482,7],[483,0,485,0],[483,1,485,1],[483,2,485,2],[483,3,485,3],[483,4,485,4],[483,5,483,7],[484,5,485,5],[484,6,485,6],[522,0,522,7],[523,0,523,5],[523,6,523,7],[524,0,526,0],[524,1,526,1],[524,2,526,2],[524,3,526,3],[524,4,526,4],[524,5,524,7],[525,5,526,5],[525,6,526,6],[563,0,563,7],[564,0,564,5],[564,6,564,7],[565,0,567,0],[565,1,567,1],[565,2,567,2],[565,3,567,3],[565,4,567,4],[565,5,565,7],[566,5,567,5],[566,6,567,6],[605,0,605,7],[606,0,606,5],[606,6,606,7],[607,0,609,0],[607,1,609,1],[607,2,609,2],[607,3,609,3],[607,4,609,4],[607,5,607,7],[608,5,609,5],[608,6,609,6],[647,0,647,7],[648,0,648,5],[648,6,648,7],[649,0,651,0],[649,1,651,1],[649,2,651,2],[649,3,651,3],[649,4,651,4],[649,5,649,7],[650,5,651,5],[650,6,651,6]],"flags":["formulas_cached_only"]}
["分部分项工程和单价措施项目清单与计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程 ",{"$nulls":5},"第1页 共17页"]
["序\r\n\r\n号","项目编码","项目名称及\r\n项目特征描述","计量单位","工程量","金额(元)"]
[{"$nulls":5},"综合单价","合 价","其中："]
[{"$nulls":7},"暂估价"]
[null,null,"广西中医药大学教师教学发展中心装修工程-拆除",{"$nulls":3},4005.36]
[null,null,"分部分项工程",{"$nulls":3},4005.36]
[null,null,"G.1 人工拆除工程",{"$nulls":3},4005.36]
["1","011601001001","砖砌体拆除","","40.68",42.26,1719.14]
[null,null,"拆除方式:人工"]
[null,null,"砌体名称:砌块墙"]
["2","010103002001","余土弃置","","40.68",28.22,1147.99]
[null,null,"废弃料品种:拆除的废弃材料"]
[null,null,"运距:起步第1km"]
[null,null,"含装车、洒水、加盖费"]
["3","桂010103003001","土方运输每增(减)1km","","366.12",2.22,812.79]
[null,null,"废弃料品种:拆除的废弃材料"]
[null,null,"含装车、洒水、加盖费"]
[null,null,"工程量暂按增运9km计算，最终按实际结算"]
["4","010103002002","弃土场消纳费","","40.68",{"v":8,"d":"8.00"},325.44]
[null,null,"废弃料品种:拆除的废弃材料"]
[null,null,"     小    计",{"$nulls":3},4005.36]
[null,null,"     ∑人工费",{"$nulls":3},1960.37]
[null,null,"     ∑材料费",{"$nulls":3},325.44]
[null,null,"     ∑机械费",{"$nulls":3},1384.34]
[null,null,"     ∑管理费",{"$nulls":3},251.81]
[null,null,"     ∑利  润",{"$nulls":3},{"v":83.4,"d":"83.40"}]
[null,null,"     合    计",{"$nulls":3},4005.36]
[null,null,"     ∑人工费",{"$nulls":3},1960.37]
[null,null,"     ∑材料费",{"$nulls":3},325.44]
[null,null,"     ∑机械费",{"$nulls":3},1384.34]
[null,null,"     ∑管理费",{"$nulls":3},251.81]
[null,null,"     ∑利  润",{"$nulls":3},{"v":83.4,"d":"83.40"}]
[null,null,"广西中医药大学教师教学发展中心装修工程-装饰装修",{"$nulls":3},1051885.29]
[null,null,"分部分项工程",{"$nulls":3},1026979.26]
[null,null,"A.1 土（石）方工程",{"$nulls":3},7662.53]
["5","010103001001","回填方","","258.52",20.77,5369.46]
[null,null,"室内房心回填，高度20cm"]
["6","010103002003","校内取土","","258.52",8.87,2293.07]
[null,null,"运距:1km以内"]
[{"$nulls":7},"表-08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程 ",{"$nulls":5},"第2页 共17页"]
["序\r\n\r\n号","项目编码","项目名称及\r\n项目特征描述","计量单位","工程量","金额(元)"]
[{"$nulls":5},"综合单价","合 价","其中："]
[{"$nulls":7},"暂估价"]
[null,null,"A.3 砌筑工程",{"$nulls":3},67357.68]
["7","010402001001","砌块墙","","165.06",408.08,67357.68]
[null,null,"砖品种、规格、强度等级:蒸压加气砼砌块"]
[null,null,"墙体类型:直形"]
[null,null,"墙体厚度:200mm"]
[null,null,"砂浆种类、强度等级:混合砂浆M5.0"]
[null,null,"A.4 混凝土及钢筋混凝土工程",{"$nulls":3},16542.58]
["8","010502002001","构造柱","","4.11",531.67,2185.16]
[null,null,"混凝土种类:非泵送商品砼"]
[null,null,"混凝土强度等级:C20"]
["9","010503004001","圈梁","","3.62",{"v":520.8,"d":"520.80"},{"v":1885.3,"d":"1885.30"}]
[null,null,"混凝土种类:非泵送商品砼"]
[null,null,"混凝土强度等级:C20"]
["10","010503005001","过梁","","0.12",542.74,65.13]
[null,null,"混凝土种类:非泵送商品砼"]
[null,null,"混凝土强度等级:C20"]
["11","010507005001","扶手、压顶","","0.50",590.98,295.49]
[null,null,"混凝土种类:非泵送商品砼"]
[null,null,"混凝土强度等级:C20"]
["12","010515001001","现浇构件钢筋","t","0.667",6810.07,4542.32]
[null,null,"钢筋种类、规格:圆钢 φ10以内"]
[null,null,"品牌相当于或优于“柳钢”"]
["13","010515001002","现浇构件钢筋","t","0.375",7095.68,2660.88]
[null,null,"钢筋种类、规格:圆钢 φ10以上"]
[null,null,"品牌相当于或优于“柳钢”"]
["14","010515001003","现浇构件钢筋","t","0.034",7116.24,241.95]
[null,null,"钢筋种类、规格:螺纹钢 10以内"]
[null,null,"品牌相当于或优于“柳钢”"]
["15","桂010515011001","砌体加固筋","t","0.617",7562.96,4666.35]
[null,null,"钢筋种类、规格:圆钢 φ10以内"]
[null,null,"品牌相当于或优于“柳钢”"]
[null,null,"A.9 楼地面工程",{"$nulls":3},328542.87]
["16","010404001001","垫层","","152.35",458.29,69820.48]
[null,null,"夯实地面用C10混凝土垫高300mm,至±0.000"]
[null,null,"混凝土种类:非泵送商品砼"]
[null,null,"混凝土强度等级:C10"]
[{"$nulls":7},"表-08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程 ",{"$nulls":5},"第3页 共17页"]
["序\r\n\r\n号","项目编码","项目名称及\r\n项目特征描述","计量单位","工程量","金额(元)"]
[{"$nulls":5},"综合单价","合 价","其中："]
[{"$nulls":7},"暂估价"]
["17","011102003001","水磨石地砖地面","㎡","566.10",153.82,{"v":87077.5,"d":"87077.50"}]
[null,null,"素水泥结合层一道"]
[null,null,"30厚M10干硬性水泥砂浆结合层"]
[null,null,"表面撒水泥粉"]
[null,null,"面贴地砖1200×600,水泥擦缝(密缝拼接)"]
["18","011102003002","水磨石地砖地面","㎡","72.73",125.71,9142.89]
[null,null,"素水泥结合层一道"]
[null,null,"30厚M10干硬性水泥砂浆结合层"]
[null,null,"表面撒水泥粉"]
[null,null,"面贴地砖600×600,水泥擦缝(密缝拼接)"]
["19","011102003003","灰麻烧毛石地面","㎡","112.68",175.66,19793.37]
[null,null,"水泥浆一道(内掺建筑胶)"]
[null,null,"30厚M10干硬性水泥砂浆结合层"]
[null,null,"表面撒水泥粉"]
[null,null,"900×600×25灰麻烧毛石铺实拍平(踏步边缘开防滑槽),水泥浆擦缝"]
["20","011103001001","仿地毯块状地胶地面","㎡","522.66",190.39,99509.24]
[null,null,"水泥浆一道(内掺建筑胶)"]
[null,null,"30厚M10干硬性水泥砂浆结合层"]
[null,null,"水泥自流平界面剂"]
[null,null,"自流平找平层"]
[null,null,"2.0厚PVC方块地胶(胶粘剂粘贴)"]
["21","011104002001","浅木纹复合木地板","㎡","114.55",197.76,22653.41]
[null,null,"30厚M10干硬性水泥砂浆结合层"]
[null,null,"泡沫塑料衬垫"]
[null,null,"安装浅木纹复合木地板1200×150×12"]
[null,null,"阳角收口采用木地板同款同色成品铝合金收边条"]
[null,null,"品牌相当于或优于“富林”"]
["22","011104002002","浅木纹复合木地板（台阶）","㎡","12.47",242.19,3020.11]
[null,null,"30厚M10干硬性水泥砂浆结合层"]
[null,null,"泡沫塑料衬垫"]
[null,null,"安装浅木纹复合木地板1200×150×12"]
[null,null,"阳角收口采用木地板同款同色成品铝合金收边条"]
[null,null,"按展开面积计算"]
[null,null,"品牌相当于或优于“富林”"]
["23","011107001001","石材台阶面","㎡","23.04",422.02,9723.34]
[{"$nulls":7},"表-08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程 ",{"$nulls":5},"第4页 共17页"]
["序\r\n\r\n号","项目编码","项目名称及\r\n项目特征描述","计量单位","工程量","金额(元)"]
[{"$nulls":5},"综合单价","合 价","其中："]
[{"$nulls":7},"暂估价"]
[null,null,"台阶做法参见图集12J003 11B/B3"]
[null,null,"30厚灰麻花岗岩饰面台阶踏步(荔枝面)及踏步踢面"]
["24","010401012001","入口砌砖花池","","6.11",1277.01,7802.53]
[null,null,"150mm厚3:7灰土垫层"]
[null,null,"非粘土烧结砖砌筑"]
[null,null,"顶部及侧面30厚灰麻花岗岩饰面(荔枝面)（1:3水泥砂浆粘结层）"]
[null,null,"60厚C20混凝土压顶Φ6钢筋@200双向"]
[null,null,"A.10 墙、柱面工程",{"$nulls":3},376701.28]
["25","011201001001","墙面一般抹灰","㎡","606.16",18.61,11280.64]
[null,null,"13厚1:0.3:3水泥石膏砂浆打底扫毛"]
["26","011201001002","墙面一般抹灰","㎡","293.34",19.49,{"v":5717.2,"d":"5717.20"}]
[null,null,"15厚M10水泥砂浆找平"]
["27","011207001001","条形吸音板墙面","㎡","262.84",265.29,69728.82]
[null,null,"U50墙面轻钢龙骨@400mm"]
[null,null,"15厚阻燃板基层"]
[null,null,"1220×2440×15吸音板(竖条纹)"]
["28","011502002001","木质装饰线","m","14.17",7.67,108.68]
[null,null,"吸音板墙面80×15实木线条"]
["29","011502002002","木质装饰线","m","11.83",6.58,77.84]
[null,null,"15宽实木半圆线120×15"]
["30","011502002003","木质装饰线","m","14.80",5.53,81.84]
[null,null,"15宽实木半圆线60×15"]
["31","011105006001","冲压黑钛不锈钢踢脚线","㎡","22.88",277.45,6348.06]
[null,null,"15厚阻燃板基层"]
[null,null,"冲压1.0厚冲压黑钛不锈钢踢脚线用万能胶拍合安装"]
[null,null,"80mm高"]
[null,null,"品牌相当于或优于“海利”"]
["32","011105006002","不锈钢墙面","㎡","16.68",338.43,5645.01]
[null,null,"15厚阻燃板基层"]
[null,null,"1.0厚304#拉丝不锈钢饰面"]
[null,null,"品牌相当于或优于“海利”"]
["33","桂011204005001","内墙面干挂石材","㎡","123.29",280.63,34598.87]
[null,null,"5#镀锌角钢横向龙骨间距600×900mm(油丹红底漆两遍,防锈漆两遍)（另列清单）"]
[{"$nulls":7},"表-08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程 ",{"$nulls":5},"第5页 共17页"]
["序\r\n\r\n号","项目编码","项目名称及\r\n项目特征描述","计量单位","工程量","金额(元)"]
[{"$nulls":5},"综合单价","合 价","其中："]
[{"$nulls":7},"暂估价"]
[null,null,"不锈钢干挂件(油丹红底漆两遍,防锈漆两遍)"]
[null,null,"麻灰烧毛石600×900×30干挂(竖向密缝拼接、横向留自然缝)"]
["34","桂011204005002","外墙面干挂石材","㎡","23.85",413.23,9855.54]
[null,null,"5#镀锌角钢横向龙骨间距600×900mm(油丹红底漆两遍,防锈漆两遍)（另列清单）"]
[null,null,"不锈钢干挂件(油丹红底漆两遍,防锈漆两遍)"]
[null,null,"25厚黑金砂花岗岩饰面干挂(竖向密缝拼接、横向留自然缝)"]
["35","桂011204007001","块料墙面","㎡","33.76",105.04,3546.15]
[null,null,"15厚1:3水泥砂浆找平"]
[null,null,"3-4厚1:1水泥砂浆加水重20%专用瓷砖胶镶贴"]
[null,null,"面贴100×100釉面砖(工字拼贴),白水泥浆擦缝"]
[null,null,"品牌相当于或优于“东鹏”"]
["36","011502001001","金属装饰线","m","61.45",28.47,1749.48]
[null,null,"1.0厚冲压黑钛不锈钢收边，宽20mm，反边27.5mm"]
[null,null,"品牌相当于或优于“海利”"]
["37","011502001002","金属装饰线","m","24.96",10.96,273.56]
[null,null,"成品黑色铝合金工字收口条，高度同硬包厚度，约18mm高"]
[null,null,"品牌相当于或优于“海利”"]
["38","011502001003","金属装饰线","m","32.80",22.03,722.58]
[null,null,"1.0厚黑钛不锈钢包边，展开宽度85mm"]
[null,null,"品牌相当于或优于“海利”"]
["39","011502001004","金属装饰线","m","7.38",15.67,115.64]
[null,null,"部位：出入口铝塑板檐口处"]
[null,null,"1.0厚黑钛不锈钢，宽度50mm"]
[null,null,"品牌相当于或优于“海利”"]
["40","011207001002","墙面装饰板","㎡","72.38",349.34,25285.23]
[null,null,"U50轻钢龙骨"]
[null,null,"15厚阻燃夹板基层"]
[null,null,"面层：12厚钢化玻璃背蓝漆"]
[null,null,"品牌相当于或优于“南玻”"]
["41","011207001003","墙面装饰板","㎡","64.37",368.16,23698.46]
[null,null,"U50轻钢龙骨"]
[null,null,"15厚阻燃夹板基层"]
[{"$nulls":7},"表-08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程 ",{"$nulls":5},"第6页 共17页"]
["序\r\n\r\n号","项目编码","项目名称及\r\n项目特征描述","计量单位","工程量","金额(元)"]
[{"$nulls":5},"综合单价","合 价","其中："]
[{"$nulls":7},"暂估价"]
[null,null,"9厚阻燃夹板基层浅咖啡色仿布纹硬包"]
["42","桂011204005003","石材墙面","㎡","124.95",428.53,53544.82]
[null,null,"5#镀锌角钢横向龙骨间距600×900mm(油丹红底漆两遍,防锈漆两遍)（另列清单）"]
[null,null,"不锈钢干挂件(油丹红底漆两遍,防锈漆两遍)"]
[null,null,"25厚西班牙米黄大理石饰面干挂"]
[null,null,"部位：外墙及部分柱面、主入口"]
["43","桂011204007002","块料墙面","㎡","43.92",177.39,7790.97]
[null,null,"15厚1:3水泥砂浆找平"]
[null,null,"3-4厚1:1水泥砂浆加水重20%专用瓷砖胶镶贴"]
[null,null,"面贴400×800深灰色仿石材瓷砖,白水泥浆擦缝"]
[null,null,"部位：外墙面"]
[null,null,"品牌相当于或优于“东鹏”"]
["44","桂011204007003","块料墙面","㎡","46.79",357.71,16737.25]
[null,null,"25厚西班牙米黄大理石（密拼）"]
[null,null,"20厚1:3水泥砂浆结合层"]
[null,null,"部位：外墙窗底部"]
["45","011207001004","墙面装饰板","㎡","3.20",68.05,217.76]
[null,null,"20×20×2镀锌方通骨架@600(油丹红底漆两遍,防锈漆两遍)（另列清单）"]
[null,null,"12厚埃特板"]
["46","011207001005","墙面装饰板","㎡","133.51",189.09,25245.41]
[null,null,"配套金属轻钢龙骨架"]
[null,null,"9厚阻燃板基层"]
[null,null,"面封竹木纤维集成墙板(密缝拼接)，600宽×9厚"]
[null,null,"阳角采用配套25×25mmL型同款同色阳角线条"]
[null,null,"阴角采用配套27×16mm同款同色阴角线条"]
["47","011207001006","聚酯纤维吸音板","㎡","31.46",172.94,5440.69]
[null,null,"U50墙面轻钢龙骨@400mm"]
[null,null,"15厚阻燃板基层"]
[null,null,"600×2400×9聚酯纤维吸音板(横竖向留V型缝)"]
["48","011207001007","防潮纸面石膏板墙面","㎡","13.46",25.61,344.71]
[null,null,"40*20*2钢骨架@1000（另列清单）"]
[null,null,"9.5厚纸面石膏板"]
[{"$nulls":7},"表-08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程 ",{"$nulls":5},"第7页 共17页"]
["序\r\n\r\n号","项目编码","项目名称及\r\n项目特征描述","计量单位","工程量","金额(元)"]
[{"$nulls":5},"综合单价","合 价","其中："]
[{"$nulls":7},"暂估价"]
[null,null,"刮腻子油白色乳胶漆（另列清单）"]
["49","011207001008","黑钛不锈钢墙面","㎡","0.64",322.55,206.43]
[null,null,"展示厅立面P-07/A"]
[null,null,"15厚阻燃板基层"]
[null,null,"1.0厚黑钛不锈钢板"]
[null,null,"定制亚克力字体（另列清单）"]
[null,null,"品牌相当于或优于“海利”"]
["50","011304001001","墙面灯槽","㎡","8.92",134.88,1203.13]
[null,null,"15厚阻燃夹板基层"]
[null,null,"9.5厚防潮纸面石膏板"]
["51","011304001002","墙面灯槽","㎡","7.59",{"v":162.4,"d":"162.40"},1232.62]
[null,null,"15厚阻燃夹板基层"]
[null,null,"9厚竹木纤维集成墙板"]
["52","011204004001","钢骨架","t","1.841",13042.52,24011.28]
[null,null,"挂石板钢骨架"]
[null,null,"含油丹红底漆两遍,防锈漆两遍"]
[null,null,"品牌相当于或优于“柳钢”"]
["53","011204004002","钢骨架","t","3.212",13042.53,41892.61]
[null,null,"挂装饰板钢骨架"]
[null,null,"含油丹红底漆两遍,防锈漆两遍"]
[null,null,"品牌相当于或优于“柳钢”"]
[null,null,"A.11 天棚工程",{"$nulls":3},{"v":144752.6,"d":"144752.60"}]
["54","011302001001","防潮纸面石膏板吊顶","㎡","825.59",105.51,{"v":87108,"d":"87108.00"}]
[null,null,"Φ8螺纹吊杆"]
[null,null,"U60轻钢龙骨标准骨架(上人型):主龙骨中距900-1000,C型次龙骨中距450,横撑龙骨中距900"]
[null,null,"双层9.5厚纸面石膏板(或双层9.5厚冲孔纸面石膏板),自攻螺钉拧紧,螺丝眼刷防锈漆,再用石膏腻子点补"]
[null,null,"刮腻子三遍油乳胶漆三遍（另列清单）"]
["55","011302001002","矿棉板吊顶","㎡","29.04",94.56,2746.02]
[null,null,"φ8螺纹吊杆T型主骨中距600~1200mm,次骨间距@600mm"]
[null,null,"安装矿棉板1200×600×15"]
[null,null,"四周采用L型边龙骨收口"]
["56","011302001003","铝塑板天棚","㎡","242.29",161.45,39117.72]
[null,null,"5#镀锌角钢架,@600mm（另列清单）"]
[null,null,"15厚阻燃夹板基层"]
[{"$nulls":7},"表-08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程 ",{"$nulls":5},"第8页 共17页"]
["序\r\n\r\n号","项目编码","项目名称及\r\n项目特征描述","计量单位","工程量","金额(元)"]
[{"$nulls":5},"综合单价","合 价","其中："]
[{"$nulls":7},"暂估价"]
[null,null,"面贴4厚铝塑板1220×2440×4"]
[null,null,"横向密缝拼接,竖向留5mm缝填黑色结构胶"]
[null,null,"清单工程量按铝塑板展开面积计算"]
[null,null,"品牌相当于或优于“奥斯特”"]
["57","011302001004","防潮纸面石膏板窗帘盒","㎡","51.60",142.86,7371.58]
[null,null,"Φ8螺纹吊杆"]
[null,null,"U60轻钢龙骨标准骨架"]
[null,null,"15厚阻燃夹板基层"]
[null,null,"9.5厚纸面石膏板(或双层9.5厚冲孔纸面石膏板),自攻螺钉拧紧,螺丝眼刷防锈漆,再用石膏腻子点补"]
[null,null,"刮腻子三遍油无机乳胶漆三遍（另列清单）"]
["58","011302001005","天棚灯槽","㎡","33.43",{"v":135.9,"d":"135.90"},4543.14]
[null,null,"15厚阻燃夹板基层"]
[null,null,"9.5厚纸面石膏板(或双层9.5厚冲孔纸面石膏板),自攻螺钉拧紧,螺丝眼刷防锈漆,再用石膏腻子点补"]
[null,null,"刮腻子三遍油无机乳胶漆三遍（另列清单）"]
["59","010606013001","∟40×40×4mm镀锌角钢间距1100mm","t","0.329",11751.18,3866.14]
[null,null,"玻璃隔墙门连窗上部"]
[null,null,"品牌相当于或优于“柳钢”"]
[null,null,"A.12 门窗工程",{"$nulls":3},10267.51]
["60","010807001001","80系列深灰色铝合金平开窗","㎡","3.84",486.35,1867.58]
[null,null,"Low-E中空玻璃（5+9A+5）"]
[null,null,"洞口面积≤2㎡"]
[null,null,"含运输、安装、配件等全部内容"]
[null,null,"品牌相当于或优于“南南铝”"]
["61","010807001002","80系列深灰色铝合金固定窗","㎡","15.08",447.45,6747.55]
[null,null,"Low-E中空玻璃（5+9A+5）"]
[null,null,"洞口面积＞2㎡"]
[null,null,"含运输、安装、配件等全部内容"]
[null,null,"品牌相当于或优于“南南铝”"]
["62","桂010811002001","门窗周边塞缝","m","227.60",7.26,1652.38]
[null,null,"水泥砂浆1:2.5"]
[null,null,"A.13 油漆、涂料、裱糊工程",{"$nulls":3},63564.87]
["63","011406003001","墙面满刮腻子","㎡","468.02",{"v":16.1,"d":"16.10"},7535.12]
[null,null,"刮腻子三遍"]
[{"$nulls":7},"表-08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程 ",{"$nulls":5},"第9页 共17页"]
["序\r\n\r\n号","项目编码","项目名称及\r\n项目特征描述","计量单位","工程量","金额(元)"]
[{"$nulls":5},"综合单价","合 价","其中："]
[{"$nulls":7},"暂估价"]
["64","011406003002","天棚满刮腻子","㎡","910.62",17.83,16236.35]
[null,null,"刮腻子三遍"]
["65","011406001001","米白色乳胶漆","㎡","1378.64",15.94,21975.52]
[null,null,"封底涂料一道"]
[null,null,"乳液内墙涂料一道"]
[null,null,"乳胶涂料一道"]
[null,null,"品牌相当于或优于“多乐士”"]
["66","011406001002","米白色硅藻泥","㎡","396.20",33.75,13371.75]
[null,null,"封底涂料一道"]
[null,null,"米白色硅藻泥涂料一道"]
[null,null,"米白色硅藻泥一道"]
[null,null,"品牌相当于或优于“五棵松”"]
["67","011406001003","抹灰面油漆","㎡","381.97",11.64,4446.13]
[null,null,"原建筑天面喷黑漆"]
[null,null,"品牌相当于或优于“多乐士”"]
[null,null,"A.14 其他装饰工程",{"$nulls":3},11587.34]
["68","01B001","0.8厚镀锌铁皮","㎡","130.10",50.62,6585.66]
[null,null,"部位：外墙面铝塑板檐口顶面"]
["69","011508002001","定制不锈钢钛金发光字","个","8",114.49,915.92]
[null,null,"规格：800×800mm"]
["70","011508002002","定制不锈钢钛金发光字","个","32",53.74,1719.68]
[null,null,"规格：300×200mm"]
["71","011508002003","5厚亚克力字","个","8",{"v":49.4,"d":"49.40"},{"v":395.2,"d":"395.20"}]
[null,null,"规格：120×120mm"]
["72","011508002004","5厚亚克力字","个","32",39.05,{"v":1249.6,"d":"1249.60"}]
[null,null,"规格：60×40mm"]
["73","010810005001","窗帘轨","m","33.30",21.66,721.28]
[null,null,"     小    计",{"$nulls":3},1026979.26]
[null,null,"     ∑人工费",{"$nulls":3},233085.45]
[null,null,"     ∑材料费",{"$nulls":3},693242.83]
[null,null,"     ∑机械费",{"$nulls":3},14610.13]
[null,null,"     ∑管理费",{"$nulls":3},68399.37]
[null,null,"     ∑利  润",{"$nulls":3},17641.48]
[null,null,"单价措施项目",{"$nulls":3},24906.03]
[null,"011701","脚手架工程",{"$nulls":3},17779.61]
["74","桂011701001001","扣件式钢管外脚手架 双排 10m以内","㎡","522.25",21.74,11353.72]
["75","桂011701002001","扣件式钢管里脚手架 3.6m以上","㎡","770.49",8.34,6425.89]
[{"$nulls":7},"表-08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程 ",{"$nulls":5},"第10页 共17页"]
["序\r\n\r\n号","项目编码","项目名称及\r\n项目特征描述","计量单位","工程量","金额(元)"]
[{"$nulls":5},"综合单价","合 价","其中："]
[{"$nulls":7},"暂估价"]
[null,"011702","混凝土模板及支架(撑)",{"$nulls":3},6125.21]
["76","011702003001","构造柱 胶合板模板 木支撑[实际4.2]","㎡","49.50",55.51,2747.75]
["77","011702008001","圈梁 直形 胶合板模板 木支撑","㎡","36.63",39.87,1460.44]
["78","011702009001","过梁 胶合板模板 木支撑","㎡","2.16",69.15,149.36]
["79","011702027001","台阶 木模板木支撑","㎡","4.16",35.52,147.76]
["80","011702028001","扶手、压顶 木模板木支撑","m","48.50",{"v":33.4,"d":"33.40"},{"v":1619.9,"d":"1619.90"}]
[null,"011705","大型机械设备进出场及安拆",{"$nulls":3},1001.21]
["81","011705001001","履带式挖掘机 1以外 场外运输费","台次","1",1001.21,1001.21]
[null,null,"     小    计",{"$nulls":3},24906.03]
[null,null,"     ∑人工费",{"$nulls":3},13189.14]
[null,null,"     ∑材料费",{"$nulls":3},4796.06]
[null,null,"     ∑机械费",{"$nulls":3},1162.72]
[null,null,"     ∑管理费",{"$nulls":3},4583.29]
[null,null,"     ∑利  润",{"$nulls":3},1174.87]
[null,null,"     合    计",{"$nulls":3},1051885.29]
[null,null,"     ∑人工费",{"$nulls":3},246274.59]
[null,null,"     ∑材料费",{"$nulls":3},698038.89]
[null,null,"     ∑机械费",{"$nulls":3},15772.85]
[null,null,"     ∑管理费",{"$nulls":3},72982.66]
[null,null,"     ∑利  润",{"$nulls":3},18816.35]
[null,null,"广西中医药大学教师教学发展中心装修工程-安装",{"$nulls":3},94075.32]
[null,null,"分部分项工程",{"$nulls":3},94075.32]
[null,null,"B4 电气设备安装工程",{"$nulls":3},94075.32]
["82","030404017001","ALzm配电箱","台","1",852.52,852.52]
[null,null,"底边距地1.5m安装"]
[null,null,"品牌相当于或优于“正泰”"]
[null,null,"箱内元件：13个断路器,1个接触器，1个熔断器，1个时控开关"]
["83","030404017002","ALG 公共照明配电箱","台","1",916.72,916.72]
[null,null,"底边距地1.5m安装"]
[null,null,"品牌相当于或优于“正泰”"]
[null,null,"箱内元件：1个双电源自动转换开关，9个断路器，1个智能照明控制开关"]
["84","030404017003","AL1-4配电箱","台","7",416.72,2917.04]
[null,null,"底边距地1.5m安装"]
[null,null,"品牌相当于或优于“正泰”"]
[null,null,"箱内元件：AL1、2-5个断路器,AL3-6个断路器，AL4-8个断路器"]
[{"$nulls":7},"表-08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程 ",{"$nulls":5},"第11页 共17页"]
["序\r\n\r\n号","项目编码","项目名称及\r\n项目特征描述","计量单位","工程量","金额(元)"]
[{"$nulls":5},"综合单价","合 价","其中："]
[{"$nulls":7},"暂估价"]
["85","030404017004","AL5配电箱","台","1",616.72,616.72]
[null,null,"底边距地1.5m安装"]
[null,null,"品牌相当于或优于“正泰”"]
[null,null,"箱内元件：15个断路器"]
["86","030404017005","AP-KT配电箱","台","1",316.72,316.72]
[null,null,"底边距地1.5m安装"]
[null,null,"品牌相当于或优于“正泰”"]
["87","030411002001","防火金属线槽（MR）:100×100","m","63.98",73.04,{"v":4673.1,"d":"4673.10"}]
[null,null,"梁底下200mm安装敷设"]
[null,null,"品牌相当于或优于“南宁乔顿”"]
["88","030411001001","吊顶内敷设 扣压式(KBG)、紧定式(JDG)电气钢导管规格 40","m","7.31",21.28,155.56]
[null,null,"品牌相当于或优于“雄塑”"]
["89","030411001002","吊顶内敷设 扣压式(KBG)、紧定式(JDG)电气钢导管规格 32","m","80.74",19.68,1588.96]
[null,null,"品牌相当于或优于“雄塑”"]
["90","030411001003","吊顶内敷设 扣压式(KBG)、紧定式(JDG)电气钢导管规格 25","m","26.22",18.34,480.87]
[null,null,"品牌相当于或优于“雄塑”"]
["91","030411001004","砖、混凝土结构暗配 扣压式(KBG)、紧定式(JDG)电气钢导管规格 20","m","1291.58",11.61,14995.24]
[null,null,"品牌相当于或优于“雄塑”"]
["92","030411004001","线槽内穿铜芯线WDZ-BYJ-0.45/0.75kV-6m㎡","m","803.27",5.89,4731.26]
[null,null,"品牌相当于或优于“银杉”"]
["93","030411004002","管道内穿铜芯线WDZ-BYJ-0.45/0.75kV-6m㎡","m","197.46",5.76,1137.37]
[null,null,"品牌相当于或优于“银杉”"]
["94","030411004003","线槽内穿配铜芯线WDZ-BYJ-0.45/0.75kV-10m㎡","m","228.90",9.71,2222.62]
[null,null,"品牌相当于或优于“银杉”"]
["95","030411004004","管道内穿铜芯线WDZ-BYJ-0.45/0.75kV-10m㎡","m","134.71",9.76,1314.77]
[null,null,"品牌相当于或优于“银杉”"]
["96","030411004005","管道内穿配铜芯线WDZ-BYJ-0.45/0.75kV-2.5m㎡","m","3890.82",2.53,9843.77]
[null,null,"品牌相当于或优于“银杉”"]
["97","030411004006","线槽内穿配铜芯线WDZ-BYJ-0.45/0.75kV-2.5m㎡","m","101.06",2.69,271.85]
[null,null,"品牌相当于或优于“银杉”"]
["98","030411004007","管道内穿配铜芯线WDZ-BYJ-0.45/0.75kV-4m㎡","m","1060.62",3.43,3637.93]
[null,null,"品牌相当于或优于“银杉”"]
[{"$nulls":7},"表-08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程 ",{"$nulls":5},"第12页 共17页"]
["序\r\n\r\n号","项目编码","项目名称及\r\n项目特征描述","计量单位","工程量","金额(元)"]
[{"$nulls":5},"综合单价","合 价","其中："]
[{"$nulls":7},"暂估价"]
["99","030413002001","凿(压)槽及恢复","m","87.80",13.54,1188.81]
["100","030404035001","墙面插座","套","55",27.43,1508.65]
[null,null,"单、三相暗插座 单相暗插座10A 5孔"]
[null,null,"底边距地0.3m"]
[null,null,"品牌相当于或优于“西蒙”"]
["101","030404035002","安全型地面插座","套","21",192.85,4049.85]
[null,null,"单、三相暗插座 单相暗插座10A 5孔"]
[null,null,"嵌地安装"]
[null,null,"品牌相当于或优于“西蒙”"]
["102","030404035003","安全型插座","套","9",27.43,246.87]
[null,null,"单、三相暗插座 单相暗插座10A 5孔"]
[null,null,"投影机用，壁装"]
[null,null,"品牌相当于或优于“西蒙”"]
["103","030404035004","安全型插座","套","3",27.43,82.29]
[null,null,"单、三相暗插座 单相暗插座10A 5孔"]
[null,null,"电视机用，底边距地1.2m"]
[null,null,"品牌相当于或优于“西蒙”"]
["104","030404035005","防水插座","套","2",32.71,65.42]
[null,null,"单、三相暗插座 单相暗插座10A 5孔"]
[null,null,"配防溅盒，底边距地1.2m"]
[null,null,"品牌相当于或优于“西蒙”"]
["105","030404034001","开关、按钮、插座安装 开关及按钮 跷板暗开关(单控) 单联","套","1",20.08,20.08]
[null,null,"品牌相当于或优于“西蒙”"]
["106","030404034002","开关、按钮、插座安装 开关及按钮 跷板暗开关(单控) 双联","套","10",23.27,{"v":232.7,"d":"232.70"}]
[null,null,"品牌相当于或优于“西蒙”"]
["107","030404034003","开关、按钮、插座安装 开关及按钮 跷板暗开关(单控) 三联","套","12",32.42,389.04]
[null,null,"品牌相当于或优于“西蒙”"]
["108","030404034004","开关、按钮、插座安装 开关及按钮 跷板暗开关(双控) 单联","套","2",19.83,39.66]
[null,null,"品牌相当于或优于“西蒙”"]
["109","030404034005","开关、按钮、插座安装 开关及按钮 跷板暗开关(双控) 双联","套","4",28.97,115.88]
[null,null,"品牌相当于或优于“西蒙”"]
["110","030412001001","6寸LED筒灯","套","27",64.41,1739.07]
[null,null,"15W   ~220V  1300lm  4000K"]
[null,null,"嵌入安装"]
[null,null,"品牌相当于或优于“三极雄光”"]
[{"$nulls":7},"表-08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程 ",{"$nulls":5},"第13页 共17页"]
["序\r\n\r\n号","项目编码","项目名称及\r\n项目特征描述","计量单位","工程量","金额(元)"]
[{"$nulls":5},"综合单价","合 价","其中："]
[{"$nulls":7},"暂估价"]
["111","030412001002","8寸LED筒灯","套","10",66.43,{"v":664.3,"d":"664.30"}]
[null,null,"18W   ~220V  1500lm  4000K"]
[null,null,"嵌入安装"]
[null,null,"品牌相当于或优于“三极雄光”"]
["112","030412001003","LED可调式天花小射灯","套","66",60.94,4022.04]
[null,null,"15W   ～220V  1062lm  4000K（24°）"]
[null,null,"嵌入安装"]
[null,null,"品牌相当于或优于“三极雄光”"]
["113","030412001004","双头LED格栅射灯","套","6",101.34,608.04]
[null,null,"2*15W   ～220V  2150lm  （24°）"]
[null,null,"嵌入安装"]
[null,null,"品牌相当于或优于“三极雄光”"]
["114","030412001005","成品工艺吊灯","套","10",151.55,{"v":1515.5,"d":"1515.50"}]
[null,null,"  15W  ~220V 1300lm(吊线式)"]
[null,null,"底距地3.2/2.2m"]
[null,null,"品牌相当于或优于“三极雄光”"]
["115","030412001006","LED平面灯盘(300x1200mm)","套","63",191.95,12092.85]
[null,null,"2x16W  ~220V 2250lm(吊线式)"]
[null,null,"品牌相当于或优于“三极雄光”"]
["116","030412001007","LED平面灯盘(300x1200mm)","套","32",192.54,6161.28]
[null,null,"35W  ~220V 2000lm"]
[null,null,"嵌入安装"]
[null,null,"品牌相当于或优于“三极雄光”"]
["117","030412001008","LED平面灯盘(300x300mm)","套","6",108.71,652.26]
[null,null,"12W  ~220V  800lm"]
[null,null,"嵌入安装",null,"5"]
[null,null,"品牌相当于或优于“三极雄光”"]
["118","030412001009","LED高压软灯带","m","271.54",29.49,8007.71]
[null,null,"PAK544217 AC200V/灯盒内安装8W/m/4000K/发光角度140°/光通量(450lm/m)"]
[null,null,"壁装"]
[null,null,"品牌相当于或优于“三极雄光”"]
[null,null,"     小    计",{"$nulls":3},94075.32]
[null,null,"     ∑人工费",{"$nulls":3},18783.86]
[null,null,"     ∑材料费",{"$nulls":3},66339.59]
[null,null,"     ∑机械费",{"$nulls":3},329.91]
[{"$nulls":7},"表-08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程 ",{"$nulls":5},"第14页 共17页"]
["序\r\n\r\n号","项目编码","项目名称及\r\n项目特征描述","计量单位","工程量","金额(元)"]
[{"$nulls":5},"综合单价","合 价","其中："]
[{"$nulls":7},"暂估价"]
[null,null,"     ∑管理费",{"$nulls":3},5870.85]
[null,null,"     ∑利  润",{"$nulls":3},2751.12]
[null,null,"     合    计",{"$nulls":3},94075.32]
[null,null,"     ∑人工费",{"$nulls":3},18783.86]
[null,null,"     ∑材料费",{"$nulls":3},66339.59]
[null,null,"     ∑机械费",{"$nulls":3},329.91]
[null,null,"     ∑管理费",{"$nulls":3},5870.85]
[null,null,"     ∑利  润",{"$nulls":3},2751.12]
[null,null,"广西中医药大学教师教学发展中心装修工程-消防",{"$nulls":3},{"v":142862.2,"d":"142862.20"}]
[null,null,"分部分项工程",{"$nulls":3},{"v":142862.2,"d":"142862.20"}]
[null,null,"消火栓系统",{"$nulls":3},19108.24]
["119","030901002001","消火栓热镀锌钢管及管件安装","m","86.31",{"v":138.5,"d":"138.50"},11953.94]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：沟槽连接"]
[null,null,"规格型号：DN100"]
[null,null,"品牌相当于或优于“雄塑”"]
["120","031002001001","管道支架制作安装","kg","96.93",{"v":20.6,"d":"20.60"},1996.76]
[null,null,"支架的材质不详，暂按40*4热镀锌角钢计，结算按实调整"]
[null,null,"面刷防锈漆二道，红色调和漆二道"]
["121","030901010001","室内消火栓","套","6",859.59,5157.54]
[null,null,"安装方式：半暗装型"]
[null,null,"规格型号：箱子尺寸1000X700X240mm"]
[null,null,"配直流水枪1支,规格为:65mmX19mm;消防龙带:材质用衬胶。口径65mm 长度及条数:25m长配1条。"]
[null,null,"自动喷淋系统",{"$nulls":3},49830.32]
["122","030901001001","喷淋热镀锌钢管及管件安装","m","31.00",219.21,6795.51]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：沟槽连接"]
[null,null,"规格型号：DN150"]
[null,null,"品牌相当于或优于“雄塑”"]
["123","030901001002","喷淋热镀锌钢管及管件安装","m","4.25",202.52,860.71]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：沟槽连接"]
[null,null,"规格型号：DN125"]
[null,null,"品牌相当于或优于“雄塑”"]
["124","030901001003","喷淋热镀锌钢管及管件安装","m","8.59",{"v":138.5,"d":"138.50"},1189.72]
[{"$nulls":7},"表-08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程 ",{"$nulls":5},"第15页 共17页"]
["序\r\n\r\n号","项目编码","项目名称及\r\n项目特征描述","计量单位","工程量","金额(元)"]
[{"$nulls":5},"综合单价","合 价","其中："]
[{"$nulls":7},"暂估价"]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：沟槽连接"]
[null,null,"规格型号：DN100"]
[null,null,"品牌相当于或优于“雄塑”"]
["125","030901001004","喷淋热镀锌钢管及管件安装","m","35.26",108.08,{"v":3810.9,"d":"3810.90"}]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：沟槽连接"]
[null,null,"规格型号：DN80"]
[null,null,"品牌相当于或优于“雄塑”"]
["126","030901001005","喷淋热镀锌钢管及管件安装","m","10.65",108.08,1151.05]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：沟槽连接"]
[null,null,"规格型号：DN65"]
[null,null,"品牌相当于或优于“雄塑”"]
["127","030901001006","喷淋热镀锌钢管及管件安装","m","27.81",73.08,2032.35]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：螺纹连接"]
[null,null,"规格型号：DN50"]
[null,null,"品牌相当于或优于“雄塑”"]
["128","030901001007","喷淋热镀锌钢管及管件安装","m","36.33",62.97,{"v":2287.7,"d":"2287.70"}]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：螺纹连接"]
[null,null,"规格型号：DN40"]
[null,null,"品牌相当于或优于“雄塑”"]
["129","030901001008","喷淋热镀锌钢管及管件安装","m","201.75",54.15,10924.76]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：螺纹连接"]
[null,null,"规格型号：DN32"]
[null,null,"品牌相当于或优于“雄塑”"]
["130","030901001009","喷淋热镀锌钢管及管件安装","m","190.09",50.05,{"v":9514,"d":"9514.00"}]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：螺纹连接"]
[null,null,"规格型号：DN25"]
[null,null,"品牌相当于或优于“雄塑”"]
["131","031002001002","管道支架","kg","290.33",{"v":20.6,"d":"20.60"},{"v":5980.8,"d":"5980.80"}]
[null,null,"管道支架制作安装"]
[{"$nulls":7},"表-08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程 ",{"$nulls":5},"第16页 共17页"]
["序\r\n\r\n号","项目编码","项目名称及\r\n项目特征描述","计量单位","工程量","金额(元)"]
[{"$nulls":5},"综合单价","合 价","其中："]
[{"$nulls":7},"暂估价"]
[null,null,"面刷防锈漆二道，红色调和漆二道"]
["132","030901003001","玻璃球闭式喷头DN15,喷头动作温度68℃","个","159",30.23,4806.57]
[null,null,"安装方式  有吊顶"]
["133","030901008001","末端试水阀","组","1",{"v":40.4,"d":"40.40"},{"v":40.4,"d":"40.40"}]
[null,null,"规格型号 DN25"]
["134","030901008002","末端试水装置","组","1",296.23,296.23]
[null,null,"规格型号 DN25"]
["135","030905002001","水灭火控制装置调试","点","1",139.62,139.62]
[null,null,"火灾自动报警系统",{"$nulls":3},63057.66]
["136","030904001001","编码型感烟探测器","个","32",262.66,8405.12]
[null,null,"安装方式 吸顶"]
["137","030904003001","编码型手动报警按钮 带电话插孔","个","4",277.82,1111.28]
[null,null,"1.安装方式:距地1.4m安装"]
["138","030904008001","短路隔离器","个","2",271.86,543.72]
["139","030904007001","火灾警报扬声器","个","10",101.75,{"v":1017.5,"d":"1017.50"}]
[null,null,"1.功率:12V 3W"]
[null,null,"2.安装方式:吸顶"]
["140","030904005001","火灾声光警报器","个","4",307.36,1229.44]
[null,null,"1.安装方式:距地2.4m安装"]
["141","030904003002","消防栓起泵按钮","个","6",237.42,1424.52]
["142","030411004008","管内穿报警线 ZR-RVS-2x1.0","m","597.97",4.33,2589.21]
[null,null,"品牌相当于或优于“银杉”"]
["143","030411004009","管内穿电源线 NH-BV-750V-4","m","1722.16",4.23,7284.74]
[null,null,"品牌相当于或优于“银杉”"]
["144","030411004010","管内穿消防广播回路 NH-RVVP-250V-2x1.5","m","263.11",{"v":5.4,"d":"5.40"},1420.79]
[null,null,"品牌相当于或优于“银杉”"]
["145","030411001005","配管","m","1459.05",14.31,20879.01]
[null,null,"材质 钢管"]
[null,null,"规格 SC15"]
[null,null,"品牌相当于或优于“雄塑”"]
["146","030413002002","管道DN25 凿槽及恢复","m","44.00",17.11,752.84]
["147","030905001001","自动报警系统调试","系统","1",16399.49,16399.49]
[null,null,"应急照明",{"$nulls":3},10865.98]
["148","030412001010","带蓄电池应急双头灯","套","13",147.22,1913.86]
[null,null,"型号规格 2x5W LED灯 ~220V A型灯具"]
[null,null,"距地2.5米安装,5W,90min"]
[{"$nulls":7},"表-08"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程 ",{"$nulls":5},"第17页 共17页"]
["序\r\n\r\n号","项目编码","项目名称及\r\n项目特征描述","计量单位","工程量","金额(元)"]
[{"$nulls":5},"综合单价","合 价","其中："]
[{"$nulls":7},"暂估价"]
[null,null,"无墙体位置吊装,距地大于2.2m"]
["149","030412001011","安全出口标志灯","套","6",{"v":165.4,"d":"165.40"},{"v":992.4,"d":"992.40"}]
[null,null,"型号规格  1x3W LED灯 ~220V A型灯具"]
[null,null,"门上0.2米安装,3W,90min"]
["150","030412001012","单向疏散指示灯","套","10",101.77,{"v":1017.7,"d":"1017.70"}]
[null,null,"型号规格 1x3W LED灯 ~220V A型灯具"]
[null,null,"距地0.5米安装,5W,90min"]
["151","030412001013","双向疏散指示灯","套","1",101.77,101.77]
[null,null,"型号规格 1x3W LED灯 ~220V A型灯具"]
[null,null,"安装方式  距地0.5m壁装"]
["152","030411004011","管内穿线NH-BV-2.5","m","609.30",4.05,2467.67]
[null,null,"品牌相当于或优于“银杉”"]
["153","030411001006","配管","m","203.10",16.98,3448.64]
[null,null,"材质 钢管"]
[null,null,"规格 SC20"]
[null,null,"品牌相当于或优于“雄塑”"]
["154","030413002003","管道DN20 凿(压)槽及恢复","m","54.00",17.11,923.94]
[null,null,"     小    计",{"$nulls":3},{"v":142862.2,"d":"142862.20"}]
[null,null,"     ∑人工费",{"$nulls":3},43280.93]
[null,null,"     ∑材料费",{"$nulls":3},77603.24]
[null,null,"     ∑机械费",{"$nulls":3},1720.27]
[null,null,"     ∑管理费",{"$nulls":3},13796.78]
[null,null,"     ∑利  润",{"$nulls":3},6460.97]
[null,null,"     合    计",{"$nulls":3},{"v":142862.2,"d":"142862.20"}]
[null,null,"     ∑人工费",{"$nulls":3},43280.93]
[null,null,"     ∑材料费",{"$nulls":3},77603.24]
[null,null,"     ∑机械费",{"$nulls":3},1720.27]
[null,null,"     ∑管理费",{"$nulls":3},13796.78]
[null,null,"     ∑利  润",{"$nulls":3},6460.97]
[null,null,"     总 合 计",{"$nulls":3},1292828.17]
[null,null,"     ∑人工费",{"$nulls":3},310299.75]
[null,null,"     ∑材料费",{"$nulls":3},842307.16]
[null,null,"     ∑机械费",{"$nulls":3},19207.37]
[null,null,"     ∑管理费",{"$nulls":3},{"v":92902.1,"d":"92902.10"}]
[null,null,"     ∑利  润",{"$nulls":3},28111.84]
[]
[{"$nulls":7},"表-08"]

{"sheet":"表-09_工程量清单综合单价分析表","index":6,"n_rows":908,"n_cols":12,"rows_kept":908,"merged":[[0,0,0,11],[1,0,1,7],[1,8,1,11],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,6,2,11],[30,0,30,11],[31,0,31,7],[31,8,31,11],[32,0,33,0],[32,1,33,1],[32,2,33,2],[32,3,33,3],[32,4,33,4],[32,6,32,11],[58,0,58,11],[59,0,59,7],[59,8,59,11],[60,0,61,0],[60,1,61,1],[60,2,61,2],[60,3,61,3],[60,4,61,4],[60,6,60,11],[87,0,87,11],[88,0,88,7],[88,8,88,11],[89,0,90,0],[89,1,90,1],[89,2,90,2],[89,3,90,3],[89,4,90,4],[89,6,89,11],[115,0,115,11],[116,0,116,7],[116,8,116,11],[117,0,118,0],[117,1,118,1],[117,2,118,2],[117,3,118,3],[117,4,118,4],[117,6,117,11],[141,0,141,11],[142,0,142,7],[142,8,142,11],[143,0,144,0],[143,1,144,1],[143,2,144,2],[143,3,144,3],[143,4,144,4],[143,6,143,11],[168,0,168,11],[169,0,169,7],[169,8,169,11],[170,0,171,0],[170,1,171,1],[170,2,171,2],[170,3,171,3],[170,4,171,4],[170,6,170,11],[196,0,196,11],[197,0,197,7],[197,8,197,11],[198,0,199,0],[198,1,199,1],[198,2,199,2],[198,3,199,3],[198,4,199,4],[198,6,198,11],[223,0,223,11],[224,0,224,7],[224,8,224,11],[225,0,226,0],[225,1,226,1],[225,2,226,2],[225,3,226,3],[225,4,226,4],[225,6,225,11],[251,0,251,11],[252,0,252,7],[252,8,252,11],[253,0,254,0],[253,1,254,1],[253,2,254,2],[253,3,254,3],[253,4,254,4],[253,6,253,11],[279,0,279,11],[280,0,280,7],[280,8,280,11],[281,0,282,0],[281,1,282,1],[281,2,282,2],[281,3,282,3],[281,4,282,4],[281,6,281,11],[306,0,306,11],[307,0,307,7],[307,8,307,11],[308,0,309,0],[308,1,309,1],[308,2,309,2],[308,3,309,3],[308,4,309,4],[308,6,308,11],[336,0,336,11],[337,0,337,7],[337,8,337,11],[338,0,339,0],[338,1,339,1],[338,2,339,2],[338,3,339,3],[338,4,339,4],[338,6,338,11],[364,0,364,11],[365,0,365,7],[365,8,365,11],[366,0,367,0],[366,1,367,1],[366,2,367,2],[366,3,367,3],[366,4,367,4],[366,6,366,11],[392,0,392,11],[393,0,393,7],[393,8,393,11],[394,0,395,0],[394,1,395,1],[394,2,395,2],[394,3,395,3],[394,4,395,4],[394,6,394,11],[419,0,419,11],[420,0,420,7],[420,8,420,11],[421,0,422,0],[421,1,422,1],[421,2,422,2],[421,3,422,3],[421,4,422,4],[421,6,421,11],[449,0,449,11],[450,0,450,7],[450,8,450,11],[451,0,452,0],[451,1,452,1],[451,2,452,2],[451,3,452,3],[451,4,452,4],[451,6,451,11],[479,0,479,11],[480,0,480,7],[480,8,480,11],[481,0,482,0],[481,1,482,1],[481,2,482,2],[481,3,482,3],[481,4,482,4],[481,6,481,11],[509,0,509,11],[510,0,510,7],[510,8,510,11],[511,0,512,0],[511,1,512,1],[511,2,512,2],[511,3,512,3],[511,4,512,4],[511,6,511,11],[538,0,538,11],[539,0,539,7],[539,8,539,11],[540,0,541,0],[540,1,541,1],[540,2,541,2],[540,3,541,3],[540,4,541,4],[540,6,540,11],[562,0,562,11],[563,0,563,7],[563,8,563,11],[564,0,565,0],[564,1,565,1],[564,2,565,2],[564,3,565,3],[564,4,565,4],[564,6,564,11],[587,0,587,11],[588,0,588,7],[588,8,588,11],[589,0,590,0],[589,1,590,1],[589,2,590,2],[589,3,590,3],[589,4,590,4],[589,6,589,11],[617,0,617,11],[618,0,618,7],[618,8,618,11],[619,0,620,0],[619,1,620,1],[619,2,620,2],[619,3,620,3],[619,4,620,4],[619,6,619,11],[642,0,642,11],[643,0,643,7],[643,8,643,11],[644,0,645,0],[644,1,645,1],[644,2,645,2],[644,3,645,3],[644,4,645,4],[644,6,644,11],[671,0,671,11],[672,0,672,7],[672,8,672,11],[673,0,674,0],[673,1,674,1],[673,2,674,2],[673,3,674,3],[673,4,674,4],[673,6,673,11],[700,0,700,11],[701,0,701,7],[701,8,701,11],[702,0,703,0],[702,1,703,1],[702,2,703,2],[702,3,703,3],[702,4,703,4],[702,6,702,11],[728,0,728,11],[729,0,729,7],[729,8,729,11],[730,0,731,0],[730,1,731,1],[730,2,731,2],[730,3,731,3],[730,4,731,4],[730,6,730,11],[759,0,759,11],[760,0,760,7],[760,8,760,11],[761,0,762,0],[761,1,762,1],[761,2,762,2],[761,3,762,3],[761,4,762,4],[761,6,761,11],[790,0,790,11],[791,0,791,7],[791,8,791,11],[792,0,793,0],[792,1,793,1],[792,2,793,2],[792,3,793,3],[792,4,793,4],[792,6,792,11],[821,0,821,11],[822,0,822,7],[822,8,822,11],[823,0,824,0],[823,1,824,1],[823,2,824,2],[823,3,824,3],[823,4,824,4],[823,6,823,11],[849,0,849,11],[850,0,850,7],[850,8,850,11],[851,0,852,0],[851,1,852,1],[851,2,852,2],[851,3,852,3],[851,4,852,4],[851,6,851,11],[879,0,879,11],[880,0,880,7],[880,8,880,11],[881,0,882,0],[881,1,882,1],[881,2,882,2],[881,3,882,3],[881,4,882,4],[881,6,881,11]],"flags":["formulas_cached_only"]}
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第1页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,null,"广西中医药大学教师教学发展中心装修工程-拆除"]
[null,null,"分部分项工程"]
[null,null,"G.1 人工拆除工程"]
["1","011601001001","砖砌体拆除","","40.68",42.26,{"v":38.4,"d":"38.40"},null,null,{"v":2.9,"d":"2.90"},0.96]
[null,null,"拆除方式:人工"]
[null,null,"砌体名称:砌块墙"]
[null,"07010034","拆除砌体 砌块墙","10","4.068",422.63,{"v":384,"d":"384.00"},null,null,29.03,{"v":9.6,"d":"9.60"}]
["2","010103002001","余土弃置","","40.68",28.22,9.79,null,15.85,1.94,0.64]
[null,null,"废弃料品种:拆除的废弃材料"]
[null,null,"运距:起步第1km"]
[null,null,"含装车、洒水、加盖费"]
[null,"07040005","加盖自卸垃圾车运渣土 人工装渣土1km以内","100","0.4068",2822.63,{"v":979.2,"d":"979.20"},null,1585.42,193.89,64.12]
["3","桂010103003001","土方运输每增(减)1km","","366.12",2.22,null,null,2.02,0.15,0.05]
[null,null,"废弃料品种:拆除的废弃材料"]
[null,null,"含装车、洒水、加盖费"]
[null,null,"工程量暂按增运9km计算，最终按实际结算"]
[null,"07040008","加盖自卸垃圾车运渣土 每增加1km","100","3.6612",222.86,null,null,202.49,15.31,5.06]
["4","010103002002","弃土场消纳费","","40.68",{"v":8,"d":"8.00"},null,{"v":8,"d":"8.00"}]
[null,null,"废弃料品种:拆除的废弃材料"]
[null,"B-换","弃土场消纳费","","40.68",{"v":8,"d":"8.00"},null,{"v":8,"d":"8.00"}]
[null,null,"广西中医药大学教师教学发展中心装修工程-装饰装修"]
[null,null,"分部分项工程"]
[null,null,"A.1 土（石）方工程"]
["5","010103001001","回填方","","258.52",20.77,16.29,null,2.27,1.76,0.45]
[null,null,"室内房心回填，高度20cm"]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第2页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,"A1-82","人工回填土 夯填","100","2.5852",2077.43,1628.64,null,227.04,176.29,45.46]
["6","010103002003","校内取土","","258.52",8.87,0.37,null,7.56,0.75,0.19]
[null,null,"运距:1km以内"]
[null,"A1-165","液压挖掘机挖土 斗容量1.8 自卸汽车运土(运距1km以内) 10t","1000","0.25852",8885.88,{"v":374.4,"d":"374.40"},null,7562.96,754.05,194.47]
[null,null,"A.3 砌筑工程"]
["7","010402001001","砌块墙","","165.06",408.08,110.56,248.42,2.17,37.39,9.54]
[null,null,"砖品种、规格、强度等级:蒸压加气砼砌块"]
[null,null,"墙体类型:直形"]
[null,null,"墙体厚度:200mm"]
[null,null,"砂浆种类、强度等级:混合砂浆M5.0"]
[null,"A3-56","蒸压加气混凝土砌块墙 墙体厚度 20cm{水泥石灰砂浆中砂M5}","10","16.506",4080.75,1105.57,2484.19,{"v":21.7,"d":"21.70"},373.92,95.37]
[null,null,"A.4 混凝土及钢筋混凝土工程"]
["8","010502002001","构造柱","","4.11",531.67,{"v":94.7,"d":"94.70"},395.76,1.26,31.83,8.12]
[null,null,"混凝土种类:非泵送商品砼"]
[null,null,"混凝土强度等级:C20"]
[null,"A4-20换","混凝土柱 构造柱{换:碎石 GD40  商品普通砼  C20}","10","0.411",5316.58,946.96,3957.57,12.59,318.28,81.18]
["9","010503004001","圈梁","","3.62",{"v":520.8,"d":"520.80"},85.29,{"v":398.9,"d":"398.90"},0.78,28.55,7.28]
[null,null,"混凝土种类:非泵送商品砼"]
[null,null,"混凝土强度等级:C20"]
[null,"A4-24换","混凝土 圈梁{换:碎石 GD40  商品普通砼  C20}","10","0.362",5207.94,852.85,3988.98,7.82,285.48,72.81]
["10","010503005001","过梁","","0.12",542.74,{"v":96.7,"d":"96.70"},403.98,1.27,{"v":32.5,"d":"32.50"},8.29]
[null,null,"混凝土种类:非泵送商品砼"]
[null,null,"混凝土强度等级:C20"]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第3页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,"A4-25换","混凝土 过梁{换:碎石 GD40  商品普通砼  C20}","10","0.012",5427.25,966.97,4039.76,12.69,324.95,82.88]
["11","010507005001","扶手、压顶","","0.50",590.98,124.93,414.04,null,41.44,10.57]
[null,null,"混凝土种类:非泵送商品砼"]
[null,null,"混凝土强度等级:C20"]
[null,"A4-53","混凝土 压顶、扶手{碎石 GD40  商品普通砼  C20}","10","0.050",5909.85,1249.33,4140.43,null,{"v":414.4,"d":"414.40"},105.69]
["12","010515001001","现浇构件钢筋","t","0.667",6810.07,709.14,5786.63,13.48,239.69,61.13]
[null,null,"钢筋种类、规格:圆钢 φ10以内"]
[null,null,"品牌相当于或优于“柳钢”"]
[null,"A4-236","现浇构件圆钢筋制安 φ10以内","t","0.667",6810.07,709.14,5786.63,13.48,239.69,61.13]
["13","010515001002","现浇构件钢筋","t","0.375",7095.68,599.47,6121.48,88.38,228.16,58.19]
[null,null,"钢筋种类、规格:圆钢 φ10以上"]
[null,null,"品牌相当于或优于“柳钢”"]
[null,"A4-237","现浇构件圆钢筋制安 φ10以上","t","0.375",7095.68,599.47,6121.48,88.38,228.16,58.19]
["14","010515001003","现浇构件钢筋","t","0.034",7116.24,878.83,5847.81,16.76,297.07,75.77]
[null,null,"钢筋种类、规格:螺纹钢 10以内"]
[null,null,"品牌相当于或优于“柳钢”"]
[null,"A4-240","现浇构件螺纹钢制安 10以内","t","0.034",7116.24,878.83,5847.81,16.76,297.07,75.77]
["15","桂010515011001","砌体加固筋","t","0.617",7562.96,1241.92,5786.58,12.32,416.03,106.11]
[null,null,"钢筋种类、规格:圆钢 φ10以内"]
[null,null,"品牌相当于或优于“柳钢”"]
[null,"A4-317","砖砌体加固钢筋 绑扎","t","0.617",7562.96,1241.92,5786.58,12.32,416.03,106.11]
[null,null,"A.9 楼地面工程"]
["16","010404001001","垫层","","152.35",458.29,58.55,374.29,0.76,19.67,5.02]
[null,null,"夯实地面用C10混凝土垫高300mm,至±0.000"]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第4页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,null,"混凝土种类:非泵送商品砼"]
[null,null,"混凝土强度等级:C10"]
[null,"A4-3换","混凝土垫层{换:碎石 GD40  商品普通砼  C10}","10","15.235",4582.81,585.47,3742.89,7.57,196.71,50.17]
["17","011102003001","水磨石地砖地面","㎡","566.10",153.82,{"v":38.7,"d":"38.70"},98.89,2.18,11.16,2.89]
[null,null,"素水泥结合层一道"]
[null,null,"30厚M10干硬性水泥砂浆结合层"]
[null,null,"表面撒水泥粉"]
[null,null,"面贴地砖1200×600,水泥擦缝(密缝拼接)"]
[null,"A9-85换","陶瓷地砖楼地面 每块周长(3200mm以上)  水泥砂浆 密缝{换:水泥砂浆中砂M10}","100㎡","5.6610",15380.31,3869.58,9888.76,217.61,{"v":1115.8,"d":"1115.80"},288.56]
["18","011102003002","水磨石地砖地面","㎡","72.73",125.71,26.34,87.39,2.18,7.79,2.01]
[null,null,"素水泥结合层一道"]
[null,null,"30厚M10干硬性水泥砂浆结合层"]
[null,null,"表面撒水泥粉"]
[null,null,"面贴地砖600×600,水泥擦缝(密缝拼接)"]
[null,"A9-83换","陶瓷地砖楼地面 每块周长(2400mm以内)  水泥砂浆 密缝{换:水泥砂浆中砂M10}","100㎡","0.7273",12570.77,2634.06,8739.26,217.61,778.51,201.33]
["19","011102003003","灰麻烧毛石地面","㎡","112.68",175.66,{"v":27.3,"d":"27.30"},{"v":135,"d":"135.00"},2.96,8.26,2.14]
[null,null,"水泥浆一道(内掺建筑胶)"]
[null,null,"30厚M10干硬性水泥砂浆结合层"]
[null,null,"表面撒水泥粉"]
[null,null,"900×600×25灰麻烧毛石铺实拍平(踏步边缘开防滑槽),水泥浆擦缝"]
[null,"A9-48换","花岗岩楼地面 不拼花 水泥砂浆{换:水泥砂浆中砂M10}","100㎡","1.1268",17565.99,2730.16,13500.18,{"v":295.9,"d":"295.90"},826.11,213.64]
["20","011103001001","仿地毯块状地胶地面","㎡","522.66",190.39,38.77,136.73,1.17,{"v":10.9,"d":"10.90"},2.82]
[null,null,"水泥浆一道(内掺建筑胶)"]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第5页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,null,"30厚M10干硬性水泥砂浆结合层"]
[null,null,"水泥自流平界面剂"]
[null,null,"自流平找平层"]
[null,null,"2.0厚PVC方块地胶(胶粘剂粘贴)"]
[null,"A9-1换","水泥砂浆找平层 混凝土或硬基层上 20mm[实际30]{换:水泥砂浆中砂M10 换:水泥砂浆中砂M10}","100㎡","5.2266",2432.37,884.01,1168.79,56.43,256.74,{"v":66.4,"d":"66.40"}]
[null,"A9-9","普通水泥自流平","100㎡","5.2266",1956.88,693.58,973.73,38.15,199.76,51.66]
[null,"A9-119换","PVC塑胶地面","100㎡","5.2266",14649.98,2299.44,11530.25,22.48,633.88,163.93]
["21","011104002001","浅木纹复合木地板","㎡","114.55",197.76,24.44,164.16,0.56,6.83,1.77]
[null,null,"30厚M10干硬性水泥砂浆结合层"]
[null,null,"泡沫塑料衬垫"]
[null,null,"安装浅木纹复合木地板1200×150×12"]
[null,null,"阳角收口采用木地板同款同色成品铝合金收边条"]
[null,null,"品牌相当于或优于“富林”"]
[null,"A9-1换","水泥砂浆找平层 混凝土或硬基层上 20mm[实际30]{换:水泥砂浆中砂M10 换:水泥砂浆中砂M10}","100㎡","1.1455",2432.37,884.01,1168.79,56.43,256.74,{"v":66.4,"d":"66.40"}]
[null,"A9-148换","长条复合 木地板 铺在 水泥地 面上 面上","100㎡","1.1455",17343.48,1559.84,15247.68,null,425.84,110.12]
["22","011104002002","浅木纹复合木地板（台阶）","㎡","12.47",242.19,24.44,208.59,0.56,6.83,1.77]
[null,null,"30厚M10干硬性水泥砂浆结合层"]
[null,null,"泡沫塑料衬垫"]
[null,null,"安装浅木纹复合木地板1200×150×12"]
[null,null,"阳角收口采用木地板同款同色成品铝合金收边条"]
[null,null,"按展开面积计算"]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第6页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,null,"品牌相当于或优于“富林”"]
[null,"A9-1换","水泥砂浆找平层 混凝土或硬基层上 20mm[实际30]{换:水泥砂浆中砂M10 换:水泥砂浆中砂M10}","100㎡","0.1247",2432.37,884.01,1168.79,56.43,256.74,{"v":66.4,"d":"66.40"}]
[null,"A9-148换","长条复合 木地板 铺在 水泥地 面上 面上","100㎡","0.1247",17343.48,1559.84,15247.68,null,425.84,110.12]
[null,"B-","铝合金收边条","m","27.70",{"v":20,"d":"20.00"},null,{"v":20,"d":"20.00"}]
["23","011107001001","石材台阶面","㎡","23.04",422.02,69.21,309.95,12.86,23.86,6.14]
[null,null,"台阶做法参见图集12J003 11B/B3"]
[null,null,"30厚灰麻花岗岩饰面台阶踏步(荔枝面)及踏步踢面"]
[null,"A3-89","灰土 垫层{灰土 3∶7}","10","0.778",3469.08,600.95,2604.79,9.29,202.42,51.63]
[null,"A4-58","混凝土 台阶{碎石 GD20  商品普通砼  C20}","10","0.156",4920.36,600.95,4040.48,{"v":20.3,"d":"20.30"},206.07,52.56]
[null,"A9-54换","花岗岩台阶 直形 水泥砂浆{素水泥浆}","100㎡","0.2304",27157.09,4484.77,19463.83,1241.08,1563.16,404.25]
["24","010401012001","入口砌砖花池","","6.11",1277.01,306.91,820.07,21.63,102.22,26.18]
[null,null,"150mm厚3:7灰土垫层"]
[null,null,"非粘土烧结砖砌筑"]
[null,null,"顶部及侧面30厚灰麻花岗岩饰面(荔枝面)（1:3水泥砂浆粘结层）"]
[null,null,"60厚C20混凝土压顶Φ6钢筋@200双向"]
[null,"A3-89","灰土 垫层{灰土 3∶7}","10","0.130",3469.08,600.95,2604.79,9.29,202.42,51.63]
[null,"A3-37","零星砌体 标准砖240×115×53{水泥石灰砂浆中砂M5}","10","0.611",7033.66,{"v":1897.7,"d":"1897.70"},4292.15,37.98,642.07,163.76]
[null,"A9-56换","花岗岩零星项目 水泥砂浆{素水泥浆}","100㎡","0.1224",23325.44,4869.15,15601.71,879.38,1569.35,405.85]
[null,"A4-53换","混凝土 压顶、扶手{换:碎石 GD40  商品普通砼  C20}","10","0.024",{"v":6302.3,"d":"6302.30"},1526.42,4140.43,null,506.31,129.14]
[null,"A4-236","现浇构件圆钢筋制安 φ10以内","t","0.007",6810.07,709.14,5786.63,13.48,239.69,61.13]
[null,null,"A.10 墙、柱面工程"]
["25","011201001001","墙面一般抹灰","㎡","606.16",18.61,8.68,6.59,0.27,2.44,0.63]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第7页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,null,"13厚1:0.3:3水泥石膏砂浆打底扫毛"]
[null,"A10-37换","内墙、内墙裙 水泥砂浆找平层 砖墙 15mm{换:混合砂浆 1∶0.5∶3}","100㎡","6.0616",2054.28,930.07,762.36,31.47,{"v":262.5,"d":"262.50"},67.88]
[null,"A10-55换","抹灰层每增减1mm 混合砂浆{换:混合砂浆 1∶0.5∶3}","100㎡","6.0616",-191.96,-61.78,-103.12,-4.34,-18.05,-4.67]
["26","011201001002","墙面一般抹灰","㎡","293.34",19.49,{"v":9.3,"d":"9.30"},6.57,0.31,2.63,0.68]
[null,null,"15厚M10水泥砂浆找平"]
[null,"A10-37换","内墙、内墙裙 水泥砂浆找平层 砖墙 15mm{换:水泥砂浆中砂M10}","100㎡","2.9334",1948.65,930.07,656.73,31.47,{"v":262.5,"d":"262.50"},67.88]
["27","011207001001","条形吸音板墙面","㎡","262.84",265.29,{"v":30.5,"d":"30.50"},221.51,2.08,{"v":8.9,"d":"8.90"},{"v":2.3,"d":"2.30"}]
[null,null,"U50墙面轻钢龙骨@400mm"]
[null,null,"15厚阻燃板基层"]
[null,null,"1220×2440×15吸音板(竖条纹)"]
[null,"A10-236","轻钢龙骨 中距(mm) 竖603横1500","100㎡","2.6284",6965.58,1223.51,5293.27,21.14,339.79,87.87]
[null,"A10-242换","板基层 15厚阻燃板","100㎡","2.6284",5015.66,611.75,4084.68,81.15,189.16,48.92]
[null,"A10-265换","硬木板条墙面、墙裙","100㎡","2.6284",14547.87,1214.93,12773.13,105.96,{"v":360.6,"d":"360.60"},93.25]
["28","011502002001","木质装饰线","m","14.17",7.67,3.54,2.91,null,0.97,0.25]
[null,null,"吸音板墙面80×15实木线条"]
[null,"A14-58换","木质装饰线 150mm内","100m","0.1417",765.62,{"v":353.5,"d":"353.50"},290.65,null,96.51,24.96]
["29","011502002002","木质装饰线","m","11.83",6.58,2.52,3.19,null,0.69,0.18]
[null,null,"15宽实木半圆线120×15"]
[null,"A14-55换","木质装饰线 宽度 50mm内","100m","0.1183",{"v":658.3,"d":"658.30"},252.25,319.38,null,68.86,17.81]
["30","011502002003","木质装饰线","m","14.80",5.53,2.52,2.14,null,0.69,0.18]
[null,null,"15宽实木半圆线60×15"]
[null,"A14-55换","木质装饰线 宽度 50mm内","100m","0.1480",{"v":553.3,"d":"553.30"},252.25,214.38,null,68.86,17.81]
["31","011105006001","冲压黑钛不锈钢踢脚线","㎡","22.88",277.45,40.78,221.57,0.81,11.35,2.94]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第8页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,null,"15厚阻燃板基层"]
[null,null,"冲压1.0厚冲压黑钛不锈钢踢脚线用万能胶拍合安装"]
[null,null,"80mm高"]
[null,null,"品牌相当于或优于“海利”"]
[null,"A10-242换","板基层 15厚阻燃板","100㎡","0.2288",5015.66,611.75,4084.68,81.15,189.16,48.92]
[null,"A9-162换","踢脚线 金属板","100㎡","0.2288",22729.75,3466.32,{"v":18072.4,"d":"18072.40"},null,946.31,244.72]
["32","011105006002","不锈钢墙面","㎡","16.68",338.43,39.77,283.91,0.81,11.08,2.86]
[null,null,"15厚阻燃板基层"]
[null,null,"1.0厚304#拉丝不锈钢饰面"]
[null,null,"品牌相当于或优于“海利”"]
[null,"A10-242换","板基层 15厚阻燃板","100㎡","0.1668",5015.66,611.75,4084.68,81.15,189.16,48.92]
[null,"A10-249换","不锈钢面板 墙面","100㎡","0.1668",28827.67,3365.08,24306.35,null,918.67,237.57]
["33","桂011204005001","内墙面干挂石材","㎡","123.29",280.63,82.14,161.52,6.51,{"v":24.2,"d":"24.20"},6.26]
[null,null,"5#镀锌角钢横向龙骨间距600×900mm(油丹红底漆两遍,防锈漆两遍)（另列清单）"]
[null,null,"不锈钢干挂件(油丹红底漆两遍,防锈漆两遍)"]
[null,null,"麻灰烧毛石600×900×30干挂(竖向密缝拼接、横向留自然缝)"]
[null,"A10-132换","干挂花岗岩 墙面 密缝","100㎡","1.2329",28063.96,8214.49,16152.05,651.17,2420.33,625.92]
["34","桂011204005002","外墙面干挂石材","㎡","23.85",413.23,82.14,294.12,6.51,{"v":24.2,"d":"24.20"},6.26]
[null,null,"5#镀锌角钢横向龙骨间距600×900mm(油丹红底漆两遍,防锈漆两遍)（另列清单）"]
[null,null,"不锈钢干挂件(油丹红底漆两遍,防锈漆两遍)"]
[null,null,"25厚黑金砂花岗岩饰面干挂(竖向密缝拼接、横向留自然缝)"]
[null,"A10-132换","干挂花岗岩 墙面 密缝","100㎡","0.2385",41323.96,8214.49,29412.05,651.17,2420.33,625.92]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第9页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
["35","桂011204007001","块料墙面","㎡","33.76",105.04,38.61,50.73,1.81,11.04,2.85]
[null,null,"15厚1:3水泥砂浆找平"]
[null,null,"3-4厚1:1水泥砂浆加水重20%专用瓷砖胶镶贴"]
[null,null,"面贴100×100釉面砖(工字拼贴),白水泥浆擦缝"]
[null,null,"品牌相当于或优于“东鹏”"]
[null,"A10-160换","面砖(周长600mm以内) 水泥砂浆粘贴 墙面、墙裙 缝宽5mm内{素水泥浆}","100㎡","0.3376",10504.25,{"v":3861,"d":"3861.00"},5073.21,181.15,1103.51,285.38]
["36","011502001001","金属装饰线","m","61.45",28.47,1.71,26.12,0.04,0.48,0.12]
[null,null,"1.0厚冲压黑钛不锈钢收边，宽20mm，反边27.5mm"]
[null,null,"品牌相当于或优于“海利”"]
[null,"A14-45换","金属装饰 压条","100m","0.6145",2846.08,170.74,2611.69,3.71,47.62,12.32]
["37","011502001002","金属装饰线","m","24.96",10.96,1.71,8.61,0.04,0.48,0.12]
[null,null,"成品黑色铝合金工字收口条，高度同硬包厚度，约18mm高"]
[null,null,"品牌相当于或优于“海利”"]
[null,"A14-45换","金属装饰 压条","100m","0.2496",1095.08,170.74,860.69,3.71,47.62,12.32]
["38","011502001003","金属装饰线","m","32.80",22.03,4.78,15.61,null,{"v":1.3,"d":"1.30"},0.34]
[null,null,"1.0厚黑钛不锈钢包边，展开宽度85mm"]
[null,null,"品牌相当于或优于“海利”"]
[null,"A14-50换","金属装饰线 镜面不锈钢 60mm外","100m","0.3280",2202.72,477.91,{"v":1560.6,"d":"1560.60"},null,130.47,33.74]
["39","011502001004","金属装饰线","m","7.38",15.67,4.78,9.25,null,{"v":1.3,"d":"1.30"},0.34]
[null,null,"部位：出入口铝塑板檐口处"]
[null,null,"1.0厚黑钛不锈钢，宽度50mm"]
[null,null,"品牌相当于或优于“海利”"]
[null,"A14-49换","金属装饰线 镜面不锈钢 60mm内","100m","0.0738",1566.87,477.91,924.75,null,130.47,33.74]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第10页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
["40","011207001002","墙面装饰板","㎡","72.38",349.34,36.31,299.18,1.02,10.19,2.64]
[null,null,"U50轻钢龙骨"]
[null,null,"15厚阻燃夹板基层"]
[null,null,"面层：12厚钢化玻璃背蓝漆"]
[null,null,"品牌相当于或优于“南玻”"]
[null,"A10-236","轻钢龙骨 中距(mm) 竖603横1500","100㎡","0.7238",6965.58,1223.51,5293.27,21.14,339.79,87.87]
[null,"A10-242换","板基层 15厚阻燃板","100㎡","0.7238",5015.66,611.75,4084.68,81.15,189.16,48.92]
[null,"A10-245换","镜面玻璃 墙面 在胶合板上粘贴","100㎡","0.7238",22952.78,1795.79,20539.96,null,490.25,126.78]
["41","011207001003","墙面装饰板","㎡","64.37",368.16,52.35,296.45,1.02,14.57,3.77]
[null,null,"U50轻钢龙骨"]
[null,null,"15厚阻燃夹板基层"]
[null,null,"9厚阻燃夹板基层浅咖啡色仿布纹硬包"]
[null,"A10-236","轻钢龙骨 中距(mm) 竖603横1500","100㎡","0.6437",6965.58,1223.51,5293.27,21.14,339.79,87.87]
[null,"A10-242换","板基层 15厚阻燃板","100㎡","0.6437",5015.66,611.75,4084.68,81.15,189.16,48.92]
[null,"A10-261换","人造革软包带衬板 墙、柱面","100㎡","0.6437",24834.79,{"v":3399.4,"d":"3399.40"},20267.35,null,928.04,{"v":240,"d":"240.00"}]
["42","桂011204005003","石材墙面","㎡","124.95",428.53,82.14,309.42,6.51,{"v":24.2,"d":"24.20"},6.26]
[null,null,"5#镀锌角钢横向龙骨间距600×900mm(油丹红底漆两遍,防锈漆两遍)（另列清单）"]
[null,null,"不锈钢干挂件(油丹红底漆两遍,防锈漆两遍)"]
[null,null,"25厚西班牙米黄大理石饰面干挂"]
[null,null,"部位：外墙及部分柱面、主入口"]
[null,"A10-132换","干挂花岗岩 墙面 密缝","100㎡","1.2495",42853.96,8214.49,30942.05,651.17,2420.33,625.92]
["43","桂011204007002","块料墙面","㎡","43.92",177.39,38.61,123.08,1.81,11.04,2.85]
[null,null,"15厚1:3水泥砂浆找平"]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第11页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,null,"3-4厚1:1水泥砂浆加水重20%专用瓷砖胶镶贴"]
[null,null,"面贴400×800深灰色仿石材瓷砖,白水泥浆擦缝"]
[null,null,"部位：外墙面"]
[null,null,"品牌相当于或优于“东鹏”"]
[null,"A10-160换","面砖(周长600mm以内) 水泥砂浆粘贴 墙面、墙裙 缝宽5mm内{素水泥浆}","100㎡","0.4392",17738.75,{"v":3861,"d":"3861.00"},12307.71,181.15,1103.51,285.38]
["44","桂011204007003","块料墙面","㎡","46.79",357.71,50.54,282.71,5.28,15.24,3.94]
[null,null,"25厚西班牙米黄大理石（密拼）"]
[null,null,"20厚1:3水泥砂浆结合层"]
[null,null,"部位：外墙窗底部"]
[null,"A10-105换","粘贴大理石 水泥砂浆粘贴 砖墙面{素水泥浆}","100㎡","0.4679",35771.51,5053.62,28271.46,528.44,{"v":1523.9,"d":"1523.90"},394.09]
["45","011207001004","墙面装饰板","㎡","3.20",68.05,8.39,56.78,null,2.29,0.59]
[null,null,"20×20×2镀锌方通骨架@600(油丹红底漆两遍,防锈漆两遍)（另列清单）"]
[null,null,"12厚埃特板"]
[null,"A10-266换","埃特板墙面","100㎡","0.0320",{"v":6805.5,"d":"6805.50"},839.12,5678.06,null,229.08,59.24]
["46","011207001005","墙面装饰板","㎡","133.51",189.09,30.06,147.34,1.02,8.48,2.19]
[null,null,"配套金属轻钢龙骨架"]
[null,null,"9厚阻燃板基层"]
[null,null,"面封竹木纤维集成墙板(密缝拼接)，600宽×9厚"]
[null,null,"阳角采用配套25×25mmL型同款同色阳角线条"]
[null,null,"阴角采用配套27×16mm同款同色阴角线条"]
[null,"A10-236","轻钢龙骨 中距(mm) 竖603横1500","100㎡","1.3351",6965.58,1223.51,5293.27,21.14,339.79,87.87]
[null,"A10-242换","板基层 9厚阻燃板","100㎡","1.3351",4070.66,611.75,3139.68,81.15,189.16,48.92]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第12页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,"A10-267换","竹片内墙面","100㎡","1.3351",7873.89,1170.31,6301.47,null,319.49,82.62]
["47","011207001006","聚酯纤维吸音板","㎡","31.46",172.94,22.64,141.15,1.02,6.46,1.67]
[null,null,"U50墙面轻钢龙骨@400mm"]
[null,null,"15厚阻燃板基层"]
[null,null,"600×2400×9聚酯纤维吸音板(横竖向留V型缝)"]
[null,"A10-236","轻钢龙骨 中距(mm) 竖603横1500","100㎡","0.3146",6965.58,1223.51,5293.27,21.14,339.79,87.87]
[null,"A10-242换","板基层 15厚阻燃板","100㎡","0.3146",5015.66,611.75,4084.68,81.15,189.16,48.92]
[null,"A10-268换","纤维板","100㎡","0.3146",5313.33,{"v":429,"d":"429.00"},4736.92,null,117.12,30.29]
["48","011207001007","防潮纸面石膏板墙面","㎡","13.46",25.61,8.39,14.34,null,2.29,0.59]
[null,null,"40*20*2钢骨架@1000（另列清单）"]
[null,null,"9.5厚纸面石膏板"]
[null,null,"刮腻子油白色乳胶漆（另列清单）"]
[null,"A10-266换","石膏板墙面","100㎡","0.1346",{"v":2561.4,"d":"2561.40"},839.12,1433.96,null,229.08,59.24]
["49","011207001008","黑钛不锈钢墙面","㎡","0.64",322.55,42.06,264.53,1.12,11.79,3.05]
[null,null,"展示厅立面P-07/A"]
[null,null,"15厚阻燃板基层"]
[null,null,"1.0厚黑钛不锈钢板"]
[null,null,"定制亚克力字体（另列清单）"]
[null,null,"品牌相当于或优于“海利”"]
[null,"A10-242换","板基层 15厚阻燃板","100㎡","0.0088",5015.66,611.75,4084.68,81.15,189.16,48.92]
[null,"A10-249换","不锈钢面板 墙面","100㎡","0.0064",25358.17,3365.08,20836.85,null,918.67,237.57]
["50","011304001001","墙面灯槽","㎡","8.92",134.88,{"v":46.2,"d":"46.20"},72.73,0.05,12.63,3.27]
[null,null,"15厚阻燃夹板基层"]
[null,null,"9.5厚防潮纸面石膏板"]
[null,"A11-171换","悬挑式灯槽 直型 胶合板面","100㎡","0.0892",10925.68,3781.21,{"v":5838.6,"d":"5838.60"},4.95,1033.62,{"v":267.3,"d":"267.30"}]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第13页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,"A10-266换","石膏板墙面","100㎡","0.0892",{"v":2561.4,"d":"2561.40"},839.12,1433.96,null,229.08,59.24]
["51","011304001002","墙面灯槽","㎡","7.59",{"v":162.4,"d":"162.40"},{"v":42.1,"d":"42.10"},105.76,0.05,11.51,2.98]
[null,null,"15厚阻燃夹板基层"]
[null,null,"9厚竹木纤维集成墙板"]
[null,"A11-171换","悬挑式灯槽 直型 胶合板面","100㎡","0.0759",10925.68,3781.21,{"v":5838.6,"d":"5838.60"},4.95,1033.62,{"v":267.3,"d":"267.30"}]
[null,"A10-268换","纤维板","100㎡","0.0759",5313.33,{"v":429,"d":"429.00"},4736.92,null,117.12,30.29]
["52","011204004001","钢骨架","t","1.841",13042.52,2402.48,8582.28,917.14,906.25,234.37]
[null,null,"挂石板钢骨架"]
[null,null,"含油丹红底漆两遍,防锈漆两遍"]
[null,null,"品牌相当于或优于“柳钢”"]
[null,"A10-142","挂石板钢骨架 镀锌钢骨架","t","1.841",12406.63,2071.21,8391.48,917.14,815.82,210.98]
[null,"A13-140","红丹防锈漆 金属面 4遍","100㎡","0.6996",1673.35,871.73,{"v":502.1,"d":"502.10"},null,237.98,61.54]
["53","011204004002","钢骨架","t","3.212",13042.53,2402.48,8582.28,917.14,906.26,234.37]
[null,null,"挂装饰板钢骨架"]
[null,null,"含油丹红底漆两遍,防锈漆两遍"]
[null,null,"品牌相当于或优于“柳钢”"]
[null,"A10-142","挂石板钢骨架 镀锌钢骨架","t","3.212",12406.63,2071.21,8391.48,917.14,815.82,210.98]
[null,"A13-140","红丹防锈漆 金属面 4遍","100㎡","1.2206",1673.35,871.73,{"v":502.1,"d":"502.10"},null,237.98,61.54]
[null,null,"A.11 天棚工程"]
["54","011302001001","防潮纸面石膏板吊顶","㎡","825.59",105.51,36.16,56.63,0.22,9.93,2.57]
[null,null,"Φ8螺纹吊杆"]
[null,null,"U60轻钢龙骨标准骨架(上人型):主龙骨中距900-1000,C型次龙骨中距450,横撑龙骨中距900"]
[null,null,"双层9.5厚纸面石膏板(或双层9.5厚冲孔纸面石膏板),自攻螺钉拧紧,螺丝眼刷防锈漆,再用石膏腻子点补"]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第14页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,null,"刮腻子三遍油乳胶漆三遍（另列清单）"]
[null,"A11-39","装配式U型轻钢天棚龙骨(上人型) 面层规格(600×600mm) 以上 平面","100㎡","8.2559",5119.04,1465.46,3120.34,22.11,406.11,105.02]
[null,"A11-76换","天棚石膏板基层","100㎡","8.2559",2768.51,{"v":1158.3,"d":"1158.30"},1212.21,null,316.22,81.78]
[null,"A11-94换","天棚石膏板面层 安在U型轻钢龙骨上","100㎡","8.2559",2663.91,992.71,{"v":1330.1,"d":"1330.10"},null,271.01,70.09]
["55","011302001002","矿棉板吊顶","㎡","29.04",94.56,22.92,63.39,0.28,6.33,1.64]
[null,null,"φ8螺纹吊杆T型主骨中距600~1200mm,次骨间距@600mm"]
[null,null,"安装矿棉板1200×600×15"]
[null,null,"四周采用L型边龙骨收口"]
[null,"A11-53","装配式T型铝合金天棚龙骨(上人型) 面层规格(600×600mm)  平面","100㎡","0.2904",4938.87,1410.55,3006.31,27.79,392.67,101.55]
[null,"A11-91","天棚矿棉板面层 搁放在 龙骨上","100㎡","0.2904",4516.67,881.17,3332.73,null,240.56,62.21]
["56","011302001003","铝塑板天棚","㎡","242.29",161.45,30.99,119.81,null,8.46,2.19]
[null,null,"5#镀锌角钢架,@600mm（另列清单）"]
[null,null,"15厚阻燃夹板基层"]
[null,null,"面贴4厚铝塑板1220×2440×4"]
[null,null,"横向密缝拼接,竖向留5mm缝填黑色结构胶"]
[null,null,"清单工程量按铝塑板展开面积计算"]
[null,null,"品牌相当于或优于“奥斯特”"]
[null,"A11-75换","15厚阻燃夹板基层","100㎡","2.4229",5124.09,838.27,3997.79,null,228.85,59.18]
[null,"A10-257换","铝塑板墙面 胶合板基层上","100㎡","2.4229",11021.05,2260.83,{"v":7983.4,"d":"7983.40"},null,617.21,159.61]
["57","011302001004","防潮纸面石膏板窗帘盒","㎡","51.60",142.86,35.14,95.35,0.22,9.65,{"v":2.5,"d":"2.50"}]
[null,null,"Φ8螺纹吊杆"]
[null,null,"U60轻钢龙骨标准骨架"]
[null,null,"15厚阻燃夹板基层"]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第15页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,null,"9.5厚纸面石膏板(或双层9.5厚冲孔纸面石膏板),自攻螺钉拧紧,螺丝眼刷防锈漆,再用石膏腻子点补"]
[null,null,"刮腻子三遍油无机乳胶漆三遍（另列清单）"]
[null,"A11-40","装配式U型轻钢天棚龙骨(上人型) 面层规格(600×600mm) 以上 跌级","100㎡","0.5160",6499.06,{"v":1683.4,"d":"1683.40"},4207.54,22.11,{"v":465.6,"d":"465.60"},120.41]
[null,"A11-75换","15厚阻燃夹板基层","100㎡","0.5160",5124.09,838.27,3997.79,null,228.85,59.18]
[null,"A11-94换","天棚石膏板面层 安在U型轻钢龙骨上","100㎡","0.5160",2663.91,992.71,{"v":1330.1,"d":"1330.10"},null,271.01,70.09]
["58","011302001005","天棚灯槽","㎡","33.43",{"v":135.9,"d":"135.90"},47.74,71.69,0.05,13.05,3.37]
[null,null,"15厚阻燃夹板基层"]
[null,null,"9.5厚纸面石膏板(或双层9.5厚冲孔纸面石膏板),自攻螺钉拧紧,螺丝眼刷防锈漆,再用石膏腻子点补"]
[null,null,"刮腻子三遍油无机乳胶漆三遍（另列清单）"]
[null,"A11-171换","悬挑式灯槽 直型 胶合板面","100㎡","0.3343",10925.68,3781.21,{"v":5838.6,"d":"5838.60"},4.95,1033.62,{"v":267.3,"d":"267.30"}]
[null,"A11-94换","天棚石膏板面层 安在U型轻钢龙骨上","100㎡","0.3343",2663.91,992.71,{"v":1330.1,"d":"1330.10"},null,271.01,70.09]
["59","010606013001","∟40×40×4mm镀锌角钢间距1100mm","t","0.329",11751.18,2274.87,{"v":6580.1,"d":"6580.10"},1376.25,1211.08,308.88]
[null,null,"玻璃隔墙门连窗上部"]
[null,null,"品牌相当于或优于“柳钢”"]
[null,"A6-54","金属零星构件制作","t","0.329",10248.64,1474.59,6546.63,1139.27,867.02,221.13]
[null,"A6-100","金属零星构件 安装","t","0.329",1502.54,800.28,33.47,236.98,344.06,87.75]
[null,null,"A.12 门窗工程"]
["60","010807001001","80系列深灰色铝合金平开窗","㎡","3.84",486.35,34.04,439.92,0.52,9.43,2.44]
[null,null,"Low-E中空玻璃（5+9A+5）"]
[null,null,"洞口面积≤2㎡"]
[null,null,"含运输、安装、配件等全部内容"]
[null,null,"品牌相当于或优于“南南铝”"]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第16页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,"A12-117换","铝合金平开窗 不带亮","100㎡","0.0384",48635.49,3403.69,{"v":43992.4,"d":"43992.40"},52.02,943.41,243.97]
["61","010807001002","80系列深灰色铝合金固定窗","㎡","15.08",447.45,23.62,415.07,0.48,6.58,{"v":1.7,"d":"1.70"}]
[null,null,"Low-E中空玻璃（5+9A+5）"]
[null,null,"洞口面积＞2㎡"]
[null,null,"含运输、安装、配件等全部内容"]
[null,null,"品牌相当于或优于“南南铝”"]
[null,"A12-118换","铝合金固定窗(矩形)","100㎡","0.1508",44745.51,2362.07,41507.11,48.17,{"v":658,"d":"658.00"},170.16]
["62","桂010811002001","门窗周边塞缝","m","227.60",7.26,{"v":4.8,"d":"4.80"},0.81,null,1.31,0.34]
[null,null,"水泥砂浆1:2.5"]
[null,"A12-166","门窗周边塞缝 水泥砂浆1:2.5{水泥砂浆 1∶2.5}","100m","2.2760",726.15,480.48,80.58,null,131.17,33.92]
[null,null,"A.13 油漆、涂料、裱糊工程"]
["63","011406003001","墙面满刮腻子","㎡","468.02",{"v":16.1,"d":"16.10"},10.36,2.18,null,2.83,0.73]
[null,null,"刮腻子三遍"]
[null,"A13-204换","刮熟胶粉腻子 内墙面 两遍[实际3]","100㎡","4.6802",{"v":1610.8,"d":"1610.80"},1036.46,218.22,null,282.95,73.17]
["64","011406003002","天棚满刮腻子","㎡","910.62",17.83,11.65,2.18,null,3.18,0.82]
[null,null,"刮腻子三遍"]
[null,"A13-204换","刮熟胶粉腻子 内墙面 两遍[实际3]","100㎡","9.1062",1783.67,1165.11,218.22,null,318.08,82.26]
["65","011406001001","米白色乳胶漆","㎡","1378.64",15.94,7.13,6.36,null,1.95,{"v":0.5,"d":"0.50"}]
[null,null,"封底涂料一道"]
[null,null,"乳液内墙涂料一道"]
[null,null,"乳胶涂料一道"]
[null,null,"品牌相当于或优于“多乐士”"]
[null,"A13-210换","乳胶漆 内墙、柱、天棚抹灰面 二遍[实际3]","100㎡","13.7864",1593.81,{"v":713,"d":"713.00"},635.82,null,194.65,50.34]
["66","011406001002","米白色硅藻泥","㎡","396.20",33.75,{"v":3.9,"d":"3.90"},28.22,0.22,1.12,0.29]
[null,null,"封底涂料一道"]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第17页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,null,"米白色硅藻泥涂料一道"]
[null,null,"米白色硅藻泥一道"]
[null,null,"品牌相当于或优于“五棵松”"]
[null,"A10-370","硅藻泥墙面（无图案不分色） 喷涂两遍成活 毛面","100㎡","3.9620",3375.18,389.95,2822.17,21.64,112.36,29.06]
["67","011406001003","抹灰面油漆","㎡","381.97",11.64,5.57,4.16,null,1.52,0.39]
[null,null,"原建筑天面喷黑漆"]
[null,null,"品牌相当于或优于“多乐士”"]
[null,"A13-210","乳胶漆 内墙、柱、天棚抹灰面 二遍","100㎡","3.8197",1164.63,556.84,416.46,null,152.02,39.31]
[null,null,"A.14 其他装饰工程"]
["68","01B001","0.8厚镀锌铁皮","㎡","130.10",50.62,7.71,{"v":39.7,"d":"39.70"},null,2.56,0.65]
[null,null,"部位：外墙面铝塑板檐口顶面"]
[null,"A7-37换","屋面铁皮","100㎡","1.3010",5062.09,771.38,3969.58,null,255.87,65.26]
["69","011508002001","定制不锈钢钛金发光字","个","8",114.49,53.28,42.23,{"v":0.5,"d":"0.50"},14.68,{"v":3.8,"d":"3.80"}]
[null,null,"规格：800×800mm"]
[null,"A14-220换","金属字 1.0以内 其他面","10个","0.8",1144.93,532.82,422.33,4.99,146.82,37.97]
["70","011508002002","定制不锈钢钛金发光字","个","32",53.74,25.85,18.85,0.12,7.09,1.83]
[null,null,"规格：300×200mm"]
[null,"A14-212换","金属字 0.2以内 其他面","10个","3.1",554.78,266.84,194.58,1.24,73.19,18.93]
["71","011508002003","5厚亚克力字","个","8",{"v":49.4,"d":"49.40"},25.05,15.74,null,6.84,1.77]
[null,null,"规格：120×120mm"]
[null,"A14-188换","泡沫塑料、有机玻璃字 0.2以内 其他面","10个","0.8",494.03,250.54,{"v":157.4,"d":"157.40"},null,{"v":68.4,"d":"68.40"},17.69]
["72","011508002004","5厚亚克力字","个","32",39.05,24.27,6.44,null,6.63,1.71]
[null,null,"规格：60×40mm"]
[null,"A14-188换","泡沫塑料、有机玻璃字 0.2以内 其他面","10个","3.1",403.13,250.54,{"v":66.5,"d":"66.50"},null,{"v":68.4,"d":"68.40"},17.69]
["73","010810005001","窗帘轨","m","33.30",21.66,{"v":3.4,"d":"3.40"},17.09,null,0.93,0.24]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第18页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,"A12-163换","明装式铝合金窗帘轨 单轨","100m","0.3330",2165.98,339.77,1709.46,null,92.76,23.99]
[null,null,"单价措施项目"]
[null,"011701","脚手架工程"]
["74","桂011701001001","扣件式钢管外脚手架 双排 10m以内","㎡","522.25",21.74,11.98,4.06,{"v":0.5,"d":"0.50"},4.14,1.06]
[null,"A15-5","扣件式钢管外脚手架 双排 10m以内","100㎡","5.2225",{"v":2174.5,"d":"2174.50"},{"v":1198.2,"d":"1198.20"},406.23,50.32,414.13,105.62]
["75","桂011701002001","扣件式钢管里脚手架 3.6m以上","㎡","770.49",8.34,4.68,1.38,0.23,1.63,0.42]
[null,"A15-2","扣件式钢管里脚手架 3.6m以上","100㎡","7.7049",834.83,468.31,138.47,23.36,163.09,{"v":41.6,"d":"41.60"}]
[null,"011702","混凝土模板及支架(撑)"]
["76","011702003001","构造柱 胶合板模板 木支撑[实际4.2]","㎡","49.50",55.51,28.89,14.23,0.25,9.67,2.47]
[null,"A17-58换","构造柱 胶合板模板 木支撑[实际4.2]","100㎡","0.4950",5550.31,2889.46,1422.64,24.94,966.71,246.56]
["77","011702008001","圈梁 直形 胶合板模板 木支撑","㎡","36.63",39.87,22.05,8.27,0.26,{"v":7.4,"d":"7.40"},1.89]
[null,"A17-72","圈梁 直形 胶合板模板 木支撑","100㎡","0.3663",3987.67,2205.22,827.29,26.21,740.17,188.78]
["78","011702009001","过梁 胶合板模板 木支撑","㎡","2.16",69.15,35.58,17.91,{"v":0.6,"d":"0.60"},{"v":12,"d":"12.00"},3.06]
[null,"A17-76","过梁 胶合板模板 木支撑","100㎡","0.0216",6915.27,3558.28,1791.28,59.59,1200.05,306.07]
["79","011702027001","台阶 木模板木支撑","㎡","4.16",35.52,19.12,{"v":7.9,"d":"7.90"},0.38,6.47,1.65]
[null,"A17-122","台阶 木模板木支撑","10㎡投影面积","0.416",355.19,191.18,79.04,{"v":3.8,"d":"3.80"},64.67,{"v":16.5,"d":"16.50"}]
["80","011702028001","扶手、压顶 木模板木支撑","m","48.50",{"v":33.4,"d":"33.40"},{"v":17.7,"d":"17.70"},7.78,0.39,{"v":6,"d":"6.00"},1.53]
[null,"A17-118","压顶、扶手 木模板木支撑","100延长米","0.485",{"v":3339.9,"d":"3339.90"},1770.25,777.84,38.73,600.04,153.04]
[null,"011705","大型机械设备进出场及安拆"]
["81","011705001001","履带式挖掘机 1以外 场外运输费","台次","1",1001.21,{"v":74.1,"d":"74.10"},156.24,680.68,{"v":71.7,"d":"71.70"},18.49]
[null,"A20-21","履带式挖掘机 1以外 场外运输费","台次","1",1001.21,{"v":74.1,"d":"74.10"},156.24,680.68,{"v":71.7,"d":"71.70"},18.49]
[null,null,"广西中医药大学教师教学发展中心装修工程-安装"]
[null,null,"分部分项工程"]
[null,null,"B4 电气设备安装工程"]
["82","030404017001","ALzm配电箱","台","1",852.52,104.34,677.69,16.09,37.07,17.33]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第19页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,null,"底边距地1.5m安装"]
[null,null,"品牌相当于或优于“正泰”"]
[null,null,"箱内元件：13个断路器,1个接触器，1个熔断器，1个时控开关"]
[null,"B4-0302换","成套配电箱安装 悬挂嵌入式(半周长m) 1","台","1",852.52,104.34,677.69,16.09,37.07,17.33]
["83","030404017002","ALG 公共照明配电箱","台","1",916.72,86.95,{"v":775.9,"d":"775.90"},10.05,29.86,13.96]
[null,null,"底边距地1.5m安装"]
[null,null,"品牌相当于或优于“正泰”"]
[null,null,"箱内元件：1个双电源自动转换开关，9个断路器，1个智能照明控制开关"]
[null,"B4-0301","成套配电箱安装 悬挂嵌入式(半周长m) 0.5","台","1",916.72,86.95,{"v":775.9,"d":"775.90"},10.05,29.86,13.96]
["84","030404017003","AL1-4配电箱","台","7",416.72,86.95,{"v":275.9,"d":"275.90"},10.05,29.86,13.96]
[null,null,"底边距地1.5m安装"]
[null,null,"品牌相当于或优于“正泰”"]
[null,null,"箱内元件：AL1、2-5个断路器,AL3-6个断路器，AL4-8个断路器"]
[null,"B4-0301","成套配电箱安装 悬挂嵌入式(半周长m) 0.5","台","7",416.72,86.95,{"v":275.9,"d":"275.90"},10.05,29.86,13.96]
["85","030404017004","AL5配电箱","台","1",616.72,86.95,{"v":475.9,"d":"475.90"},10.05,29.86,13.96]
[null,null,"底边距地1.5m安装"]
[null,null,"品牌相当于或优于“正泰”"]
[null,null,"箱内元件：15个断路器"]
[null,"B4-0301","成套配电箱安装 悬挂嵌入式(半周长m) 0.5","台","1",616.72,86.95,{"v":475.9,"d":"475.90"},10.05,29.86,13.96]
["86","030404017005","AP-KT配电箱","台","1",316.72,86.95,{"v":175.9,"d":"175.90"},10.05,29.86,13.96]
[null,null,"底边距地1.5m安装"]
[null,null,"品牌相当于或优于“正泰”"]
[null,"B4-0301","成套配电箱安装 悬挂嵌入式(半周长m) 0.5","台","1",316.72,86.95,{"v":175.9,"d":"175.90"},10.05,29.86,13.96]
["87","030411002001","防火金属线槽（MR）:100×100","m","63.98",73.04,17.71,47.12,0.14,{"v":5.5,"d":"5.50"},2.57]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第20页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,null,"梁底下200mm安装敷设"]
[null,null,"品牌相当于或优于“南宁乔顿”"]
[null,"B4-0926换","金属线槽敷设 金属线槽(宽mm以下) 100","10m","6.398",730.32,177.13,471.14,1.41,54.95,25.69]
["88","030411001001","吊顶内敷设 扣压式(KBG)、紧定式(JDG)电气钢导管规格 40","m","7.31",21.28,8.19,9.17,0.15,2.57,{"v":1.2,"d":"1.20"}]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B4-1529换","吊顶内敷设 扣压式(KBG)、紧定式(JDG)电气钢导管规格 40","100m","0.0731",2127.49,818.78,917.32,14.84,256.59,119.96]
["89","030411001002","吊顶内敷设 扣压式(KBG)、紧定式(JDG)电气钢导管规格 32","m","80.74",19.68,7.42,8.77,{"v":0.1,"d":"0.10"},2.31,1.08]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B4-1528换","吊顶内敷设 扣压式(KBG)、紧定式(JDG)电气钢导管规格 32","100m","0.8074",1967.84,741.81,877.15,9.51,231.26,108.11]
["90","030411001003","吊顶内敷设 扣压式(KBG)、紧定式(JDG)电气钢导管规格 25","m","26.22",18.34,6.75,{"v":8.4,"d":"8.40"},{"v":0.1,"d":"0.10"},2.11,0.98]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B4-1527换","吊顶内敷设 扣压式(KBG)、紧定式(JDG)电气钢导管规格 25","100m","0.2622",1833.83,674.95,{"v":840.2,"d":"840.20"},9.51,210.68,98.49]
["91","030411001004","砖、混凝土结构暗配 扣压式(KBG)、紧定式(JDG)电气钢导管规格 20","m","1291.58",11.61,5.33,3.87,null,1.64,0.77]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B4-1521换","砖、混凝土结构暗配 扣压式(KBG)、紧定式(JDG)电气钢导管规格 20","100m","12.9158",1161.06,533.05,387.23,null,164.07,76.71]
["92","030411004001","线槽内穿铜芯线WDZ-BYJ-0.45/0.75kV-6m㎡","m","803.27",5.89,0.88,4.61,null,0.27,0.13]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B4-1629换","线槽配线 动力线路 导线截面(m㎡以内) 6","100m单线","8.0327",588.63,87.72,461.29,null,{"v":27,"d":"27.00"},12.62]
["93","030411004002","管道内穿铜芯线WDZ-BYJ-0.45/0.75kV-6m㎡","m","197.46",5.76,0.57,4.93,null,0.18,0.08]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第21页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B4-1584换","管内穿线 动力线路 铜芯 导线截面(m㎡以内) 6","100m单线","1.9746",575.36,57.07,492.51,null,17.57,8.21]
["94","030411004003","线槽内穿配铜芯线WDZ-BYJ-0.45/0.75kV-10m㎡","m","228.90",9.71,0.96,8.31,null,{"v":0.3,"d":"0.30"},0.14]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B4-1630换","线槽配线 动力线路 导线截面(m㎡以内) 10","100m单线","2.289",971.25,96.23,831.55,null,29.62,13.85]
["95","030411004004","管道内穿铜芯线WDZ-BYJ-0.45/0.75kV-10m㎡","m","134.71",9.76,0.68,8.77,null,0.21,{"v":0.1,"d":"0.10"}]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B4-1585换","管内穿线 动力线路 铜芯 导线截面(m㎡以内) 10","100m单线","1.3471",975.17,67.75,876.82,null,20.85,9.75]
["96","030411004005","管道内穿配铜芯线WDZ-BYJ-0.45/0.75kV-2.5m㎡","m","3890.82",2.53,{"v":0.5,"d":"0.50"},1.81,null,0.15,0.07]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B4-1564换","管内穿线 照明线路 铜芯 导线截面(m㎡以内) 2.5","100m单线","38.9082",253.48,50.24,180.55,null,15.46,7.23]
["97","030411004006","线槽内穿配铜芯线WDZ-BYJ-0.45/0.75kV-2.5m㎡","m","101.06",2.69,0.72,1.65,null,0.22,{"v":0.1,"d":"0.10"}]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B4-1625换","线槽配线 照明线路 导线截面(m㎡以内) 2.5","100m单线","1.0106",269.51,72.01,164.98,null,22.16,10.36]
["98","030411004007","管道内穿配铜芯线WDZ-BYJ-0.45/0.75kV-4m㎡","m","1060.62",3.43,0.48,2.73,null,0.15,0.07]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B4-1565换","管内穿线 照明线路 铜芯 导线截面(m㎡以内) 4","100m单线","10.5331",344.71,47.86,275.23,null,14.73,6.89]
["99","030413002001","凿(压)槽及恢复","m","87.80",13.54,{"v":6.7,"d":"6.70"},3.47,0.24,2.13,{"v":1,"d":"1.00"}]
[null,"B4-2007","凿槽、刨沟  砖结构（公称管径32mm以内）","10m","8.780",73.73,{"v":43.8,"d":"43.80"},{"v":8.2,"d":"8.20"},1.34,13.89,{"v":6.5,"d":"6.50"}]
[null,"B4-2019","所凿沟槽恢复  沟槽尺寸（公称管径32mm以内）{水泥砂浆 1∶2.5}","10m","8.780",61.62,23.19,26.49,1.01,7.45,3.48]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第22页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
["100","030404035001","墙面插座","套","55",27.43,10.33,12.43,null,3.18,1.49]
[null,null,"单、三相暗插座 单相暗插座10A 5孔"]
[null,null,"底边距地0.3m"]
[null,null,"品牌相当于或优于“西蒙”"]
[null,"B4-0436换","单、三相暗插座 单相暗插座10A 5孔","10套","5.5",274.24,103.32,124.25,null,{"v":31.8,"d":"31.80"},14.87]
["101","030404035002","安全型地面插座","套","21",192.85,10.33,177.85,null,3.18,1.49]
[null,null,"单、三相暗插座 单相暗插座10A 5孔"]
[null,null,"嵌地安装"]
[null,null,"品牌相当于或优于“西蒙”"]
[null,"B4-0436换","单、三相暗插座 单相暗插座10A 5孔","10套","2.1",1928.48,103.32,1778.49,null,{"v":31.8,"d":"31.80"},14.87]
["102","030404035003","安全型插座","套","9",27.43,10.33,12.43,null,3.18,1.49]
[null,null,"单、三相暗插座 单相暗插座10A 5孔"]
[null,null,"投影机用，壁装"]
[null,null,"品牌相当于或优于“西蒙”"]
[null,"B4-0436换","单、三相暗插座 单相暗插座10A 5孔","10套","0.9",274.24,103.32,124.25,null,{"v":31.8,"d":"31.80"},14.87]
["103","030404035004","安全型插座","套","3",27.43,10.33,12.43,null,3.18,1.49]
[null,null,"单、三相暗插座 单相暗插座10A 5孔"]
[null,null,"电视机用，底边距地1.2m"]
[null,null,"品牌相当于或优于“西蒙”"]
[null,"B4-0436换","单、三相暗插座 单相暗插座10A 5孔","10套","0.3",274.24,103.32,124.25,null,{"v":31.8,"d":"31.80"},14.87]
["104","030404035005","防水插座","套","2",32.71,10.33,17.71,null,3.18,1.49]
[null,null,"单、三相暗插座 单相暗插座10A 5孔"]
[null,null,"配防溅盒，底边距地1.2m"]
[null,null,"品牌相当于或优于“西蒙”"]
[null,"B4-0436换","单、三相暗插座 单相暗插座10A 5孔","10套","0.2",327.08,103.32,177.09,null,{"v":31.8,"d":"31.80"},14.87]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第23页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
["105","030404034001","开关、按钮、插座安装 开关及按钮 跷板暗开关(单控) 单联","套","1",20.08,8.67,7.49,null,2.67,1.25]
[null,null,"品牌相当于或优于“西蒙”"]
[null,"B4-0412换","开关、按钮、插座安装 开关及按钮 跷板暗开关(单控) 单联","10套","0.1",200.75,86.69,74.91,null,26.68,12.47]
["106","030404034002","开关、按钮、插座安装 开关及按钮 跷板暗开关(单控) 双联","套","10",23.27,8.93,{"v":10.3,"d":"10.30"},null,2.75,1.29]
[null,null,"品牌相当于或优于“西蒙”"]
[null,"B4-0413换","开关、按钮、插座安装 开关及按钮 跷板暗开关(单控) 双联","10套","1",232.71,89.34,103.01,null,{"v":27.5,"d":"27.50"},12.86]
["107","030404034003","开关、按钮、插座安装 开关及按钮 跷板暗开关(单控) 三联","套","12",32.42,{"v":9.2,"d":"9.20"},19.07,null,2.83,1.32]
[null,null,"品牌相当于或优于“西蒙”"]
[null,"B4-0414换","开关、按钮、插座安装 开关及按钮 跷板暗开关(单控) 三联","10套","1.2",324.22,91.98,190.69,null,28.31,13.24]
["108","030404034004","开关、按钮、插座安装 开关及按钮 跷板暗开关(双控) 单联","套","2",19.83,8.87,6.95,null,2.73,1.28]
[null,null,"品牌相当于或优于“西蒙”"]
[null,"B4-0418换","开关、按钮、插座安装 开关及按钮 跷板暗开关(双控) 单联","10套","0.2",198.29,88.69,69.54,null,{"v":27.3,"d":"27.30"},12.76]
["109","030404034005","开关、按钮、插座安装 开关及按钮 跷板暗开关(双控) 双联","套","4",28.97,9.13,15.72,null,2.81,1.31]
[null,null,"品牌相当于或优于“西蒙”"]
[null,"B4-0419换","开关、按钮、插座安装 开关及按钮 跷板暗开关(双控) 双联","10套","0.4",289.81,91.34,157.22,null,28.11,13.14]
["110","030412001001","6寸LED筒灯","套","27",64.41,16.05,41.11,null,4.94,2.31]
[null,null,"15W   ~220V  1300lm  4000K"]
[null,null,"嵌入安装"]
[null,null,"品牌相当于或优于“三极雄光”"]
[null,"B4-1853换","装饰灯具安装 点光源艺术装饰灯具 筒灯 嵌入式 灯具直径(150)","10套","2.7",643.99,160.45,411.06,null,49.39,23.09]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第24页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
["111","030412001002","8寸LED筒灯","套","10",66.43,16.05,43.13,null,4.94,2.31]
[null,null,"18W   ~220V  1500lm  4000K"]
[null,null,"嵌入安装"]
[null,null,"品牌相当于或优于“三极雄光”"]
[null,"B4-1853换","装饰灯具安装 点光源艺术装饰灯具 筒灯 嵌入式 灯具直径(150)","10套","1",664.19,160.45,431.26,null,49.39,23.09]
["112","030412001003","LED可调式天花小射灯","套","66",60.94,8.49,48.25,0.25,2.69,1.26]
[null,null,"15W   ～220V  1062lm  4000K（24°）"]
[null,null,"嵌入安装"]
[null,null,"品牌相当于或优于“三极雄光”"]
[null,"B4-1856换","装饰灯具安装 点光源艺术装饰灯具 射灯 吸顶式","10套","6.6",609.37,{"v":84.9,"d":"84.90"},482.54,2.47,26.89,12.57]
["113","030412001004","双头LED格栅射灯","套","6",101.34,8.49,88.65,0.25,2.69,1.26]
[null,null,"2*15W   ～220V  2150lm  （24°）"]
[null,null,"嵌入安装"]
[null,null,"品牌相当于或优于“三极雄光”"]
[null,"B4-1856换","装饰灯具安装 点光源艺术装饰灯具 射灯 吸顶式","10套","0.6",1013.37,{"v":84.9,"d":"84.90"},886.54,2.47,26.89,12.57]
["114","030412001005","成品工艺吊灯","套","10",151.55,14.32,130.55,0.15,4.45,2.08]
[null,null,"  15W  ~220V 1300lm(吊线式)"]
[null,null,"底距地3.2/2.2m"]
[null,null,"品牌相当于或优于“三极雄光”"]
[null,"B4-1749换","其他普通灯具 吊链灯","10套","1",1515.46,143.18,1305.45,1.48,44.53,20.82]
["115","030412001006","LED平面灯盘(300x1200mm)","套","63",191.95,14.32,170.95,0.15,4.45,2.08]
[null,null,"2x16W  ~220V 2250lm(吊线式)"]
[null,null,"品牌相当于或优于“三极雄光”"]
[null,"B4-1749换","其他普通灯具 吊链灯","10套","6.3",1919.46,143.18,1709.45,1.48,44.53,20.82]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第25页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
["116","030412001007","LED平面灯盘(300x1200mm)","套","32",192.54,19.07,{"v":164.5,"d":"164.50"},0.25,5.94,2.78]
[null,null,"35W  ~220V 2000lm"]
[null,null,"嵌入安装"]
[null,null,"品牌相当于或优于“三极雄光”"]
[null,"B4-1746换","普通灯具安装 吸顶灯具 灯罩周长 2000mm以上","10套","3.2",1925.36,190.65,1645.01,2.47,59.44,27.79]
["117","030412001008","LED平面灯盘(300x300mm)","套","6",108.71,19.07,80.67,0.25,5.94,2.78]
[null,null,"12W  ~220V  800lm"]
[null,null,"嵌入安装",null,"5"]
[null,null,"品牌相当于或优于“三极雄光”"]
[null,"B4-1746换","普通灯具安装 吸顶灯具 灯罩周长 2000mm以上","10套","0.6",1087.06,190.65,806.71,2.47,59.44,27.79]
["118","030412001009","LED高压软灯带","m","271.54",29.49,{"v":2,"d":"2.00"},25.87,0.49,0.77,0.36]
[null,null,"PAK544217 AC200V/灯盒内安装8W/m/4000K/发光角度140°/光通量(450lm/m)"]
[null,null,"壁装"]
[null,null,"品牌相当于或优于“三极雄光”"]
[null,"B4-1990换","其他照明灯具安装  LED光灯带","10m","27.154",294.86,19.97,{"v":258.7,"d":"258.70"},4.94,7.67,3.58]
[null,null,"广西中医药大学教师教学发展中心装修工程-消防"]
[null,null,"分部分项工程"]
[null,null,"消火栓系统"]
["119","030901002001","消火栓热镀锌钢管及管件安装","m","86.31",{"v":138.5,"d":"138.50"},25.78,100.59,0.33,8.04,3.76]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：沟槽连接"]
[null,null,"规格型号：DN100"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B9-0038换","消火栓热镀锌钢管(沟槽连接)安装 DN100","10m","8.631",1385.02,257.83,1005.95,3.29,80.37,37.58]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第26页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
["120","031002001001","管道支架制作安装","kg","96.93",{"v":20.6,"d":"20.60"},5.79,11.05,0.89,1.96,0.91]
[null,null,"支架的材质不详，暂按40*4热镀锌角钢计，结算按实调整"]
[null,null,"面刷防锈漆二道，红色调和漆二道"]
[null,"B4-2001换","一般铁构件制作安装","100kg","0.9693",{"v":1846.2,"d":"1846.20"},498.53,1051.78,{"v":48.7,"d":"48.70"},168.44,78.75]
[null,"B11-0119","金属结构刷油 一般钢结构 防锈漆 第一遍","100kg","0.9693",55.62,19.84,16.01,10.01,6.81,2.95]
[null,"B11-0120","金属结构刷油 一般钢结构 防锈漆 第二遍","100kg","0.9693",53.29,19.84,13.68,10.01,6.81,2.95]
[null,"B11-0126","金属结构刷油 一般钢结构 调和漆 第一遍","100kg","0.9693",53.17,20.49,12.71,10.01,6.95,3.01]
[null,"B11-0127","金属结构刷油 一般钢结构 调和漆 第二遍","100kg","0.9693",50.74,19.84,11.13,10.01,6.81,2.95]
["121","030901010001","室内消火栓","套","6",859.59,148.14,643.71,0.57,45.77,{"v":21.4,"d":"21.40"}]
[null,null,"安装方式：半暗装型"]
[null,null,"规格型号：箱子尺寸1000X700X240mm"]
[null,null,"配直流水枪1支,规格为:65mmX19mm;消防龙带:材质用衬胶。口径65mm 长度及条数:25m长配1条。"]
[null,"B9-0832换","甲型单栓带消防软管卷盘消火栓 箱子尺寸1000X700X240mm","套","6",859.59,148.14,643.71,0.57,45.77,{"v":21.4,"d":"21.40"}]
[null,null,"自动喷淋系统"]
["122","030901001001","喷淋热镀锌钢管及管件安装","m","31.00",219.21,31.35,173.32,0.26,9.73,4.55]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：沟槽连接"]
[null,null,"规格型号：DN150"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B9-0040换","喷淋热镀锌钢管(沟槽连接)安装 DN150","10m","3.100",2191.99,313.48,1733.15,2.59,97.29,45.48]
["123","030901001002","喷淋热镀锌钢管及管件安装","m","4.25",202.52,28.57,160.82,0.16,8.84,4.13]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：沟槽连接"]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第27页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,null,"规格型号：DN125"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B9-0039换","喷淋热镀锌钢管(沟槽连接)安装 DN125","10m","0.425",{"v":2025.1,"d":"2025.10"},285.66,1608.13,1.57,88.41,41.33]
["124","030901001003","喷淋热镀锌钢管及管件安装","m","8.59",{"v":138.5,"d":"138.50"},25.78,100.59,0.33,8.04,3.76]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：沟槽连接"]
[null,null,"规格型号：DN100"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B9-0038换","喷淋热镀锌钢管(沟槽连接)安装 DN100","10m","0.859",1385.02,257.83,1005.95,3.29,80.37,37.58]
["125","030901001004","喷淋热镀锌钢管及管件安装","m","35.26",108.08,23.56,73.19,0.47,{"v":7.4,"d":"7.40"},3.46]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：沟槽连接"]
[null,null,"规格型号：DN80"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B9-0037换","喷淋热镀锌钢管(沟槽连接)安装 DN80","10m","3.526",1080.82,235.62,{"v":731.9,"d":"731.90"},4.73,73.98,34.59]
["126","030901001005","喷淋热镀锌钢管及管件安装","m","10.65",108.08,23.56,73.19,0.47,{"v":7.4,"d":"7.40"},3.46]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：沟槽连接"]
[null,null,"规格型号：DN65"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B9-0037换","喷淋热镀锌钢管(沟槽连接)安装 DN80","10m","1.065",1080.82,235.62,{"v":731.9,"d":"731.90"},4.73,73.98,34.59]
["127","030901001006","喷淋热镀锌钢管及管件安装","m","27.81",73.08,{"v":23.1,"d":"23.10"},38.57,0.67,7.32,3.42]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：螺纹连接"]
[null,null,"规格型号：DN50"]
[null,null,"品牌相当于或优于“雄塑”"]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第28页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,"B9-0005换","喷淋热镀锌钢管(螺纹连接)安装 DN50","10m","2.781",730.69,230.97,385.68,6.69,73.15,{"v":34.2,"d":"34.20"}]
["128","030901001007","喷淋热镀锌钢管及管件安装","m","36.33",62.97,22.26,29.81,0.58,7.03,3.29]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：螺纹连接"]
[null,null,"规格型号：DN40"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B9-0004换","喷淋热镀锌钢管(螺纹连接)安装 DN40","10m","3.633",629.71,{"v":222.6,"d":"222.60"},298.09,5.84,70.31,32.87]
["129","030901001008","喷淋热镀锌钢管及管件安装","m","201.75",54.15,19.85,24.58,0.52,6.27,2.93]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：螺纹连接"]
[null,null,"规格型号：DN32"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B9-0003换","喷淋热镀锌钢管(螺纹连接)安装 DN32","10m","20.175",541.49,198.51,245.82,5.16,62.69,29.31]
["130","030901001009","喷淋热镀锌钢管及管件安装","m","190.09",50.05,19.21,21.62,0.37,6.03,2.82]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：螺纹连接"]
[null,null,"规格型号：DN25"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B9-0002换","喷淋热镀锌钢管(螺纹连接)安装 DN25","10m","19.009",500.39,192.07,216.22,3.68,60.25,28.17]
["131","031002001002","管道支架","kg","290.33",{"v":20.6,"d":"20.60"},5.79,11.05,0.89,1.96,0.91]
[null,null,"管道支架制作安装"]
[null,null,"面刷防锈漆二道，红色调和漆二道"]
[null,"B4-2001换","一般铁构件制作安装","100kg","2.9033",{"v":1846.2,"d":"1846.20"},498.53,1051.78,{"v":48.7,"d":"48.70"},168.44,78.75]
[null,"B11-0119","金属结构刷油 一般钢结构 防锈漆 第一遍","100kg","2.9033",55.62,19.84,16.01,10.01,6.81,2.95]
[null,"B11-0120","金属结构刷油 一般钢结构 防锈漆 第二遍","100kg","2.9033",53.29,19.84,13.68,10.01,6.81,2.95]
[null,"B11-0126","金属结构刷油 一般钢结构 调和漆 第一遍","100kg","2.9033",53.17,20.49,12.71,10.01,6.95,3.01]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第29页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,"B11-0127","金属结构刷油 一般钢结构 调和漆 第二遍","100kg","2.9033",50.74,19.84,11.13,10.01,6.81,2.95]
["132","030901003001","玻璃球闭式喷头DN15,喷头动作温度68℃","个","159",30.23,{"v":12.5,"d":"12.50"},11.13,0.66,4.05,1.89]
[null,null,"安装方式  有吊顶"]
[null,"B9-0800换","闭式喷头安装 公称直径15mm以内 有吊顶","10个","15.9",302.17,124.96,111.21,6.58,40.49,18.93]
["133","030901008001","末端试水阀","组","1",{"v":40.4,"d":"40.40"},7.73,29.18,null,2.38,1.11]
[null,null,"规格型号 DN25"]
[null,"B9-0315换","螺纹阀门安装 螺纹阀 公称直径(mm以内) 25","个","1",{"v":40.4,"d":"40.40"},7.73,29.18,null,2.38,1.11]
["134","030901008002","末端试水装置","组","1",296.23,97.26,152.05,2.06,30.57,14.29]
[null,null,"规格型号 DN25"]
[null,"B9-0827换","末端试水装置安装 DN25","组","1",296.23,97.26,152.05,2.06,30.57,14.29]
["135","030905002001","水灭火控制装置调试","点","1",139.62,78.31,{"v":2.6,"d":"2.60"},16.08,29.05,13.58]
[null,"B5-1391","水灭火控制装置调试 自动喷水灭火系统","点","1",139.62,78.31,{"v":2.6,"d":"2.60"},16.08,29.05,13.58]
[null,null,"火灾自动报警系统"]
["136","030904001001","编码型感烟探测器","个","32",262.66,38.93,205.36,0.54,12.15,5.68]
[null,null,"安装方式 吸顶"]
[null,"B5-1308换","编码型感烟探测器","个","32",262.66,38.93,205.36,0.54,12.15,5.68]
["137","030904003001","编码型手动报警按钮 带电话插孔","个","4",277.82,57.72,193.95,0.06,17.78,8.31]
[null,null,"1.安装方式:距地1.4m安装"]
[null,"B5-1316换","编码型手动报警按钮 带电话插孔","个","4",277.82,57.72,193.95,0.06,17.78,8.31]
["138","030904008001","短路隔离器","个","2",271.86,92.03,136.39,1.29,28.72,13.43]
[null,"B5-1329换","短路隔离器","个","2",271.86,92.03,136.39,1.29,28.72,13.43]
["139","030904007001","火灾警报扬声器","个","10",101.75,21.26,70.09,0.55,6.71,3.14]
[null,null,"1.功率:12V 3W"]
[null,null,"2.安装方式:吸顶"]
[null,"B5-1327换","火灾警报扬声器","个","10",101.75,21.26,70.09,0.55,6.71,3.14]
["140","030904005001","火灾声光警报器","个","4",307.36,44.67,241.71,0.55,13.92,6.51]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第30页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,null,"1.安装方式:距地2.4m安装"]
[null,"B5-1318换","火灾声光警报器","个","4",307.36,44.67,241.71,0.55,13.92,6.51]
["141","030904003002","消防栓起泵按钮","个","6",237.42,57.72,153.55,0.06,17.78,8.31]
[null,"B5-1316换","按钮安装 消防栓起泵按钮","个","6",237.42,57.72,153.55,0.06,17.78,8.31]
["142","030411004008","管内穿报警线 ZR-RVS-2x1.0","m","597.97",4.33,0.59,3.47,null,0.18,0.09]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B4-1611换","报警线 ZR-RVS-2x1.0","100m束","5.9797",432.66,59.19,346.73,null,18.22,8.52]
["143","030411004009","管内穿电源线 NH-BV-750V-4","m","1722.16",4.23,{"v":0.5,"d":"0.50"},3.51,null,0.15,0.07]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B4-1582换","电源线回路  NH-BV-750V-4","100m单线","17.2216",423.27,49.92,{"v":350.8,"d":"350.80"},null,15.37,7.18]
["144","030411004010","管内穿消防广播回路 NH-RVVP-250V-2x1.5","m","263.11",{"v":5.4,"d":"5.40"},0.59,4.51,0.02,0.19,0.09]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B5-0257换","消防广播回路 NH-RVVP-250V-2x1.5","100m","2.6311",540.03,58.92,450.97,2.43,18.88,8.83]
["145","030411001005","配管","m","1459.05",14.31,{"v":4.9,"d":"4.90"},6.88,0.22,1.57,0.74]
[null,null,"材质 钢管"]
[null,null,"规格 SC15"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B4-1417换","电线管敷设 砖、混凝土结构暗配 电线管公称口径(mm以内)15","100m","14.5905",{"v":1430.6,"d":"1430.60"},489.58,688.09,{"v":21.9,"d":"21.90"},157.43,{"v":73.6,"d":"73.60"}]
["146","030413002002","管道DN25 凿槽及恢复","m","44.00",17.11,9.18,3.31,0.32,2.93,1.37]
[null,"B4-2012","凿槽、刨沟  混凝土结构（公称管径15mm以内）","10m","4.400",121.89,73.81,{"v":11.2,"d":"11.20"},2.44,23.47,10.97]
[null,"B4-2018","所凿沟槽恢复  沟槽尺寸（公称管径20mm以内）{水泥砂浆 1∶2.5}","10m","4.400",49.18,18.03,21.86,0.79,5.79,2.71]
["147","030905001001","自动报警系统调试","系统","1",16399.49,10560.01,289.11,537.59,3415.84,1596.94]
[null,"B5-1383","自动报警系统调试 500点以下","系统","1",16399.49,10560.01,289.11,537.59,3415.84,1596.94]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第31页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,null,"应急照明"]
["148","030412001010","带蓄电池应急双头灯","套","13",147.22,15.88,123.95,0.15,4.93,2.31]
[null,null,"型号规格 2x5W LED灯 ~220V A型灯具"]
[null,null,"距地2.5米安装,5W,90min"]
[null,null,"无墙体位置吊装,距地大于2.2m"]
[null,"B4-1846换","自带电源事故照明灯","10套","1.3",1472.12,158.78,1239.47,1.48,49.33,23.06]
["149","030412001011","安全出口标志灯","套","6",{"v":165.4,"d":"165.40"},15.88,142.13,0.15,4.93,2.31]
[null,null,"型号规格  1x3W LED灯 ~220V A型灯具"]
[null,null,"门上0.2米安装,3W,90min"]
[null,"B4-1846换","安全出口标志灯","10套","0.6",1653.92,158.78,1421.27,1.48,49.33,23.06]
["150","030412001012","单向疏散指示灯","套","10",101.77,15.88,{"v":78.5,"d":"78.50"},0.15,4.93,2.31]
[null,null,"型号规格 1x3W LED灯 ~220V A型灯具"]
[null,null,"距地0.5米安装,5W,90min"]
[null,"B4-1846换","单向疏散指示灯","10套","1",1017.62,158.78,784.97,1.48,49.33,23.06]
["151","030412001013","双向疏散指示灯","套","1",101.77,15.88,{"v":78.5,"d":"78.50"},0.15,4.93,2.31]
[null,null,"型号规格 1x3W LED灯 ~220V A型灯具"]
[null,null,"安装方式  距地0.5m壁装"]
[null,"B4-1846换","双向疏散指示灯","10套","0.1",1017.62,158.78,784.97,1.48,49.33,23.06]
["152","030411004011","管内穿线NH-BV-2.5","m","609.30",4.05,{"v":0.5,"d":"0.50"},3.33,null,0.15,0.07]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B4-1582换","管内穿线 动力线路 铜芯 导线截面(m㎡以内) 2.5","100m单线","6.093",405.42,49.92,332.95,null,15.37,7.18]
["153","030411001006","配管","m","203.10",16.98,5.38,8.85,0.22,1.72,0.81]
[null,null,"材质 钢管"]
[null,null,"规格 SC20"]
[null,null,"品牌相当于或优于“雄塑”"]
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":7},"第32页 共32页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价","综合单价"]
[{"$nulls":5},"（元）","人工费","材料费","机械费","管理费","利润","其中:\r\n暂估价"]
[null,"B4-1418换","电线管敷设 砖、混凝土结构暗配 电线管公称口径(mm以内)20","100m","2.0310",1698.89,538.47,{"v":885.4,"d":"885.40"},{"v":21.9,"d":"21.90"},172.48,80.64]
["154","030413002003","管道DN20 凿(压)槽及恢复","m","54.00",17.11,9.18,3.31,0.32,2.93,1.37]
[null,"B4-2012","凿槽、刨沟  混凝土结构（公称管径20mm以内）","10m","5.400",121.89,73.81,{"v":11.2,"d":"11.20"},2.44,23.47,10.97]
[null,"B4-2018","所凿沟槽恢复  沟槽尺寸（公称管径20mm以内）{水泥砂浆 1∶2.5}","10m","5.400",49.18,18.03,21.86,0.79,5.79,2.71]
{"$rows_empty":20}
[" ",null,null," ",null,null," "," "," "," ",null,"表－09"]

{"sheet":"表-11_总价措施项目清单与计价表","index":7,"n_rows":29,"n_cols":7,"rows_kept":29,"merged":[[0,0,0,6],[1,0,1,4],[5,3,6,3],[9,3,12,3],[15,3,17,3],[21,3,23,3],[27,0,27,6]],"flags":["formulas_cached_only"]}
["总价措施项目清单与计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程   ",{"$nulls":5},"第1页 共1页"]
["序\r\n号","项目编码","项 目 名 称","计 算 基 础","费 率(%)\r\n或标准","金 额(元)","备注"]
[null,null,"广西中医药大学教师教学发展中心装修工程-拆除",null,null,82.58]
["一",null,"建筑拆除工程(营改增)简易计税法",null,null,82.58]
["2","桂011801001001","安全文明施工费","∑(分部分项人材机+单价措施人材机)\r\n(3670.15+0)","2.00",{"v":73.4,"d":"73.40"}]
["4","桂011801003001","雨季施工增加费",null,"0.25",9.18]
[null,null,"广西中医药大学教师教学发展中心装修工程-装饰装修",null,null,77286.94]
["一",null,"建筑装饰装修工程(营改增)一般计税法",null,null,77286.94]
["1","桂011801001001","安全文明施工费","∑(分部分项人材机+单价措施人材机)\r\n(940938.41+19147.92)","7.36",70662.35]
["2","桂011801002001","检验试验配合费",null,"0.11",1056.09]
["3","桂011801003001","雨季施工增加费",null,"0.53",5088.46]
["4","桂011801004001","工程定位复测费",null,"0.05",480.04]
[null,null,"广西中医药大学教师教学发展中心装修工程-安装",null,null,4107.99]
["一",null,"给排水、燃气、电气、通风空调、消防、建筑智能、通信、自控仪表工程(营改增)一般计税法",null,null,4107.99]
["1","桂031401001001","安全文明施工费","∑分部分项及单价措施费定额(人工费+机械费)\r\n(18783.86+329.91+0+0)","12.12",2316.59]
["2","桂031401002001","检验试验配合费",null,"0.51",97.48]
["3","桂031401003001","雨季施工增加费",null,"4.09",781.75]
["10","桂031401010001","脚手架搭拆费",null,null,912.17]
[null,null,"广西中医药大学教师教学发展中心装修工程-消防",null,null,9694.03]
["一",null,"给排水、燃气、电气、通风空调、消防、建筑智能、通信、自控仪表工程(营改增)一般计税法",null,null,9694.03]
["1","桂031401001001","安全文明施工费","∑分部分项及单价措施费定额(人工费+机械费)\r\n(43280.93+1720.27+0+0)","12.12",5454.15]
["2","桂031401002001","检验试验配合费",null,"0.51",229.51]
["3","桂031401003001","雨季施工增加费",null,"4.09",1840.55]
["10","桂031401010001","脚手架搭拆费",null,null,2169.82]
[null,null,"      合     计",null,null,91171.54]
[]
["注：以项计算的总价措施，无“计算基础”和“费率”的数值，可只填“金额”数值，但应在备注栏说明施工方案出处或计算方式。"]
[{"$nulls":6},"表-11"]

{"sheet":"表-12_其他项目清单与计价汇总表","index":8,"n_rows":42,"n_cols":4,"rows_kept":42,"merged":[[0,0,0,3],[1,0,1,2],[41,0,41,2]],"flags":["formulas_cached_only"]}
["其他项目清单与计价汇总表"]
["工程名称:广西中医药大学教师教学发展中心装修工程   ",null,null,"第1页 共1页"]
["序号","项目名称","金额（元）","备注"]
[null,"广西中医药大学教师教学发展中心装修工程-拆除"]
["1","暂列金额",null,"明细详见表－12－1"]
["2","材料暂估价",null,"明细详见表－12－2"]
["3","专业工程暂估价",null,"明细详见表－12－3"]
["4","计日工",null,"明细详见表－12－4"]
["5","总承包服务费",null,"明细详见表－12－5"]
[null,"广西中医药大学教师教学发展中心装修工程-装饰装修"]
["1","暂列金额",null,"明细详见表－12－1"]
["2","材料暂估价",null,"明细详见表－12－2"]
["3","专业工程暂估价",null,"明细详见表－12－3"]
["4","计日工",null,"明细详见表－12－4"]
["5","总承包服务费",null,"明细详见表－12－5"]
[null,"广西中医药大学教师教学发展中心装修工程-安装"]
["1","暂列金额",null,"明细详见表－12－1"]
["2","材料暂估价",null,"明细详见表－12－2"]
["3","专业工程暂估价",null,"明细详见表－12－3"]
["4","计日工",null,"明细详见表－12－4"]
["5","总承包服务费",null,"明细详见表－12－5"]
[null,"广西中医药大学教师教学发展中心装修工程-消防"]
["1","暂列金额",null,"明细详见表－12－1"]
["2","材料暂估价",null,"明细详见表－12－2"]
["3","专业工程暂估价",null,"明细详见表－12－3"]
["4","计日工",null,"明细详见表－12－4"]
["5","总承包服务费",null,"明细详见表－12－5"]
[null,"            合           计"]
{"$rows_empty":13}
["注:材料暂估单价进入清单综合单价，此处不汇总。",null,null,"表－12"]

{"sheet":"表-15_规费、增值税计价表","index":9,"n_rows":99,"n_cols":5,"rows_kept":99,"merged":[[0,0,0,4],[1,0,1,3],[6,2,11,2],[12,2,13,2],[14,2,19,2],[23,2,27,2],[29,0,29,4],[30,0,30,3],[32,2,33,2],[39,2,46,2],[51,2,57,2],[59,0,59,4],[60,0,60,3]],"flags":["formulas_cached_only"]}
["规费、增值税计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程",{"$nulls":3},"第1页 共3页"]
["序号","项目名称","计算基础","计算费率(%)","金额(元)"]
[null,"广西中医药大学教师教学发展中心装修工程-拆除",null,null,785.36]
["一","建筑拆除工程(营改增)简易计税法",null,null,785.36]
["1","规费","1+2+3",null,622.38]
["1.1","社会保险费","∑(分部分项人工费+单价措施人工费)\r\n(1960.37+0)","29.35",575.37]
["1.1.1","养老保险费",null,"17.22",337.58]
["1.1.2","失业保险费",null,"0.34",6.67]
["1.1.3","医疗保险费",null,"10.25",200.94]
["1.1.4","生育保险费",null,"0.64",12.55]
["1.1.5","工伤保险费",null,"0.90",17.64]
["1.2","住房公积金","分部分项及单价措施工程费+总价措施项目费+其他项目费\r\n(4005.36+82.58+0)","1.02",{"v":41.7,"d":"41.70"}]
["1.3","工程排污费",null,"0.13",5.31]
["2","税金","分部分项及单价措施工程费+总价措施项目费+其他项目费+税前项目费+规费\r\n(4005.36+82.58+0+0+622.38)","3.46",162.98]
["2.1","增值税",null,"3.00",141.31]
["2.2","城市维护建设税",null,"0.21",9.89]
["2.3","教育附加费",null,"0.09",4.24]
["2.4","地方教育附加费",null,"0.06",2.83]
["2.5","水利建设基金",null,"0.10",4.71]
[null,"广西中医药大学教师教学发展中心装修工程-装饰装修",null,null,218425.96]
["一","建筑装饰装修工程(营改增)一般计税法",null,null,218425.96]
["1","规费","1.1+1.2+1.3",null,80966.04]
["1.1","社会保险费","∑(分部分项人工费+单价措施人工费)\r\n(233085.45+13189.14)","29.35",72281.59]
["1.1.1","养老保险费",null,"17.22",42408.48]
["1.1.2","失业保险费",null,"0.34",837.33]
["1.1.3","医疗保险费",null,"10.25",25243.15]
["1.1.4","生育保险费",null,"0.64",1576.16]
[{"$nulls":4},"表-15"]
["规费、增值税计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程",{"$nulls":3},"第2页 共3页"]
["序号","项目名称","计算基础","计算费率(%)","金额(元)"]
["1.1.5","工伤保险费","∑(分部分项人工费+单价措施人工费)\r\n(233085.45+13189.14)","0.90",2216.47]
["1.2","住房公积金",null,"1.85",4556.08]
["1.3","工程排污费","∑(分部分项人材机+单价措施人材机)\r\n(940938.41+19147.92)","0.43",4128.37]
["2","增值税","Σ（分部分项工程费及单价措施项目费+总价措施项目费+其他项目费+税前项目费+规费）\r\n(1051885.29+77286.94+0+317194.12+80966.04)","9.00",137459.92]
[null,"广西中医药大学教师教学发展中心装修工程-安装",null,null,15306.41]
["一","给排水、燃气、电气、通风空调、消防、建筑智能、通信、自控仪表工程(营改增)一般计税法",null,null,15306.41]
["1","规费","1.1+1.2+1.3",null,{"v":5935.7,"d":"5935.70"}]
["1.1","社会保险费","∑(分部分项人工费+单价措施人工费)\r\n(18783.86+0)","29.35",5513.06]
["1.1.1","养老保险费",null,"17.22",3234.58]
["1.1.2","失业保险费",null,"0.34",63.87]
["1.1.3","医疗保险费",null,"10.25",1925.35]
["1.1.4","生育保险费",null,"0.64",120.22]
["1.1.5","工伤保险费",null,"0.90",169.05]
["1.2","住房公积金",null,"1.85",{"v":347.5,"d":"347.50"}]
["1.3","工程排污费",null,"0.40",75.14]
["2","增值税","Σ（分部分项工程费及单价措施项目费+总价措施项目费+其他项目费+税前项目费+规费）\r\n(94075.32+4107.99+0+0+5935.7)","9.00",9370.71]
[null,"广西中医药大学教师教学发展中心装修工程-消防",null,null,28637.74]
["一","给排水、燃气、电气、通风空调、消防、建筑智能、通信、自控仪表工程(营改增)一般计税法",null,null,28637.74]
["1","规费","1.1+1.2+1.3",null,13676.77]
["1.1","社会保险费","∑(分部分项人工费+单价措施人工费)\r\n(43280.93+0)","29.35",12702.95]
["1.1.1","养老保险费",null,"17.22",7452.98]
["1.1.2","失业保险费",null,"0.34",147.16]
["1.1.3","医疗保险费",null,"10.25",{"v":4436.3,"d":"4436.30"}]
["1.1.4","生育保险费",null,"0.64",{"v":277,"d":"277.00"}]
["1.1.5","工伤保险费",null,"0.90",389.53]
["1.2","住房公积金",null,"1.85",{"v":800.7,"d":"800.70"}]
[{"$nulls":4},"表-15"]
["规费、增值税计价表"]
["工程名称:广西中医药大学教师教学发展中心装修工程",{"$nulls":3},"第3页 共3页"]
["序号","项目名称","计算基础","计算费率(%)","金额(元)"]
["1.3","工程排污费","∑(分部分项人工费+单价措施人工费)\r\n(43280.93+0)","0.40",173.12]
["2","增值税","Σ（分部分项工程费及单价措施项目费+总价措施项目费+其他项目费+税前项目费+规费）\r\n(142862.2+9694.03+0+0+13676.77)","9.00",14960.97]
[null,"       合          计",null,null,263155.47]
{"$rows_empty":33}
[{"$nulls":4},"表-15"]

{"sheet":"主要材料及价格表(有信息价)","index":10,"n_rows":117,"n_cols":6,"rows_kept":117,"merged":[[0,0,0,5],[1,0,1,2],[1,4,1,5],[42,0,42,5],[43,0,43,2],[43,4,43,5],[84,0,84,5],[85,0,85,2],[85,4,85,5]],"flags":["formulas_cached_only"]}
["主要材料及价格表"]
["工程名称:广西中医药大学教师教学发展中心装修工程",{"$nulls":3},"第1页  共3页"]
["序号","材料编码","项目名称及规格、型号等特殊要求","单位","数量","单价（元）"]
[1,"R0101001","建筑综合工日(一类)","工日",30.632,{"v":64,"d":"64.00"}]
[2,"010103001","螺纹钢筋HRB400 10以内(综合)","t",0.036,{"v":5569,"d":"5569.00"}]
[3,"010310001","镀锌铁丝(综合)","kg",4.156,6.02]
[4,"010310002","镀锌铁丝 Φ4","kg",22.531,{"v":5,"d":"5.00"}]
[5,"010310004","镀锌铁丝 Φ2.8","kg",47.055,{"v":5,"d":"5.00"}]
[6,"010310013","镀锌铁丝 Φ0.7","kg",{"v":30.46,"d":"30.460"},{"v":5,"d":"5.00"}]
[7,"010902001","圆钢HPB300 Φ10以内(综合)","t",1.316,{"v":5629,"d":"5629.00"}]
[8,"010902002","圆钢HPB300 Φ10以上(综合)","t",0.408,{"v":5799,"d":"5799.00"}]
[9,"011301001","扁钢(综合)","t",0.001,{"v":5461,"d":"5461.00"}]
[10,"012102001","等边角钢(综合)","t",{"v":0.04,"d":"0.040"},{"v":5724,"d":"5724.00"}]
[11,"012703001","镀锌型钢(综合)","t",5.356,{"v":5800,"d":"5800.00"}]
[12,"012901001","钢板(综合)","t",0.292,{"v":5815,"d":"5815.00"}]
[13,"012907006","0.8厚镀锌铁皮","㎡",137.125,{"v":37,"d":"37.00"}]
[14,"023501001","浅咖啡色仿布纹硬包","㎡",70.807,{"v":149,"d":"149.00"}]
[15,"030139001","穿墙螺栓 M16","套",1940.352,4.34]
[16,"030156001","膨胀螺栓","套",3588.656,0.53]
[17,"031311001","电焊条（综合）","kg",138.309,{"v":6.5,"d":"6.50"}]
[18,"032118014","镀锌全螺纹吊杆Φ8","m",{"v":2408.47,"d":"2408.470"},1.59]
[19,"040102001","普通硅酸盐水泥 32.5MPa","t",27.582,481.42]
[20,"040102004","普通硅酸盐水泥 42.5MPa","kg",{"v":8.58,"d":"8.580"},{"v":0.4,"d":"0.40"}]
[21,"040103001","白水泥(综合)","t",0.086,725.66]
[22,"040103002","白水泥(综合)","kg",{"v":1188.6,"d":"1188.600"},0.72]
[23,"040301001","砂(综合)","",{"v":17.05,"d":"17.050"},179.61]
[24,"040301004","中砂","",80.965,184.47]
[25,"040902001","生石灰","kg",2696.215,0.78]
[26,"040902004","石灰膏","",4.501,320.39]
[27,"041301001","页岩标准砖 240×115×53","千块",3.369,638.83]
[28,"041504001","蒸压加气砼配块","",8.088,216.81]
[29,"041504004","蒸压加气砼砌块 590×200×200","",147.894,216.81]
[30,"050102005","周转圆木","",{"v":0.01,"d":"0.010"},794.34]
[31,"050301001","一等杉木板枋材(综合)","",0.717,1151.33]
[32,"050301003","一等杉木枋材","",0.101,1194.69]
[33,"050305003","1220×2440×15吸音板(竖条纹)","㎡",268.097,{"v":125,"d":"125.00"}]
[34,"050306001","周转板枋材","",{"v":0.24,"d":"0.240"},920.35]
[35,"050306002","周转枋材","",0.673,920.35]
[36,"050306003","周转板材","",0.175,992.92]
[37,"050501001","胶合板 3mm","㎡",{"v":2.38,"d":"2.380"},11.19]
[38,"050501004","15厚阻燃夹板","㎡",343.687,{"v":38,"d":"38.00"}]
[]
["主要材料及价格表"]
["工程名称:广西中医药大学教师教学发展中心装修工程",{"$nulls":3},"第2页  共3页"]
["序号","材料编码","项目名称及规格、型号等特殊要求","单位","数量","单价（元）"]
[39,"050501008","15厚阻燃板","㎡",512.401,{"v":38,"d":"38.00"}]
[40,"050501008","9厚阻燃板","㎡",140.186,{"v":29,"d":"29.00"}]
[41,"050501008","9厚阻燃夹板","㎡",67.589,{"v":29,"d":"29.00"}]
[42,"050701002","600×2400×9聚酯纤维吸音板(横竖向留V型缝)","㎡",41.003,{"v":45,"d":"45.00"}]
[43,"053501001","竹木纤维集成墙板","㎡",140.186,{"v":59,"d":"59.00"}]
[44,"062102003","12厚钢化玻璃背蓝漆","㎡",89.027,{"v":150,"d":"150.00"}]
[45,"070103003","100X100釉面砖(","㎡",31.312,{"v":42,"d":"42.00"}]
[46,"070103003","400×800深灰色仿石材瓷砖","㎡",40.736,{"v":120,"d":"120.00"}]
[47,"070501006","水磨石地面砖 600*600","㎡",74.548,{"v":73,"d":"73.00"}]
[48,"070501008","水磨石地面砖 1200*600","㎡",588.744,{"v":83,"d":"83.00"}]
[49,"071302001","浅木纹复合木地板1200×150","㎡",133.372,{"v":143,"d":"143.00"}]
[50,"072901007","仿地毯块状地胶2.0厚","㎡",533.113,{"v":110,"d":"110.00"}]
[51,"080101002","25厚西班牙米黄大理石","㎡",47.726,{"v":265,"d":"265.00"}]
[52,"080301001","30厚灰麻花岗岩饰面(荔枝面)","㎡",14.402,{"v":120,"d":"120.00"}]
[53,"080301001","30厚灰麻花岗岩饰面台阶","㎡",{"v":36.15,"d":"36.150"},111.66]
[54,"080301001","900X600X25灰麻烧花岗岩","㎡",114.934,{"v":120,"d":"120.00"}]
[55,"080301002","25厚黑金砂花岗岩","㎡",24.327,{"v":250,"d":"250.00"}]
[56,"080301002","25厚西班牙米黄大理石","㎡",127.449,{"v":265,"d":"265.00"}]
[57,"080301002","麻灰烧毛石","㎡",125.756,{"v":120,"d":"120.00"}]
[58,"090101001","9.5厚纸面石膏板","㎡",1846.521,9.58]
[59,"090505008","1.0厚黑钛不锈钢","㎡",3.157,{"v":175,"d":"175.00"}]
[60,"090505009","1.0厚304#拉丝不锈钢","㎡",{"v":19.29,"d":"19.290"},{"v":205,"d":"205.00"}]
[61,"090505009","1.0厚黑钛不锈钢板","㎡",{"v":0.74,"d":"0.740"},{"v":175,"d":"175.00"}]
[62,"091301001","4厚铝塑板1220X2440X4","㎡",278.246,{"v":60,"d":"60.00"}]
[63,"091501002","埃特板 12mm","㎡",{"v":3.36,"d":"3.360"},{"v":50,"d":"50.00"}]
[64,"110910001","80系列深灰色铝合金平开窗Low-E中空玻璃（5+9A+5）","㎡",3.588,463.13]
[65,"110911001","80系列深灰色铝合金固定窗Low-E中空玻璃（5+9A+5）","㎡",14.189,434.13]
[66,"120104001","80*15实木线条","m",14.879,{"v":2.3,"d":"2.30"}]
[67,"120112001","实木半圆线120×15","m",12.422,{"v":2.8,"d":"2.80"}]
[68,"120112001","实木半圆线60×15","m",{"v":15.54,"d":"15.540"},{"v":1.8,"d":"1.80"}]
[69,"120301001","1.0厚冲压黑钛不锈钢踢脚线","㎡",23.338,{"v":175,"d":"175.00"}]
[70,"120305002","1.0厚冲压黑钛不锈钢收边，宽20mm","m",63.294,{"v":25,"d":"25.00"}]
[71,"120305002","成品黑色铝合金工字收口条","m",25.709,{"v":8,"d":"8.00"}]
[72,"120310002","不锈钢压条 15×6.5mm","m",90.222,10.65]
[73,"123904001","5厚亚克力字120*120mm","个",{"v":8.08,"d":"8.080"},{"v":15,"d":"15.00"}]
[74,"123904001","5厚亚克力字60*40mm","个",{"v":31.31,"d":"31.310"},{"v":6,"d":"6.00"}]
[75,"130102001","调和漆(综合)","kg",{"v":0.33,"d":"0.330"},10.62]
[76,"130301001","乳胶漆","kg",702.626,14.16]
[]
["主要材料及价格表"]
["工程名称:广西中医药大学教师教学发展中心装修工程",{"$nulls":3},"第3页  共3页"]
["序号","材料编码","项目名称及规格、型号等特殊要求","单位","数量","单价（元）"]
[77,"130312001","双飞粉","kg",3124.963,0.22]
[78,"130507002","红丹防锈漆","kg",94.006,9.73]
[79,"133508002","嵌缝膏","kg",0.498,6.19]
[80,"143520001","隔离剂","kg",10.638,1.33]
[81,"143901001","乙炔气","",1.066,6.64]
[82,"143906001","氧气","",{"v":19.1,"d":"19.100"},3.98]
[83,"144101005","建筑胶","kg",1989.334,1.06]
[84,"144108001","乳白胶","kg",135.332,4.87]
[85,"144114001","密封胶","kg",122.429,10.62]
[86,"144115001","万能胶","kg",13.973,10.62]
[87,"150502001","矿棉板","㎡",30.492,{"v":31.6,"d":"31.60"}]
[88,"151901031","硅藻泥","kg",538.832,{"v":15,"d":"15.00"}]
[89,"341101001","水","",195.576,3.34]
[90,"350103001","胶合板模板 1830×915×18","㎡",14.992,28.32]
[91,"350302001","回转扣件","个",3.429,5.75]
[92,"350302002","对接扣件","个",4.439,5.31]
[93,"350302003","直角扣件","个",42.086,6.02]
[94,"350303001","脚手架焊接钢管 Φ48.3×3.6","t",0.291,3938.05]
[95,"350307002","竹脚手板","㎡",53.655,18.58]
[96,"043103003","碎石 GD20  商品普通砼  C20","",1.583,389.32]
[97,"043104001","碎石 GD40  商品普通砼  C10","",153.874,368.93]
[98,"043104003","碎石 GD40  商品普通砼  C20","",0.508,389.32]
[99,"043104003","碎石 GD40  商品普通砼  C20","",8.212,389.32]
[100,"Z130105001","酚醛调和漆（各色）","kg",5.809,{"v":15,"d":"15.00"}]
[101,"Z130507003","酚醛防锈漆 （各种颜色）","kg",6.584,{"v":15,"d":"15.00"}]
[102,"140301004","国V汽油 92#","kg",{"v":77.75,"d":"77.750"},{"v":7.9,"d":"7.90"}]
[103,"140304001","轻柴油 0#","kg",148.254,6.58]
[104,"341103001","电","kW.h",6123.117,0.59]
[105,"C1403001","轻柴油0#","kg",93.316,6.58]
[106,"R0800001","机械台班工日","工日",4.022,{"v":75,"d":"75.00"}]

{"sheet":"表-09_工程量清单综合单价分析表(主材)","index":11,"n_rows":955,"n_cols":13,"rows_kept":955,"merged":[[0,0,0,12],[1,0,1,8],[1,9,1,12],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,5],[2,6,2,12],[3,6,4,6],[3,7,3,8],[3,9,4,9],[3,10,4,10],[3,11,4,11],[3,12,4,12],[30,0,30,12],[31,0,31,8],[31,9,31,12],[32,0,34,0],[32,1,34,1],[32,2,34,2],[32,3,34,3],[32,4,34,4],[32,5,34,5],[32,6,32,12],[33,6,34,6],[33,7,33,8],[33,9,34,9],[33,10,34,10],[33,11,34,11],[33,12,34,12],[59,0,59,12],[60,0,60,8],[60,9,60,12],[61,0,63,0],[61,1,63,1],[61,2,63,2],[61,3,63,3],[61,4,63,4],[61,5,63,5],[61,6,61,12],[62,6,63,6],[62,7,62,8],[62,9,63,9],[62,10,63,10],[62,11,63,11],[62,12,63,12],[89,0,89,12],[90,0,90,8],[90,9,90,12],[91,0,93,0],[91,1,93,1],[91,2,93,2],[91,3,93,3],[91,4,93,4],[91,5,93,5],[91,6,91,12],[92,6,93,6],[92,7,92,8],[92,9,93,9],[92,10,93,10],[92,11,93,11],[92,12,93,12],[117,0,117,12],[118,0,118,8],[118,9,118,12],[119,0,121,0],[119,1,121,1],[119,2,121,2],[119,3,121,3],[119,4,121,4],[119,5,121,5],[119,6,119,12],[120,6,121,6],[120,7,120,8],[120,9,121,9],[120,10,121,10],[120,11,121,11],[120,12,121,12],[144,0,144,12],[145,0,145,8],[145,9,145,12],[146,0,148,0],[146,1,148,1],[146,2,148,2],[146,3,148,3],[146,4,148,4],[146,5,148,5],[146,6,146,12],[147,6,148,6],[147,7,147,8],[147,9,148,9],[147,10,148,10],[147,11,148,11],[147,12,148,12],[171,0,171,12],[172,0,172,8],[172,9,172,12],[173,0,175,0],[173,1,175,1],[173,2,175,2],[173,3,175,3],[173,4,175,4],[173,5,175,5],[173,6,173,12],[174,6,175,6],[174,7,174,8],[174,9,175,9],[174,10,175,10],[174,11,175,11],[174,12,175,12],[200,0,200,12],[201,0,201,8],[201,9,201,12],[202,0,204,0],[202,1,204,1],[202,2,204,2],[202,3,204,3],[202,4,204,4],[202,5,204,5],[202,6,202,12],[203,6,204,6],[203,7,203,8],[203,9,204,9],[203,10,204,10],[203,11,204,11],[203,12,204,12],[228,0,228,12],[229,0,229,8],[229,9,229,12],[230,0,232,0],[230,1,232,1],[230,2,232,2],[230,3,232,3],[230,4,232,4],[230,5,232,5],[230,6,230,12],[231,6,232,6],[231,7,231,8],[231,9,232,9],[231,10,232,10],[231,11,232,11],[231,12,232,12],[255,0,255,12],[256,0,256,8],[256,9,256,12],[257,0,259,0],[257,1,259,1],[257,2,259,2],[257,3,259,3],[257,4,259,4],[257,5,259,5],[257,6,257,12],[258,6,259,6],[258,7,258,8],[258,9,259,9],[258,10,259,10],[258,11,259,11],[258,12,259,12],[285,0,285,12],[286,0,286,8],[286,9,286,12],[287,0,289,0],[287,1,289,1],[287,2,289,2],[287,3,289,3],[287,4,289,4],[287,5,289,5],[287,6,287,12],[288,6,289,6],[288,7,288,8],[288,9,289,9],[288,10,289,10],[288,11,289,11],[288,12,289,12],[313,0,313,12],[314,0,314,8],[314,9,314,12],[315,0,317,0],[315,1,317,1],[315,2,317,2],[315,3,317,3],[315,4,317,4],[315,5,317,5],[315,6,315,12],[316,6,317,6],[316,7,316,8],[316,9,317,9],[316,10,317,10],[316,11,317,11],[316,12,317,12],[342,0,342,12],[343,0,343,8],[343,9,343,12],[344,0,346,0],[344,1,346,1],[344,2,346,2],[344,3,346,3],[344,4,346,4],[344,5,346,5],[344,6,344,12],[345,6,346,6],[345,7,345,8],[345,9,346,9],[345,10,346,10],[345,11,346,11],[345,12,346,12],[373,0,373,12],[374,0,374,8],[374,9,374,12],[375,0,377,0],[375,1,377,1],[375,2,377,2],[375,3,377,3],[375,4,377,4],[375,5,377,5],[375,6,375,12],[376,6,377,6],[376,7,376,8],[376,9,377,9],[376,10,377,10],[376,11,377,11],[376,12,377,12],[400,0,400,12],[401,0,401,8],[401,9,401,12],[402,0,404,0],[402,1,404,1],[402,2,404,2],[402,3,404,3],[402,4,404,4],[402,5,404,5],[402,6,402,12],[403,6,404,6],[403,7,403,8],[403,9,404,9],[403,10,404,10],[403,11,404,11],[403,12,404,12],[428,0,428,12],[429,0,429,8],[429,9,429,12],[430,0,432,0],[430,1,432,1],[430,2,432,2],[430,3,432,3],[430,4,432,4],[430,5,432,5],[430,6,430,12],[431,6,432,6],[431,7,431,8],[431,9,432,9],[431,10,432,10],[431,11,432,11],[431,12,432,12],[459,0,459,12],[460,0,460,8],[460,9,460,12],[461,0,463,0],[461,1,463,1],[461,2,463,2],[461,3,463,3],[461,4,463,4],[461,5,463,5],[461,6,461,12],[462,6,463,6],[462,7,462,8],[462,9,463,9],[462,10,463,10],[462,11,463,11],[462,12,463,12],[490,0,490,12],[491,0,491,8],[491,9,491,12],[492,0,494,0],[492,1,494,1],[492,2,494,2],[492,3,494,3],[492,4,494,4],[492,5,494,5],[492,6,492,12],[493,6,494,6],[493,7,493,8],[493,9,494,9],[493,10,494,10],[493,11,494,11],[493,12,494,12],[521,0,521,12],[522,0,522,8],[522,9,522,12],[523,0,525,0],[523,1,525,1],[523,2,525,2],[523,3,525,3],[523,4,525,4],[523,5,525,5],[523,6,523,12],[524,6,525,6],[524,7,524,8],[524,9,525,9],[524,10,525,10],[524,11,525,11],[524,12,525,12],[550,0,550,12],[551,0,551,8],[551,9,551,12],[552,0,554,0],[552,1,554,1],[552,2,554,2],[552,3,554,3],[552,4,554,4],[552,5,554,5],[552,6,552,12],[553,6,554,6],[553,7,553,8],[553,9,554,9],[553,10,554,10],[553,11,554,11],[553,12,554,12],[578,0,578,12],[579,0,579,8],[579,9,579,12],[580,0,582,0],[580,1,582,1],[580,2,582,2],[580,3,582,3],[580,4,582,4],[580,5,582,5],[580,6,580,12],[581,6,582,6],[581,7,581,8],[581,9,582,9],[581,10,582,10],[581,11,582,11],[581,12,582,12],[603,0,603,12],[604,0,604,8],[604,9,604,12],[605,0,607,0],[605,1,607,1],[605,2,607,2],[605,3,607,3],[605,4,607,4],[605,5,607,5],[605,6,605,12],[606,6,607,6],[606,7,606,8],[606,9,607,9],[606,10,607,10],[606,11,607,11],[606,12,607,12],[631,0,631,12],[632,0,632,8],[632,9,632,12],[633,0,635,0],[633,1,635,1],[633,2,635,2],[633,3,635,3],[633,4,635,4],[633,5,635,5],[633,6,633,12],[634,6,635,6],[634,7,634,8],[634,9,635,9],[634,10,635,10],[634,11,635,11],[634,12,635,12],[659,0,659,12],[660,0,660,8],[660,9,660,12],[661,0,663,0],[661,1,663,1],[661,2,663,2],[661,3,663,3],[661,4,663,4],[661,5,663,5],[661,6,661,12],[662,6,663,6],[662,7,662,8],[662,9,663,9],[662,10,663,10],[662,11,663,11],[662,12,663,12],[686,0,686,12],[687,0,687,8],[687,9,687,12],[688,0,690,0],[688,1,690,1],[688,2,690,2],[688,3,690,3],[688,4,690,4],[688,5,690,5],[688,6,688,12],[689,6,690,6],[689,7,689,8],[689,9,690,9],[689,10,690,10],[689,11,690,11],[689,12,690,12],[716,0,716,12],[717,0,717,8],[717,9,717,12],[718,0,720,0],[718,1,720,1],[718,2,720,2],[718,3,720,3],[718,4,720,4],[718,5,720,5],[718,6,718,12],[719,6,720,6],[719,7,719,8],[719,9,720,9],[719,10,720,10],[719,11,720,11],[719,12,720,12],[745,0,745,12],[746,0,746,8],[746,9,746,12],[747,0,749,0],[747,1,749,1],[747,2,749,2],[747,3,749,3],[747,4,749,4],[747,5,749,5],[747,6,747,12],[748,6,749,6],[748,7,748,8],[748,9,749,9],[748,10,749,10],[748,11,749,11],[748,12,749,12],[774,0,774,12],[775,0,775,8],[775,9,775,12],[776,0,778,0],[776,1,778,1],[776,2,778,2],[776,3,778,3],[776,4,778,4],[776,5,778,5],[776,6,776,12],[777,6,778,6],[777,7,777,8],[777,9,778,9],[777,10,778,10],[777,11,778,11],[777,12,778,12],[805,0,805,12],[806,0,806,8],[806,9,806,12],[807,0,809,0],[807,1,809,1],[807,2,809,2],[807,3,809,3],[807,4,809,4],[807,5,809,5],[807,6,807,12],[808,6,809,6],[808,7,808,8],[808,9,809,9],[808,10,809,10],[808,11,809,11],[808,12,809,12],[836,0,836,12],[837,0,837,8],[837,9,837,12],[838,0,840,0],[838,1,840,1],[838,2,840,2],[838,3,840,3],[838,4,840,4],[838,5,840,5],[838,6,838,12],[839,6,840,6],[839,7,839,8],[839,9,840,9],[839,10,840,10],[839,11,840,11],[839,12,840,12],[867,0,867,12],[868,0,868,8],[868,9,868,12],[869,0,871,0],[869,1,871,1],[869,2,871,2],[869,3,871,3],[869,4,871,4],[869,5,871,5],[869,6,869,12],[870,6,871,6],[870,7,870,8],[870,9,871,9],[870,10,871,10],[870,11,871,11],[870,12,871,12],[896,0,896,12],[897,0,897,8],[897,9,897,12],[898,0,900,0],[898,1,900,1],[898,2,900,2],[898,3,900,3],[898,4,900,4],[898,5,900,5],[898,6,898,12],[899,6,900,6],[899,7,899,8],[899,9,900,9],[899,10,900,10],[899,11,900,11],[899,12,900,12],[925,0,925,12],[926,0,926,8],[926,9,926,12],[927,0,929,0],[927,1,929,1],[927,2,929,2],[927,3,929,3],[927,4,929,4],[927,5,929,5],[927,6,927,12],[928,6,929,6],[928,7,928,8],[928,9,929,9],[928,10,929,10],[928,11,929,11],[928,12,929,12]],"flags":["formulas_cached_only"]}
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第1页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,null,"广西中医药大学教师教学发展中心装修工程-拆除"]
[null,null,"分部分项工程"]
[null,null,"G.1 人工拆除工程"]
["1","011601001001","砖砌体拆除","","40.68",42.26,{"v":38.4,"d":"38.40"},{"$nulls":3},{"v":2.9,"d":"2.90"},0.96]
[null,null,"拆除方式:人工"]
[null,null,"砌体名称:砌块墙"]
[null,"07010034","拆除砌体 砌块墙","10","4.068",422.63,{"v":384,"d":"384.00"},{"$nulls":3},29.03,{"v":9.6,"d":"9.60"}]
["2","010103002001","余土弃置","","40.68",28.22,9.79,null,null,15.85,1.94,0.64]
[null,null,"废弃料品种:拆除的废弃材料"]
[null,null,"运距:起步第1km"]
[null,null,"含装车、洒水、加盖费"]
[null,"07040005","加盖自卸垃圾车运渣土 人工装渣土1km以内","100","0.4068",2822.63,{"v":979.2,"d":"979.20"},null,null,1585.42,193.89,64.12]
["3","桂010103003001","土方运输每增(减)1km","","366.12",2.22,{"$nulls":3},2.02,0.15,0.05]
[null,null,"废弃料品种:拆除的废弃材料"]
[null,null,"含装车、洒水、加盖费"]
[null,null,"工程量暂按增运9km计算，最终按实际结算"]
[null,"07040008","加盖自卸垃圾车运渣土 每增加1km","100","3.6612",222.86,{"$nulls":3},202.49,15.31,5.06]
["4","010103002002","弃土场消纳费","","40.68",{"v":8,"d":"8.00"},null,{"v":8,"d":"8.00"}]
[null,null,"废弃料品种:拆除的废弃材料"]
[null,"B-换","弃土场消纳费","","40.68",{"v":8,"d":"8.00"},null,{"v":8,"d":"8.00"}]
[null,null,"单价措施项目"]
[]
[null,null,"广西中医药大学教师教学发展中心装修工程-装饰装修"]
[null,null,"分部分项工程"]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第2页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,null,"A.1 土（石）方工程"]
["5","010103001001","回填方","","258.52",20.77,16.29,null,null,2.27,1.76,0.45]
[null,null,"室内房心回填，高度20cm"]
[null,"A1-82","人工回填土 夯填","100","2.5852",2077.43,1628.64,null,null,227.04,176.29,45.46]
["6","010103002003","校内取土","","258.52",8.87,0.37,null,null,7.56,0.75,0.19]
[null,null,"运距:1km以内"]
[null,"A1-165","液压挖掘机挖土 斗容量1.8 自卸汽车运土(运距1km以内) 10t","1000","0.25852",8885.88,{"v":374.4,"d":"374.40"},null,null,7562.96,754.05,194.47]
[null,null,"A.3 砌筑工程"]
["7","010402001001","砌块墙","","165.06",408.08,110.56,248.42,null,2.17,37.39,9.54]
[null,null,"砖品种、规格、强度等级:蒸压加气砼砌块"]
[null,null,"墙体类型:直形"]
[null,null,"墙体厚度:200mm"]
[null,null,"砂浆种类、强度等级:混合砂浆M5.0"]
[null,"A3-56","蒸压加气混凝土砌块墙 墙体厚度 20cm{水泥石灰砂浆中砂M5}","10","16.506",4080.75,1105.57,2484.19,null,{"v":21.7,"d":"21.70"},373.92,95.37]
[null,null,"A.4 混凝土及钢筋混凝土工程"]
["8","010502002001","构造柱","","4.11",531.67,{"v":94.7,"d":"94.70"},395.76,null,1.26,31.83,8.12]
[null,null,"混凝土种类:非泵送商品砼"]
[null,null,"混凝土强度等级:C20"]
[null,"A4-20换","混凝土柱 构造柱{换:碎石 GD40  商品普通砼  C20}","10","0.411",5316.58,946.96,3957.57,null,12.59,318.28,81.18]
["9","010503004001","圈梁","","3.62",{"v":520.8,"d":"520.80"},85.29,{"v":398.9,"d":"398.90"},null,0.78,28.55,7.28]
[null,null,"混凝土种类:非泵送商品砼"]
[null,null,"混凝土强度等级:C20"]
[null,"A4-24换","混凝土 圈梁{换:碎石 GD40  商品普通砼  C20}","10","0.362",5207.94,852.85,3988.98,null,7.82,285.48,72.81]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第3页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
["10","010503005001","过梁","","0.12",542.74,{"v":96.7,"d":"96.70"},403.98,null,1.27,{"v":32.5,"d":"32.50"},8.29]
[null,null,"混凝土种类:非泵送商品砼"]
[null,null,"混凝土强度等级:C20"]
[null,"A4-25换","混凝土 过梁{换:碎石 GD40  商品普通砼  C20}","10","0.012",5427.25,966.97,4039.76,null,12.69,324.95,82.88]
["11","010507005001","扶手、压顶","","0.50",590.98,124.93,414.04,null,null,41.44,10.57]
[null,null,"混凝土种类:非泵送商品砼"]
[null,null,"混凝土强度等级:C20"]
[null,"A4-53","混凝土 压顶、扶手{碎石 GD40  商品普通砼  C20}","10","0.050",5909.85,1249.33,4140.43,null,null,{"v":414.4,"d":"414.40"},105.69]
["12","010515001001","现浇构件钢筋","t","0.667",6810.07,709.14,5786.63,null,13.48,239.69,61.13]
[null,null,"钢筋种类、规格:圆钢 φ10以内"]
[null,null,"品牌相当于或优于“柳钢”"]
[null,"A4-236","现浇构件圆钢筋制安 φ10以内","t","0.667",6810.07,709.14,5786.63,null,13.48,239.69,61.13]
["13","010515001002","现浇构件钢筋","t","0.375",7095.68,599.47,6121.48,null,88.38,228.16,58.19]
[null,null,"钢筋种类、规格:圆钢 φ10以上"]
[null,null,"品牌相当于或优于“柳钢”"]
[null,"A4-237","现浇构件圆钢筋制安 φ10以上","t","0.375",7095.68,599.47,6121.48,null,88.38,228.16,58.19]
["14","010515001003","现浇构件钢筋","t","0.034",7116.24,878.83,5847.81,null,16.76,297.07,75.77]
[null,null,"钢筋种类、规格:螺纹钢 10以内"]
[null,null,"品牌相当于或优于“柳钢”"]
[null,"A4-240","现浇构件螺纹钢制安 10以内","t","0.034",7116.24,878.83,5847.81,null,16.76,297.07,75.77]
["15","桂010515011001","砌体加固筋","t","0.617",7562.96,1241.92,5786.58,null,12.32,416.03,106.11]
[null,null,"钢筋种类、规格:圆钢 φ10以内"]
[null,null,"品牌相当于或优于“柳钢”"]
[null,"A4-317","砖砌体加固钢筋 绑扎","t","0.617",7562.96,1241.92,5786.58,null,12.32,416.03,106.11]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第4页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,null,"A.9 楼地面工程"]
["16","010404001001","垫层","","152.35",458.29,58.55,374.29,null,0.76,19.67,5.02]
[null,null,"夯实地面用C10混凝土垫高300mm,至±0.000"]
[null,null,"混凝土种类:非泵送商品砼"]
[null,null,"混凝土强度等级:C10"]
[null,"A4-3换","混凝土垫层{换:碎石 GD40  商品普通砼  C10}","10","15.235",4582.81,585.47,3742.89,null,7.57,196.71,50.17]
["17","011102003001","水磨石地砖地面","㎡","566.10",153.82,{"v":38.7,"d":"38.70"},98.89,null,2.18,11.16,2.89]
[null,null,"素水泥结合层一道"]
[null,null,"30厚M10干硬性水泥砂浆结合层"]
[null,null,"表面撒水泥粉"]
[null,null,"面贴地砖1200×600,水泥擦缝(密缝拼接)"]
[null,"A9-85换","陶瓷地砖楼地面 每块周长(3200mm以上)  水泥砂浆 密缝{换:水泥砂浆中砂M10}","100㎡","5.6610",15380.31,3869.58,9888.76,null,217.61,{"v":1115.8,"d":"1115.80"},288.56]
["18","011102003002","水磨石地砖地面","㎡","72.73",125.71,26.34,87.39,null,2.18,7.79,2.01]
[null,null,"素水泥结合层一道"]
[null,null,"30厚M10干硬性水泥砂浆结合层"]
[null,null,"表面撒水泥粉"]
[null,null,"面贴地砖600×600,水泥擦缝(密缝拼接)"]
[null,"A9-83换","陶瓷地砖楼地面 每块周长(2400mm以内)  水泥砂浆 密缝{换:水泥砂浆中砂M10}","100㎡","0.7273",12570.77,2634.06,8739.26,null,217.61,778.51,201.33]
["19","011102003003","灰麻烧毛石地面","㎡","112.68",175.66,{"v":27.3,"d":"27.30"},{"v":135,"d":"135.00"},null,2.96,8.26,2.14]
[null,null,"水泥浆一道(内掺建筑胶)"]
[null,null,"30厚M10干硬性水泥砂浆结合层"]
[null,null,"表面撒水泥粉"]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第5页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,null,"900×600×25灰麻烧毛石铺实拍平(踏步边缘开防滑槽),水泥浆擦缝"]
[null,"A9-48换","花岗岩楼地面 不拼花 水泥砂浆{换:水泥砂浆中砂M10}","100㎡","1.1268",17565.99,2730.16,13500.18,null,{"v":295.9,"d":"295.90"},826.11,213.64]
["20","011103001001","仿地毯块状地胶地面","㎡","522.66",190.39,38.77,136.73,null,1.17,{"v":10.9,"d":"10.90"},2.82]
[null,null,"水泥浆一道(内掺建筑胶)"]
[null,null,"30厚M10干硬性水泥砂浆结合层"]
[null,null,"水泥自流平界面剂"]
[null,null,"自流平找平层"]
[null,null,"2.0厚PVC方块地胶(胶粘剂粘贴)"]
[null,"A9-1换","水泥砂浆找平层 混凝土或硬基层上 20mm[实际30]{换:水泥砂浆中砂M10 换:水泥砂浆中砂M10}","100㎡","5.2266",2432.37,884.01,1168.79,null,56.43,256.74,{"v":66.4,"d":"66.40"}]
[null,"A9-9","普通水泥自流平","100㎡","5.2266",1956.88,693.58,973.73,null,38.15,199.76,51.66]
[null,"A9-119换","PVC塑胶地面","100㎡","5.2266",14649.98,2299.44,11530.25,null,22.48,633.88,163.93]
["21","011104002001","浅木纹复合木地板","㎡","114.55",197.76,24.44,164.16,null,0.56,6.83,1.77]
[null,null,"30厚M10干硬性水泥砂浆结合层"]
[null,null,"泡沫塑料衬垫"]
[null,null,"安装浅木纹复合木地板1200×150×12"]
[null,null,"阳角收口采用木地板同款同色成品铝合金收边条"]
[null,null,"品牌相当于或优于“富林”"]
[null,"A9-1换","水泥砂浆找平层 混凝土或硬基层上 20mm[实际30]{换:水泥砂浆中砂M10 换:水泥砂浆中砂M10}","100㎡","1.1455",2432.37,884.01,1168.79,null,56.43,256.74,{"v":66.4,"d":"66.40"}]
[null,"A9-148换","长条复合 木地板 铺在 水泥地 面上 面上","100㎡","1.1455",17343.48,1559.84,15247.68,null,null,425.84,110.12]
["22","011104002002","浅木纹复合木地板（台阶）","㎡","12.47",242.19,24.44,208.59,null,0.56,6.83,1.77]
[null,null,"30厚M10干硬性水泥砂浆结合层"]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第6页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,null,"泡沫塑料衬垫"]
[null,null,"安装浅木纹复合木地板1200×150×12"]
[null,null,"阳角收口采用木地板同款同色成品铝合金收边条"]
[null,null,"按展开面积计算"]
[null,null,"品牌相当于或优于“富林”"]
[null,"A9-1换","水泥砂浆找平层 混凝土或硬基层上 20mm[实际30]{换:水泥砂浆中砂M10 换:水泥砂浆中砂M10}","100㎡","0.1247",2432.37,884.01,1168.79,null,56.43,256.74,{"v":66.4,"d":"66.40"}]
[null,"A9-148换","长条复合 木地板 铺在 水泥地 面上 面上","100㎡","0.1247",17343.48,1559.84,15247.68,null,null,425.84,110.12]
[null,"B-","铝合金收边条","m","27.70",{"v":20,"d":"20.00"},null,{"v":20,"d":"20.00"}]
["23","011107001001","石材台阶面","㎡","23.04",422.02,69.21,309.95,null,12.86,23.86,6.14]
[null,null,"台阶做法参见图集12J003 11B/B3"]
[null,null,"30厚灰麻花岗岩饰面台阶踏步(荔枝面)及踏步踢面"]
[null,"A3-89","灰土 垫层{灰土 3∶7}","10","0.778",3469.08,600.95,2604.79,null,9.29,202.42,51.63]
[null,"A4-58","混凝土 台阶{碎石 GD20  商品普通砼  C20}","10","0.156",4920.36,600.95,4040.48,null,{"v":20.3,"d":"20.30"},206.07,52.56]
[null,"A9-54换","花岗岩台阶 直形 水泥砂浆{素水泥浆}","100㎡","0.2304",27157.09,4484.77,19463.83,null,1241.08,1563.16,404.25]
["24","010401012001","入口砌砖花池","","6.11",1277.01,306.91,820.07,null,21.63,102.22,26.18]
[null,null,"150mm厚3:7灰土垫层"]
[null,null,"非粘土烧结砖砌筑"]
[null,null,"顶部及侧面30厚灰麻花岗岩饰面(荔枝面)（1:3水泥砂浆粘结层）"]
[null,null,"60厚C20混凝土压顶Φ6钢筋@200双向"]
[null,"A3-89","灰土 垫层{灰土 3∶7}","10","0.130",3469.08,600.95,2604.79,null,9.29,202.42,51.63]
[null,"A3-37","零星砌体 标准砖240×115×53{水泥石灰砂浆中砂M5}","10","0.611",7033.66,{"v":1897.7,"d":"1897.70"},4292.15,null,37.98,642.07,163.76]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第7页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,"A9-56换","花岗岩零星项目 水泥砂浆{素水泥浆}","100㎡","0.1224",23325.44,4869.15,15601.71,null,879.38,1569.35,405.85]
[null,"A4-53换","混凝土 压顶、扶手{换:碎石 GD40  商品普通砼  C20}","10","0.024",{"v":6302.3,"d":"6302.30"},1526.42,4140.43,null,null,506.31,129.14]
[null,"A4-236","现浇构件圆钢筋制安 φ10以内","t","0.007",6810.07,709.14,5786.63,null,13.48,239.69,61.13]
[null,null,"A.10 墙、柱面工程"]
["25","011201001001","墙面一般抹灰","㎡","606.16",18.61,8.68,6.59,null,0.27,2.44,0.63]
[null,null,"13厚1:0.3:3水泥石膏砂浆打底扫毛"]
[null,"A10-37换","内墙、内墙裙 水泥砂浆找平层 砖墙 15mm{换:混合砂浆 1∶0.5∶3}","100㎡","6.0616",2054.28,930.07,762.36,null,31.47,{"v":262.5,"d":"262.50"},67.88]
[null,"A10-55换","抹灰层每增减1mm 混合砂浆{换:混合砂浆 1∶0.5∶3}","100㎡","6.0616",-191.96,-61.78,-103.12,null,-4.34,-18.05,-4.67]
["26","011201001002","墙面一般抹灰","㎡","293.34",19.49,{"v":9.3,"d":"9.30"},6.57,null,0.31,2.63,0.68]
[null,null,"15厚M10水泥砂浆找平"]
[null,"A10-37换","内墙、内墙裙 水泥砂浆找平层 砖墙 15mm{换:水泥砂浆中砂M10}","100㎡","2.9334",1948.65,930.07,656.73,null,31.47,{"v":262.5,"d":"262.50"},67.88]
["27","011207001001","条形吸音板墙面","㎡","262.84",265.29,{"v":30.5,"d":"30.50"},221.51,null,2.08,{"v":8.9,"d":"8.90"},{"v":2.3,"d":"2.30"}]
[null,null,"U50墙面轻钢龙骨@400mm"]
[null,null,"15厚阻燃板基层"]
[null,null,"1220×2440×15吸音板(竖条纹)"]
[null,"A10-236","轻钢龙骨 中距(mm) 竖603横1500","100㎡","2.6284",6965.58,1223.51,5293.27,null,21.14,339.79,87.87]
[null,"A10-242换","板基层 15厚阻燃板","100㎡","2.6284",5015.66,611.75,4084.68,null,81.15,189.16,48.92]
[null,"A10-265换","硬木板条墙面、墙裙","100㎡","2.6284",14547.87,1214.93,12773.13,null,105.96,{"v":360.6,"d":"360.60"},93.25]
["28","011502002001","木质装饰线","m","14.17",7.67,3.54,2.91,null,null,0.97,0.25]
[null,null,"吸音板墙面80×15实木线条"]
[null,"A14-58换","木质装饰线 150mm内","100m","0.1417",765.62,{"v":353.5,"d":"353.50"},290.65,null,null,96.51,24.96]
["29","011502002002","木质装饰线","m","11.83",6.58,2.52,3.19,null,null,0.69,0.18]
[null,null,"15宽实木半圆线120×15"]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第8页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,"A14-55换","木质装饰线 宽度 50mm内","100m","0.1183",{"v":658.3,"d":"658.30"},252.25,319.38,null,null,68.86,17.81]
["30","011502002003","木质装饰线","m","14.80",5.53,2.52,2.14,null,null,0.69,0.18]
[null,null,"15宽实木半圆线60×15"]
[null,"A14-55换","木质装饰线 宽度 50mm内","100m","0.1480",{"v":553.3,"d":"553.30"},252.25,214.38,null,null,68.86,17.81]
["31","011105006001","冲压黑钛不锈钢踢脚线","㎡","22.88",277.45,40.78,221.57,null,0.81,11.35,2.94]
[null,null,"15厚阻燃板基层"]
[null,null,"冲压1.0厚冲压黑钛不锈钢踢脚线用万能胶拍合安装"]
[null,null,"80mm高"]
[null,null,"品牌相当于或优于“海利”"]
[null,"A10-242换","板基层 15厚阻燃板","100㎡","0.2288",5015.66,611.75,4084.68,null,81.15,189.16,48.92]
[null,"A9-162换","踢脚线 金属板","100㎡","0.2288",22729.75,3466.32,{"v":18072.4,"d":"18072.40"},null,null,946.31,244.72]
["32","011105006002","不锈钢墙面","㎡","16.68",338.43,39.77,283.91,null,0.81,11.08,2.86]
[null,null,"15厚阻燃板基层"]
[null,null,"1.0厚304#拉丝不锈钢饰面"]
[null,null,"品牌相当于或优于“海利”"]
[null,"A10-242换","板基层 15厚阻燃板","100㎡","0.1668",5015.66,611.75,4084.68,null,81.15,189.16,48.92]
[null,"A10-249换","不锈钢面板 墙面","100㎡","0.1668",28827.67,3365.08,24306.35,null,null,918.67,237.57]
["33","桂011204005001","内墙面干挂石材","㎡","123.29",280.63,82.14,161.52,null,6.51,{"v":24.2,"d":"24.20"},6.26]
[null,null,"5#镀锌角钢横向龙骨间距600×900mm(油丹红底漆两遍,防锈漆两遍)（另列清单）"]
[null,null,"不锈钢干挂件(油丹红底漆两遍,防锈漆两遍)"]
[null,null,"麻灰烧毛石600×900×30干挂(竖向密缝拼接、横向留自然缝)"]
[null,"A10-132换","干挂花岗岩 墙面 密缝","100㎡","1.2329",28063.96,8214.49,16152.05,null,651.17,2420.33,625.92]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第9页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
["34","桂011204005002","外墙面干挂石材","㎡","23.85",413.23,82.14,294.12,null,6.51,{"v":24.2,"d":"24.20"},6.26]
[null,null,"5#镀锌角钢横向龙骨间距600×900mm(油丹红底漆两遍,防锈漆两遍)（另列清单）"]
[null,null,"不锈钢干挂件(油丹红底漆两遍,防锈漆两遍)"]
[null,null,"25厚黑金砂花岗岩饰面干挂(竖向密缝拼接、横向留自然缝)"]
[null,"A10-132换","干挂花岗岩 墙面 密缝","100㎡","0.2385",41323.96,8214.49,29412.05,null,651.17,2420.33,625.92]
["35","桂011204007001","块料墙面","㎡","33.76",105.04,38.61,50.73,null,1.81,11.04,2.85]
[null,null,"15厚1:3水泥砂浆找平"]
[null,null,"3-4厚1:1水泥砂浆加水重20%专用瓷砖胶镶贴"]
[null,null,"面贴100×100釉面砖(工字拼贴),白水泥浆擦缝"]
[null,null,"品牌相当于或优于“东鹏”"]
[null,"A10-160换","面砖(周长600mm以内) 水泥砂浆粘贴 墙面、墙裙 缝宽5mm内{素水泥浆}","100㎡","0.3376",10504.25,{"v":3861,"d":"3861.00"},5073.21,null,181.15,1103.51,285.38]
["36","011502001001","金属装饰线","m","61.45",28.47,1.71,26.12,null,0.04,0.48,0.12]
[null,null,"1.0厚冲压黑钛不锈钢收边，宽20mm，反边27.5mm"]
[null,null,"品牌相当于或优于“海利”"]
[null,"A14-45换","金属装饰 压条","100m","0.6145",2846.08,170.74,2611.69,null,3.71,47.62,12.32]
["37","011502001002","金属装饰线","m","24.96",10.96,1.71,8.61,null,0.04,0.48,0.12]
[null,null,"成品黑色铝合金工字收口条，高度同硬包厚度，约18mm高"]
[null,null,"品牌相当于或优于“海利”"]
[null,"A14-45换","金属装饰 压条","100m","0.2496",1095.08,170.74,860.69,null,3.71,47.62,12.32]
["38","011502001003","金属装饰线","m","32.80",22.03,4.78,15.61,null,null,{"v":1.3,"d":"1.30"},0.34]
[null,null,"1.0厚黑钛不锈钢包边，展开宽度85mm"]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第10页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,null,"品牌相当于或优于“海利”"]
[null,"A14-50换","金属装饰线 镜面不锈钢 60mm外","100m","0.3280",2202.72,477.91,{"v":1560.6,"d":"1560.60"},null,null,130.47,33.74]
["39","011502001004","金属装饰线","m","7.38",15.67,4.78,9.25,null,null,{"v":1.3,"d":"1.30"},0.34]
[null,null,"部位：出入口铝塑板檐口处"]
[null,null,"1.0厚黑钛不锈钢，宽度50mm"]
[null,null,"品牌相当于或优于“海利”"]
[null,"A14-49换","金属装饰线 镜面不锈钢 60mm内","100m","0.0738",1566.87,477.91,924.75,null,null,130.47,33.74]
["40","011207001002","墙面装饰板","㎡","72.38",349.34,36.31,299.18,null,1.02,10.19,2.64]
[null,null,"U50轻钢龙骨"]
[null,null,"15厚阻燃夹板基层"]
[null,null,"面层：12厚钢化玻璃背蓝漆"]
[null,null,"品牌相当于或优于“南玻”"]
[null,"A10-236","轻钢龙骨 中距(mm) 竖603横1500","100㎡","0.7238",6965.58,1223.51,5293.27,null,21.14,339.79,87.87]
[null,"A10-242换","板基层 15厚阻燃板","100㎡","0.7238",5015.66,611.75,4084.68,null,81.15,189.16,48.92]
[null,"A10-245换","镜面玻璃 墙面 在胶合板上粘贴","100㎡","0.7238",22952.78,1795.79,20539.96,null,null,490.25,126.78]
["41","011207001003","墙面装饰板","㎡","64.37",368.16,52.35,296.45,null,1.02,14.57,3.77]
[null,null,"U50轻钢龙骨"]
[null,null,"15厚阻燃夹板基层"]
[null,null,"9厚阻燃夹板基层浅咖啡色仿布纹硬包"]
[null,"A10-236","轻钢龙骨 中距(mm) 竖603横1500","100㎡","0.6437",6965.58,1223.51,5293.27,null,21.14,339.79,87.87]
[null,"A10-242换","板基层 15厚阻燃板","100㎡","0.6437",5015.66,611.75,4084.68,null,81.15,189.16,48.92]
[null,"A10-261换","人造革软包带衬板 墙、柱面","100㎡","0.6437",24834.79,{"v":3399.4,"d":"3399.40"},20267.35,null,null,928.04,{"v":240,"d":"240.00"}]
["42","桂011204005003","石材墙面","㎡","124.95",428.53,82.14,309.42,null,6.51,{"v":24.2,"d":"24.20"},6.26]
[null,null,"5#镀锌角钢横向龙骨间距600×900mm(油丹红底漆两遍,防锈漆两遍)（另列清单）"]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第11页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,null,"不锈钢干挂件(油丹红底漆两遍,防锈漆两遍)"]
[null,null,"25厚西班牙米黄大理石饰面干挂"]
[null,null,"部位：外墙及部分柱面、主入口"]
[null,"A10-132换","干挂花岗岩 墙面 密缝","100㎡","1.2495",42853.96,8214.49,30942.05,null,651.17,2420.33,625.92]
["43","桂011204007002","块料墙面","㎡","43.92",177.39,38.61,123.08,null,1.81,11.04,2.85]
[null,null,"15厚1:3水泥砂浆找平"]
[null,null,"3-4厚1:1水泥砂浆加水重20%专用瓷砖胶镶贴"]
[null,null,"面贴400×800深灰色仿石材瓷砖,白水泥浆擦缝"]
[null,null,"部位：外墙面"]
[null,null,"品牌相当于或优于“东鹏”"]
[null,"A10-160换","面砖(周长600mm以内) 水泥砂浆粘贴 墙面、墙裙 缝宽5mm内{素水泥浆}","100㎡","0.4392",17738.75,{"v":3861,"d":"3861.00"},12307.71,null,181.15,1103.51,285.38]
["44","桂011204007003","块料墙面","㎡","46.79",357.71,50.54,282.71,null,5.28,15.24,3.94]
[null,null,"25厚西班牙米黄大理石（密拼）"]
[null,null,"20厚1:3水泥砂浆结合层"]
[null,null,"部位：外墙窗底部"]
[null,"A10-105换","粘贴大理石 水泥砂浆粘贴 砖墙面{素水泥浆}","100㎡","0.4679",35771.51,5053.62,28271.46,null,528.44,{"v":1523.9,"d":"1523.90"},394.09]
["45","011207001004","墙面装饰板","㎡","3.20",68.05,8.39,56.78,null,null,2.29,0.59]
[null,null,"20×20×2镀锌方通骨架@600(油丹红底漆两遍,防锈漆两遍)（另列清单）"]
[null,null,"12厚埃特板"]
[null,"A10-266换","埃特板墙面","100㎡","0.0320",{"v":6805.5,"d":"6805.50"},839.12,5678.06,null,null,229.08,59.24]
["46","011207001005","墙面装饰板","㎡","133.51",189.09,30.06,147.34,null,1.02,8.48,2.19]
[null,null,"配套金属轻钢龙骨架"]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第12页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,null,"9厚阻燃板基层"]
[null,null,"面封竹木纤维集成墙板(密缝拼接)，600宽×9厚"]
[null,null,"阳角采用配套25×25mmL型同款同色阳角线条"]
[null,null,"阴角采用配套27×16mm同款同色阴角线条"]
[null,"A10-236","轻钢龙骨 中距(mm) 竖603横1500","100㎡","1.3351",6965.58,1223.51,5293.27,null,21.14,339.79,87.87]
[null,"A10-242换","板基层 9厚阻燃板","100㎡","1.3351",4070.66,611.75,3139.68,null,81.15,189.16,48.92]
[null,"A10-267换","竹片内墙面","100㎡","1.3351",7873.89,1170.31,6301.47,null,null,319.49,82.62]
["47","011207001006","聚酯纤维吸音板","㎡","31.46",172.94,22.64,141.15,null,1.02,6.46,1.67]
[null,null,"U50墙面轻钢龙骨@400mm"]
[null,null,"15厚阻燃板基层"]
[null,null,"600×2400×9聚酯纤维吸音板(横竖向留V型缝)"]
[null,"A10-236","轻钢龙骨 中距(mm) 竖603横1500","100㎡","0.3146",6965.58,1223.51,5293.27,null,21.14,339.79,87.87]
[null,"A10-242换","板基层 15厚阻燃板","100㎡","0.3146",5015.66,611.75,4084.68,null,81.15,189.16,48.92]
[null,"A10-268换","纤维板","100㎡","0.3146",5313.33,{"v":429,"d":"429.00"},4736.92,null,null,117.12,30.29]
["48","011207001007","防潮纸面石膏板墙面","㎡","13.46",25.61,8.39,14.34,null,null,2.29,0.59]
[null,null,"40*20*2钢骨架@1000（另列清单）"]
[null,null,"9.5厚纸面石膏板"]
[null,null,"刮腻子油白色乳胶漆（另列清单）"]
[null,"A10-266换","石膏板墙面","100㎡","0.1346",{"v":2561.4,"d":"2561.40"},839.12,1433.96,null,null,229.08,59.24]
["49","011207001008","黑钛不锈钢墙面","㎡","0.64",322.55,42.06,264.53,null,1.12,11.79,3.05]
[null,null,"展示厅立面P-07/A"]
[null,null,"15厚阻燃板基层"]
[null,null,"1.0厚黑钛不锈钢板"]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第13页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,null,"定制亚克力字体（另列清单）"]
[null,null,"品牌相当于或优于“海利”"]
[null,"A10-242换","板基层 15厚阻燃板","100㎡","0.0088",5015.66,611.75,4084.68,null,81.15,189.16,48.92]
[null,"A10-249换","不锈钢面板 墙面","100㎡","0.0064",25358.17,3365.08,20836.85,null,null,918.67,237.57]
["50","011304001001","墙面灯槽","㎡","8.92",134.88,{"v":46.2,"d":"46.20"},72.73,null,0.05,12.63,3.27]
[null,null,"15厚阻燃夹板基层"]
[null,null,"9.5厚防潮纸面石膏板"]
[null,"A11-171换","悬挑式灯槽 直型 胶合板面","100㎡","0.0892",10925.68,3781.21,{"v":5838.6,"d":"5838.60"},null,4.95,1033.62,{"v":267.3,"d":"267.30"}]
[null,"A10-266换","石膏板墙面","100㎡","0.0892",{"v":2561.4,"d":"2561.40"},839.12,1433.96,null,null,229.08,59.24]
["51","011304001002","墙面灯槽","㎡","7.59",{"v":162.4,"d":"162.40"},{"v":42.1,"d":"42.10"},105.76,null,0.05,11.51,2.98]
[null,null,"15厚阻燃夹板基层"]
[null,null,"9厚竹木纤维集成墙板"]
[null,"A11-171换","悬挑式灯槽 直型 胶合板面","100㎡","0.0759",10925.68,3781.21,{"v":5838.6,"d":"5838.60"},null,4.95,1033.62,{"v":267.3,"d":"267.30"}]
[null,"A10-268换","纤维板","100㎡","0.0759",5313.33,{"v":429,"d":"429.00"},4736.92,null,null,117.12,30.29]
["52","011204004001","钢骨架","t","1.841",13042.52,2402.48,8582.28,null,917.14,906.25,234.37]
[null,null,"挂石板钢骨架"]
[null,null,"含油丹红底漆两遍,防锈漆两遍"]
[null,null,"品牌相当于或优于“柳钢”"]
[null,"A10-142","挂石板钢骨架 镀锌钢骨架","t","1.841",12406.63,2071.21,8391.48,null,917.14,815.82,210.98]
[null,"A13-140","红丹防锈漆 金属面 4遍","100㎡","0.6996",1673.35,871.73,{"v":502.1,"d":"502.10"},null,null,237.98,61.54]
["53","011204004002","钢骨架","t","3.212",13042.53,2402.48,8582.28,null,917.14,906.26,234.37]
[null,null,"挂装饰板钢骨架"]
[null,null,"含油丹红底漆两遍,防锈漆两遍"]
[null,null,"品牌相当于或优于“柳钢”"]
[null,"A10-142","挂石板钢骨架 镀锌钢骨架","t","3.212",12406.63,2071.21,8391.48,null,917.14,815.82,210.98]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第14页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,"A13-140","红丹防锈漆 金属面 4遍","100㎡","1.2206",1673.35,871.73,{"v":502.1,"d":"502.10"},null,null,237.98,61.54]
[null,null,"A.11 天棚工程"]
["54","011302001001","防潮纸面石膏板吊顶","㎡","825.59",105.51,36.16,56.63,null,0.22,9.93,2.57]
[null,null,"Φ8螺纹吊杆"]
[null,null,"U60轻钢龙骨标准骨架(上人型):主龙骨中距900-1000,C型次龙骨中距450,横撑龙骨中距900"]
[null,null,"双层9.5厚纸面石膏板(或双层9.5厚冲孔纸面石膏板),自攻螺钉拧紧,螺丝眼刷防锈漆,再用石膏腻子点补"]
[null,null,"刮腻子三遍油乳胶漆三遍（另列清单）"]
[null,"A11-39","装配式U型轻钢天棚龙骨(上人型) 面层规格(600×600mm) 以上 平面","100㎡","8.2559",5119.04,1465.46,3120.34,null,22.11,406.11,105.02]
[null,"A11-76换","天棚石膏板基层","100㎡","8.2559",2768.51,{"v":1158.3,"d":"1158.30"},1212.21,null,null,316.22,81.78]
[null,"A11-94换","天棚石膏板面层 安在U型轻钢龙骨上","100㎡","8.2559",2663.91,992.71,{"v":1330.1,"d":"1330.10"},null,null,271.01,70.09]
["55","011302001002","矿棉板吊顶","㎡","29.04",94.56,22.92,63.39,null,0.28,6.33,1.64]
[null,null,"φ8螺纹吊杆T型主骨中距600~1200mm,次骨间距@600mm"]
[null,null,"安装矿棉板1200×600×15"]
[null,null,"四周采用L型边龙骨收口"]
[null,"A11-53","装配式T型铝合金天棚龙骨(上人型) 面层规格(600×600mm)  平面","100㎡","0.2904",4938.87,1410.55,3006.31,null,27.79,392.67,101.55]
[null,"A11-91","天棚矿棉板面层 搁放在 龙骨上","100㎡","0.2904",4516.67,881.17,3332.73,null,null,240.56,62.21]
["56","011302001003","铝塑板天棚","㎡","242.29",161.45,30.99,119.81,null,null,8.46,2.19]
[null,null,"5#镀锌角钢架,@600mm（另列清单）"]
[null,null,"15厚阻燃夹板基层"]
[null,null,"面贴4厚铝塑板1220×2440×4"]
[null,null,"横向密缝拼接,竖向留5mm缝填黑色结构胶"]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第15页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,null,"清单工程量按铝塑板展开面积计算"]
[null,null,"品牌相当于或优于“奥斯特”"]
[null,"A11-75换","15厚阻燃夹板基层","100㎡","2.4229",5124.09,838.27,3997.79,null,null,228.85,59.18]
[null,"A10-257换","铝塑板墙面 胶合板基层上","100㎡","2.4229",11021.05,2260.83,{"v":7983.4,"d":"7983.40"},null,null,617.21,159.61]
["57","011302001004","防潮纸面石膏板窗帘盒","㎡","51.60",142.86,35.14,95.35,null,0.22,9.65,{"v":2.5,"d":"2.50"}]
[null,null,"Φ8螺纹吊杆"]
[null,null,"U60轻钢龙骨标准骨架"]
[null,null,"15厚阻燃夹板基层"]
[null,null,"9.5厚纸面石膏板(或双层9.5厚冲孔纸面石膏板),自攻螺钉拧紧,螺丝眼刷防锈漆,再用石膏腻子点补"]
[null,null,"刮腻子三遍油无机乳胶漆三遍（另列清单）"]
[null,"A11-40","装配式U型轻钢天棚龙骨(上人型) 面层规格(600×600mm) 以上 跌级","100㎡","0.5160",6499.06,{"v":1683.4,"d":"1683.40"},4207.54,null,22.11,{"v":465.6,"d":"465.60"},120.41]
[null,"A11-75换","15厚阻燃夹板基层","100㎡","0.5160",5124.09,838.27,3997.79,null,null,228.85,59.18]
[null,"A11-94换","天棚石膏板面层 安在U型轻钢龙骨上","100㎡","0.5160",2663.91,992.71,{"v":1330.1,"d":"1330.10"},null,null,271.01,70.09]
["58","011302001005","天棚灯槽","㎡","33.43",{"v":135.9,"d":"135.90"},47.74,71.69,null,0.05,13.05,3.37]
[null,null,"15厚阻燃夹板基层"]
[null,null,"9.5厚纸面石膏板(或双层9.5厚冲孔纸面石膏板),自攻螺钉拧紧,螺丝眼刷防锈漆,再用石膏腻子点补"]
[null,null,"刮腻子三遍油无机乳胶漆三遍（另列清单）"]
[null,"A11-171换","悬挑式灯槽 直型 胶合板面","100㎡","0.3343",10925.68,3781.21,{"v":5838.6,"d":"5838.60"},null,4.95,1033.62,{"v":267.3,"d":"267.30"}]
[null,"A11-94换","天棚石膏板面层 安在U型轻钢龙骨上","100㎡","0.3343",2663.91,992.71,{"v":1330.1,"d":"1330.10"},null,null,271.01,70.09]
["59","010606013001","∟40×40×4mm镀锌角钢间距1100mm","t","0.329",11751.18,2274.87,{"v":6580.1,"d":"6580.10"},null,1376.25,1211.08,308.88]
[null,null,"玻璃隔墙门连窗上部"]
[null,null,"品牌相当于或优于“柳钢”"]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第16页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,"A6-54","金属零星构件制作","t","0.329",10248.64,1474.59,6546.63,null,1139.27,867.02,221.13]
[null,"A6-100","金属零星构件 安装","t","0.329",1502.54,800.28,33.47,null,236.98,344.06,87.75]
[null,null,"A.12 门窗工程"]
["60","010807001001","80系列深灰色铝合金平开窗","㎡","3.84",486.35,34.04,439.92,null,0.52,9.43,2.44]
[null,null,"Low-E中空玻璃（5+9A+5）"]
[null,null,"洞口面积≤2㎡"]
[null,null,"含运输、安装、配件等全部内容"]
[null,null,"品牌相当于或优于“南南铝”"]
[null,"A12-117换","铝合金平开窗 不带亮","100㎡","0.0384",48635.49,3403.69,{"v":43992.4,"d":"43992.40"},null,52.02,943.41,243.97]
["61","010807001002","80系列深灰色铝合金固定窗","㎡","15.08",447.45,23.62,415.07,null,0.48,6.58,{"v":1.7,"d":"1.70"}]
[null,null,"Low-E中空玻璃（5+9A+5）"]
[null,null,"洞口面积＞2㎡"]
[null,null,"含运输、安装、配件等全部内容"]
[null,null,"品牌相当于或优于“南南铝”"]
[null,"A12-118换","铝合金固定窗(矩形)","100㎡","0.1508",44745.51,2362.07,41507.11,null,48.17,{"v":658,"d":"658.00"},170.16]
["62","桂010811002001","门窗周边塞缝","m","227.60",7.26,{"v":4.8,"d":"4.80"},0.81,null,null,1.31,0.34]
[null,null,"水泥砂浆1:2.5"]
[null,"A12-166","门窗周边塞缝 水泥砂浆1:2.5{水泥砂浆 1∶2.5}","100m","2.2760",726.15,480.48,80.58,null,null,131.17,33.92]
[null,null,"A.13 油漆、涂料、裱糊工程"]
["63","011406003001","墙面满刮腻子","㎡","468.02",{"v":16.1,"d":"16.10"},10.36,2.18,null,null,2.83,0.73]
[null,null,"刮腻子三遍"]
[null,"A13-204换","刮熟胶粉腻子 内墙面 两遍[实际3]","100㎡","4.6802",{"v":1610.8,"d":"1610.80"},1036.46,218.22,null,null,282.95,73.17]
["64","011406003002","天棚满刮腻子","㎡","910.62",17.83,11.65,2.18,null,null,3.18,0.82]
[null,null,"刮腻子三遍"]
[null,"A13-204换","刮熟胶粉腻子 内墙面 两遍[实际3]","100㎡","9.1062",1783.67,1165.11,218.22,null,null,318.08,82.26]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第17页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
["65","011406001001","米白色乳胶漆","㎡","1378.64",15.94,7.13,6.36,null,null,1.95,{"v":0.5,"d":"0.50"}]
[null,null,"封底涂料一道"]
[null,null,"乳液内墙涂料一道"]
[null,null,"乳胶涂料一道"]
[null,null,"品牌相当于或优于“多乐士”"]
[null,"A13-210换","乳胶漆 内墙、柱、天棚抹灰面 二遍[实际3]","100㎡","13.7864",1593.81,{"v":713,"d":"713.00"},635.82,null,null,194.65,50.34]
["66","011406001002","米白色硅藻泥","㎡","396.20",33.75,{"v":3.9,"d":"3.90"},28.22,null,0.22,1.12,0.29]
[null,null,"封底涂料一道"]
[null,null,"米白色硅藻泥涂料一道"]
[null,null,"米白色硅藻泥一道"]
[null,null,"品牌相当于或优于“五棵松”"]
[null,"A10-370","硅藻泥墙面（无图案不分色） 喷涂两遍成活 毛面","100㎡","3.9620",3375.18,389.95,2822.17,null,21.64,112.36,29.06]
["67","011406001003","抹灰面油漆","㎡","381.97",11.64,5.57,4.16,null,null,1.52,0.39]
[null,null,"原建筑天面喷黑漆"]
[null,null,"品牌相当于或优于“多乐士”"]
[null,"A13-210","乳胶漆 内墙、柱、天棚抹灰面 二遍","100㎡","3.8197",1164.63,556.84,416.46,null,null,152.02,39.31]
[null,null,"A.14 其他装饰工程"]
["68","01B001","0.8厚镀锌铁皮","㎡","130.10",50.62,7.71,{"v":39.7,"d":"39.70"},null,null,2.56,0.65]
[null,null,"部位：外墙面铝塑板檐口顶面"]
[null,"A7-37换","屋面铁皮","100㎡","1.3010",5062.09,771.38,3969.58,null,null,255.87,65.26]
["69","011508002001","定制不锈钢钛金发光字","个","8",114.49,53.28,42.23,null,{"v":0.5,"d":"0.50"},14.68,{"v":3.8,"d":"3.80"}]
[null,null,"规格：800×800mm"]
[null,"A14-220换","金属字 1.0以内 其他面","10个","0.8",1144.93,532.82,422.33,null,4.99,146.82,37.97]
["70","011508002002","定制不锈钢钛金发光字","个","32",53.74,25.85,18.85,null,0.12,7.09,1.83]
[null,null,"规格：300×200mm"]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第18页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,"A14-212换","金属字 0.2以内 其他面","10个","3.1",554.78,266.84,194.58,null,1.24,73.19,18.93]
["71","011508002003","5厚亚克力字","个","8",{"v":49.4,"d":"49.40"},25.05,15.74,null,null,6.84,1.77]
[null,null,"规格：120×120mm"]
[null,"A14-188换","泡沫塑料、有机玻璃字 0.2以内 其他面","10个","0.8",494.03,250.54,{"v":157.4,"d":"157.40"},null,null,{"v":68.4,"d":"68.40"},17.69]
["72","011508002004","5厚亚克力字","个","32",39.05,24.27,6.44,null,null,6.63,1.71]
[null,null,"规格：60×40mm"]
[null,"A14-188换","泡沫塑料、有机玻璃字 0.2以内 其他面","10个","3.1",403.13,250.54,{"v":66.5,"d":"66.50"},null,null,{"v":68.4,"d":"68.40"},17.69]
["73","010810005001","窗帘轨","m","33.30",21.66,{"v":3.4,"d":"3.40"},17.09,null,null,0.93,0.24]
[null,"A12-163换","明装式铝合金窗帘轨 单轨","100m","0.3330",2165.98,339.77,1709.46,null,null,92.76,23.99]
[null,null,"单价措施项目"]
[null,"011701","脚手架工程"]
["74","桂011701001001","扣件式钢管外脚手架 双排 10m以内","㎡","522.25",21.74,11.98,4.06,null,{"v":0.5,"d":"0.50"},4.14,1.06]
[null,"A15-5","扣件式钢管外脚手架 双排 10m以内","100㎡","5.2225",{"v":2174.5,"d":"2174.50"},{"v":1198.2,"d":"1198.20"},406.23,null,50.32,414.13,105.62]
["75","桂011701002001","扣件式钢管里脚手架 3.6m以上","㎡","770.49",8.34,4.68,1.38,null,0.23,1.63,0.42]
[null,"A15-2","扣件式钢管里脚手架 3.6m以上","100㎡","7.7049",834.83,468.31,138.47,null,23.36,163.09,{"v":41.6,"d":"41.60"}]
[null,"011702","混凝土模板及支架(撑)"]
["76","011702003001","构造柱 胶合板模板 木支撑[实际4.2]","㎡","49.50",55.51,28.89,14.23,null,0.25,9.67,2.47]
[null,"A17-58换","构造柱 胶合板模板 木支撑[实际4.2]","100㎡","0.4950",5550.31,2889.46,1422.64,null,24.94,966.71,246.56]
["77","011702008001","圈梁 直形 胶合板模板 木支撑","㎡","36.63",39.87,22.05,8.27,null,0.26,{"v":7.4,"d":"7.40"},1.89]
[null,"A17-72","圈梁 直形 胶合板模板 木支撑","100㎡","0.3663",3987.67,2205.22,827.29,null,26.21,740.17,188.78]
["78","011702009001","过梁 胶合板模板 木支撑","㎡","2.16",69.15,35.58,17.91,null,{"v":0.6,"d":"0.60"},{"v":12,"d":"12.00"},3.06]
[null,"A17-76","过梁 胶合板模板 木支撑","100㎡","0.0216",6915.27,3558.28,1791.28,null,59.59,1200.05,306.07]
["79","011702027001","台阶 木模板木支撑","㎡","4.16",35.52,19.12,{"v":7.9,"d":"7.90"},null,0.38,6.47,1.65]
[null,"A17-122","台阶 木模板木支撑","10㎡投影面积","0.416",355.19,191.18,79.04,null,{"v":3.8,"d":"3.80"},64.67,{"v":16.5,"d":"16.50"}]
["80","011702028001","扶手、压顶 木模板木支撑","m","48.50",{"v":33.4,"d":"33.40"},{"v":17.7,"d":"17.70"},7.78,null,0.39,{"v":6,"d":"6.00"},1.53]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第19页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,"A17-118","压顶、扶手 木模板木支撑","100延长米","0.485",{"v":3339.9,"d":"3339.90"},1770.25,777.84,null,38.73,600.04,153.04]
[null,"011705","大型机械设备进出场及安拆"]
["81","011705001001","履带式挖掘机 1以外 场外运输费","台次","1",1001.21,{"v":74.1,"d":"74.10"},156.24,null,680.68,{"v":71.7,"d":"71.70"},18.49]
[null,"A20-21","履带式挖掘机 1以外 场外运输费","台次","1",1001.21,{"v":74.1,"d":"74.10"},156.24,null,680.68,{"v":71.7,"d":"71.70"},18.49]
[]
[]
[]
[]
[null,null,"广西中医药大学教师教学发展中心装修工程-安装"]
[null,null,"分部分项工程"]
[null,null,"B4 电气设备安装工程"]
["82","030404017001","ALzm配电箱","台","1",852.52,104.34,27.69,{"v":650,"d":"650.00"},16.09,37.07,17.33]
[null,null,"底边距地1.5m安装"]
[null,null,"品牌相当于或优于“正泰”"]
[null,null,"箱内元件：13个断路器,1个接触器，1个熔断器，1个时控开关"]
[null,"B4-0302换","成套配电箱安装 悬挂嵌入式(半周长m) 1","台","1",852.52,104.34,27.69,{"v":650,"d":"650.00"},16.09,37.07,17.33]
["83","030404017002","ALG 公共照明配电箱","台","1",916.72,86.95,{"v":25.9,"d":"25.90"},{"v":750,"d":"750.00"},10.05,29.86,13.96]
[null,null,"底边距地1.5m安装"]
[null,null,"品牌相当于或优于“正泰”"]
[null,null,"箱内元件：1个双电源自动转换开关，9个断路器，1个智能照明控制开关"]
[null,"B4-0301","成套配电箱安装 悬挂嵌入式(半周长m) 0.5","台","1",916.72,86.95,{"v":25.9,"d":"25.90"},{"v":750,"d":"750.00"},10.05,29.86,13.96]
["84","030404017003","AL1-4配电箱","台","7",416.72,86.95,{"v":25.9,"d":"25.90"},{"v":250,"d":"250.00"},10.05,29.86,13.96]
[null,null,"底边距地1.5m安装"]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第20页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,null,"品牌相当于或优于“正泰”"]
[null,null,"箱内元件：AL1、2-5个断路器,AL3-6个断路器，AL4-8个断路器"]
[null,"B4-0301","成套配电箱安装 悬挂嵌入式(半周长m) 0.5","台","7",416.72,86.95,{"v":25.9,"d":"25.90"},{"v":250,"d":"250.00"},10.05,29.86,13.96]
["85","030404017004","AL5配电箱","台","1",616.72,86.95,{"v":25.9,"d":"25.90"},{"v":450,"d":"450.00"},10.05,29.86,13.96]
[null,null,"底边距地1.5m安装"]
[null,null,"品牌相当于或优于“正泰”"]
[null,null,"箱内元件：15个断路器"]
[null,"B4-0301","成套配电箱安装 悬挂嵌入式(半周长m) 0.5","台","1",616.72,86.95,{"v":25.9,"d":"25.90"},{"v":450,"d":"450.00"},10.05,29.86,13.96]
["86","030404017005","AP-KT配电箱","台","1",316.72,86.95,{"v":25.9,"d":"25.90"},{"v":150,"d":"150.00"},10.05,29.86,13.96]
[null,null,"底边距地1.5m安装"]
[null,null,"品牌相当于或优于“正泰”"]
[null,"B4-0301","成套配电箱安装 悬挂嵌入式(半周长m) 0.5","台","1",316.72,86.95,{"v":25.9,"d":"25.90"},{"v":150,"d":"150.00"},10.05,29.86,13.96]
["87","030411002001","防火金属线槽（MR）:100×100","m","63.98",73.04,17.71,9.21,37.91,0.14,{"v":5.5,"d":"5.50"},2.57]
[null,null,"梁底下200mm安装敷设"]
[null,null,"品牌相当于或优于“南宁乔顿”"]
[null,"B4-0926换","金属线槽敷设 金属线槽(宽mm以下) 100","10m","6.398",730.32,177.13,92.09,379.05,1.41,54.95,25.69]
["88","030411001001","吊顶内敷设 扣压式(KBG)、紧定式(JDG)电气钢导管规格 40","m","7.31",21.28,8.19,4.72,4.45,0.15,2.57,{"v":1.2,"d":"1.20"}]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B4-1529换","吊顶内敷设 扣压式(KBG)、紧定式(JDG)电气钢导管规格 40","100m","0.0731",2127.49,818.78,472.36,444.96,14.84,256.59,119.96]
["89","030411001002","吊顶内敷设 扣压式(KBG)、紧定式(JDG)电气钢导管规格 32","m","80.74",19.68,7.42,5.66,3.11,{"v":0.1,"d":"0.10"},2.31,1.08]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B4-1528换","吊顶内敷设 扣压式(KBG)、紧定式(JDG)电气钢导管规格 32","100m","0.8074",1967.84,741.81,566.09,311.06,9.51,231.26,108.11]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第21页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
["90","030411001003","吊顶内敷设 扣压式(KBG)、紧定式(JDG)电气钢导管规格 25","m","26.22",18.34,6.75,5.52,2.88,{"v":0.1,"d":"0.10"},2.11,0.98]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B4-1527换","吊顶内敷设 扣压式(KBG)、紧定式(JDG)电气钢导管规格 25","100m","0.2622",1833.83,674.95,{"v":551.8,"d":"551.80"},{"v":288.4,"d":"288.40"},9.51,210.68,98.49]
["91","030411001004","砖、混凝土结构暗配 扣压式(KBG)、紧定式(JDG)电气钢导管规格 20","m","1291.58",11.61,5.33,1.82,2.05,null,1.64,0.77]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B4-1521换","砖、混凝土结构暗配 扣压式(KBG)、紧定式(JDG)电气钢导管规格 20","100m","12.9158",1161.06,533.05,182.26,204.97,null,164.07,76.71]
["92","030411004001","线槽内穿铜芯线WDZ-BYJ-0.45/0.75kV-6m㎡","m","803.27",5.89,0.88,0.02,4.59,null,0.27,0.13]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B4-1629换","线槽配线 动力线路 导线截面(m㎡以内) 6","100m单线","8.0327",588.63,87.72,2.29,{"v":459,"d":"459.00"},null,{"v":27,"d":"27.00"},12.62]
["93","030411004002","管道内穿铜芯线WDZ-BYJ-0.45/0.75kV-6m㎡","m","197.46",5.76,0.57,{"v":0.2,"d":"0.20"},4.73,null,0.18,0.08]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B4-1584换","管内穿线 动力线路 铜芯 导线截面(m㎡以内) 6","100m单线","1.9746",575.36,57.07,20.01,{"v":472.5,"d":"472.50"},null,17.57,8.21]
["94","030411004003","线槽内穿配铜芯线WDZ-BYJ-0.45/0.75kV-10m㎡","m","228.90",9.71,0.96,0.02,8.29,null,{"v":0.3,"d":"0.30"},0.14]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B4-1630换","线槽配线 动力线路 导线截面(m㎡以内) 10","100m单线","2.289",971.25,96.23,2.29,829.26,null,29.62,13.85]
["95","030411004004","管道内穿铜芯线WDZ-BYJ-0.45/0.75kV-10m㎡","m","134.71",9.76,0.68,0.23,8.54,null,0.21,{"v":0.1,"d":"0.10"}]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B4-1585换","管内穿线 动力线路 铜芯 导线截面(m㎡以内) 10","100m单线","1.3471",975.17,67.75,23.17,853.65,null,20.85,9.75]
["96","030411004005","管道内穿配铜芯线WDZ-BYJ-0.45/0.75kV-2.5m㎡","m","3890.82",2.53,{"v":0.5,"d":"0.50"},{"v":0.2,"d":"0.20"},1.61,null,0.15,0.07]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第22页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B4-1564换","管内穿线 照明线路 铜芯 导线截面(m㎡以内) 2.5","100m单线","38.9082",253.48,50.24,19.63,160.92,null,15.46,7.23]
["97","030411004006","线槽内穿配铜芯线WDZ-BYJ-0.45/0.75kV-2.5m㎡","m","101.06",2.69,0.72,0.04,1.61,null,0.22,{"v":0.1,"d":"0.10"}]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B4-1625换","线槽配线 照明线路 导线截面(m㎡以内) 2.5","100m单线","1.0106",269.51,72.01,4.06,160.92,null,22.16,10.36]
["98","030411004007","管道内穿配铜芯线WDZ-BYJ-0.45/0.75kV-4m㎡","m","1060.62",3.43,0.48,0.19,2.54,null,0.15,0.07]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B4-1565换","管内穿线 照明线路 铜芯 导线截面(m㎡以内) 4","100m单线","10.5331",344.71,47.86,19.27,255.96,null,14.73,6.89]
["99","030413002001","凿(压)槽及恢复","m","87.80",13.54,{"v":6.7,"d":"6.70"},3.47,null,0.24,2.13,{"v":1,"d":"1.00"}]
[null,"B4-2007","凿槽、刨沟  砖结构（公称管径32mm以内）","10m","8.780",73.73,{"v":43.8,"d":"43.80"},{"v":8.2,"d":"8.20"},null,1.34,13.89,{"v":6.5,"d":"6.50"}]
[null,"B4-2019","所凿沟槽恢复  沟槽尺寸（公称管径32mm以内）{水泥砂浆 1∶2.5}","10m","8.780",61.62,23.19,26.49,null,1.01,7.45,3.48]
["100","030404035001","墙面插座","套","55",27.43,10.33,2.41,10.02,null,3.18,1.49]
[null,null,"单、三相暗插座 单相暗插座10A 5孔"]
[null,null,"底边距地0.3m"]
[null,null,"品牌相当于或优于“西蒙”"]
[null,"B4-0436换","单、三相暗插座 单相暗插座10A 5孔","10套","5.5",274.24,103.32,24.09,100.16,null,{"v":31.8,"d":"31.80"},14.87]
["101","030404035002","安全型地面插座","套","21",192.85,10.33,2.41,175.44,null,3.18,1.49]
[null,null,"单、三相暗插座 单相暗插座10A 5孔"]
[null,null,"嵌地安装"]
[null,null,"品牌相当于或优于“西蒙”"]
[null,"B4-0436换","单、三相暗插座 单相暗插座10A 5孔","10套","2.1",1928.48,103.32,24.09,{"v":1754.4,"d":"1754.40"},null,{"v":31.8,"d":"31.80"},14.87]
["102","030404035003","安全型插座","套","9",27.43,10.33,2.41,10.02,null,3.18,1.49]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第23页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,null,"单、三相暗插座 单相暗插座10A 5孔"]
[null,null,"投影机用，壁装"]
[null,null,"品牌相当于或优于“西蒙”"]
[null,"B4-0436换","单、三相暗插座 单相暗插座10A 5孔","10套","0.9",274.24,103.32,24.09,100.16,null,{"v":31.8,"d":"31.80"},14.87]
["103","030404035004","安全型插座","套","3",27.43,10.33,2.41,10.02,null,3.18,1.49]
[null,null,"单、三相暗插座 单相暗插座10A 5孔"]
[null,null,"电视机用，底边距地1.2m"]
[null,null,"品牌相当于或优于“西蒙”"]
[null,"B4-0436换","单、三相暗插座 单相暗插座10A 5孔","10套","0.3",274.24,103.32,24.09,100.16,null,{"v":31.8,"d":"31.80"},14.87]
["104","030404035005","防水插座","套","2",32.71,10.33,2.41,{"v":15.3,"d":"15.30"},null,3.18,1.49]
[null,null,"单、三相暗插座 单相暗插座10A 5孔"]
[null,null,"配防溅盒，底边距地1.2m"]
[null,null,"品牌相当于或优于“西蒙”"]
[null,"B4-0436换","单、三相暗插座 单相暗插座10A 5孔","10套","0.2",327.08,103.32,24.09,{"v":153,"d":"153.00"},null,{"v":31.8,"d":"31.80"},14.87]
["105","030404034001","开关、按钮、插座安装 开关及按钮 跷板暗开关(单控) 单联","套","1",20.08,8.67,1.72,5.77,null,2.67,1.25]
[null,null,"品牌相当于或优于“西蒙”"]
[null,"B4-0412换","开关、按钮、插座安装 开关及按钮 跷板暗开关(单控) 单联","10套","0.1",200.75,86.69,17.18,57.73,null,26.68,12.47]
["106","030404034002","开关、按钮、插座安装 开关及按钮 跷板暗开关(单控) 双联","套","10",23.27,8.93,1.72,8.58,null,2.75,1.29]
[null,null,"品牌相当于或优于“西蒙”"]
[null,"B4-0413换","开关、按钮、插座安装 开关及按钮 跷板暗开关(单控) 双联","10套","1",232.71,89.34,17.23,85.78,null,{"v":27.5,"d":"27.50"},12.86]
["107","030404034003","开关、按钮、插座安装 开关及按钮 跷板暗开关(单控) 三联","套","12",32.42,{"v":9.2,"d":"9.20"},1.73,17.34,null,2.83,1.32]
[null,null,"品牌相当于或优于“西蒙”"]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第24页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,"B4-0414换","开关、按钮、插座安装 开关及按钮 跷板暗开关(单控) 三联","10套","1.2",324.22,91.98,17.29,{"v":173.4,"d":"173.40"},null,28.31,13.24]
["108","030404034004","开关、按钮、插座安装 开关及按钮 跷板暗开关(双控) 单联","套","2",19.83,8.87,1.72,5.23,null,2.73,1.28]
[null,null,"品牌相当于或优于“西蒙”"]
[null,"B4-0418换","开关、按钮、插座安装 开关及按钮 跷板暗开关(双控) 单联","10套","0.2",198.29,88.69,17.21,52.33,null,{"v":27.3,"d":"27.30"},12.76]
["109","030404034005","开关、按钮、插座安装 开关及按钮 跷板暗开关(双控) 双联","套","4",28.97,9.13,1.73,13.99,null,2.81,1.31]
[null,null,"品牌相当于或优于“西蒙”"]
[null,"B4-0419换","开关、按钮、插座安装 开关及按钮 跷板暗开关(双控) 双联","10套","0.4",289.81,91.34,17.28,139.94,null,28.11,13.14]
["110","030412001001","6寸LED筒灯","套","27",64.41,16.05,2.73,38.38,null,4.94,2.31]
[null,null,"15W   ~220V  1300lm  4000K"]
[null,null,"嵌入安装"]
[null,null,"品牌相当于或优于“三极雄光”"]
[null,"B4-1853换","装饰灯具安装 点光源艺术装饰灯具 筒灯 嵌入式 灯具直径(150)","10套","2.7",643.99,160.45,27.26,{"v":383.8,"d":"383.80"},null,49.39,23.09]
["111","030412001002","8寸LED筒灯","套","10",66.43,16.05,2.73,{"v":40.4,"d":"40.40"},null,4.94,2.31]
[null,null,"18W   ~220V  1500lm  4000K"]
[null,null,"嵌入安装"]
[null,null,"品牌相当于或优于“三极雄光”"]
[null,"B4-1853换","装饰灯具安装 点光源艺术装饰灯具 筒灯 嵌入式 灯具直径(150)","10套","1",664.19,160.45,27.26,{"v":404,"d":"404.00"},null,49.39,23.09]
["112","030412001003","LED可调式天花小射灯","套","66",60.94,8.49,{"v":2.8,"d":"2.80"},45.45,0.25,2.69,1.26]
[null,null,"15W   ～220V  1062lm  4000K（24°）"]
[null,null,"嵌入安装"]
[null,null,"品牌相当于或优于“三极雄光”"]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第25页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,"B4-1856换","装饰灯具安装 点光源艺术装饰灯具 射灯 吸顶式","10套","6.6",609.37,{"v":84.9,"d":"84.90"},28.04,{"v":454.5,"d":"454.50"},2.47,26.89,12.57]
["113","030412001004","双头LED格栅射灯","套","6",101.34,8.49,{"v":2.8,"d":"2.80"},85.85,0.25,2.69,1.26]
[null,null,"2*15W   ～220V  2150lm  （24°）"]
[null,null,"嵌入安装"]
[null,null,"品牌相当于或优于“三极雄光”"]
[null,"B4-1856换","装饰灯具安装 点光源艺术装饰灯具 射灯 吸顶式","10套","0.6",1013.37,{"v":84.9,"d":"84.90"},28.04,{"v":858.5,"d":"858.50"},2.47,26.89,12.57]
["114","030412001005","成品工艺吊灯","套","10",151.55,14.32,{"v":4.3,"d":"4.30"},126.25,0.15,4.45,2.08]
[null,null,"  15W  ~220V 1300lm(吊线式)"]
[null,null,"底距地3.2/2.2m"]
[null,null,"品牌相当于或优于“三极雄光”"]
[null,"B4-1749换","其他普通灯具 吊链灯","10套","1",1515.46,143.18,42.95,{"v":1262.5,"d":"1262.50"},1.48,44.53,20.82]
["115","030412001006","LED平面灯盘(300x1200mm)","套","63",191.95,14.32,{"v":4.3,"d":"4.30"},166.65,0.15,4.45,2.08]
[null,null,"2x16W  ~220V 2250lm(吊线式)"]
[null,null,"品牌相当于或优于“三极雄光”"]
[null,"B4-1749换","其他普通灯具 吊链灯","10套","6.3",1919.46,143.18,42.95,{"v":1666.5,"d":"1666.50"},1.48,44.53,20.82]
["116","030412001007","LED平面灯盘(300x1200mm)","套","32",192.54,19.07,4.92,159.58,0.25,5.94,2.78]
[null,null,"35W  ~220V 2000lm"]
[null,null,"嵌入安装"]
[null,null,"品牌相当于或优于“三极雄光”"]
[null,"B4-1746换","普通灯具安装 吸顶灯具 灯罩周长 2000mm以上","10套","3.2",1925.36,190.65,49.21,{"v":1595.8,"d":"1595.80"},2.47,59.44,27.79]
["117","030412001008","LED平面灯盘(300x300mm)","套","6",108.71,19.07,4.92,75.75,0.25,5.94,2.78]
[null,null,"12W  ~220V  800lm"]
[null,null,"嵌入安装",null,"5"]
[null,null,"品牌相当于或优于“三极雄光”"]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第26页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,"B4-1746换","普通灯具安装 吸顶灯具 灯罩周长 2000mm以上","10套","0.6",1087.06,190.65,49.21,{"v":757.5,"d":"757.50"},2.47,59.44,27.79]
["118","030412001009","LED高压软灯带","m","271.54",29.49,{"v":2,"d":"2.00"},11.73,14.14,0.49,0.77,0.36]
[null,null,"PAK544217 AC200V/灯盒内安装8W/m/4000K/发光角度140°/光通量(450lm/m)"]
[null,null,"壁装"]
[null,null,"品牌相当于或优于“三极雄光”"]
[null,"B4-1990换","其他照明灯具安装  LED光灯带","10m","27.154",294.86,19.97,{"v":117.3,"d":"117.30"},{"v":141.4,"d":"141.40"},4.94,7.67,3.58]
[null,null,"单价措施项目"]
[]
[null,null,"广西中医药大学教师教学发展中心装修工程-消防"]
[null,null,"分部分项工程"]
[null,null,"消火栓系统"]
["119","030901002001","消火栓热镀锌钢管及管件安装","m","86.31",{"v":138.5,"d":"138.50"},25.78,1.41,99.18,0.33,8.04,3.76]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：沟槽连接"]
[null,null,"规格型号：DN100"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B9-0038换","消火栓热镀锌钢管(沟槽连接)安装 DN100","10m","8.631",1385.02,257.83,14.14,991.81,3.29,80.37,37.58]
["120","031002001001","管道支架制作安装","kg","96.93",{"v":20.6,"d":"20.60"},5.79,3.79,7.26,0.89,1.96,0.91]
[null,null,"支架的材质不详，暂按40*4热镀锌角钢计，结算按实调整"]
[null,null,"面刷防锈漆二道，红色调和漆二道"]
[null,"B4-2001换","一般铁构件制作安装","100kg","0.9693",{"v":1846.2,"d":"1846.20"},498.53,373.38,{"v":678.4,"d":"678.40"},{"v":48.7,"d":"48.70"},168.44,78.75]
[null,"B11-0119","金属结构刷油 一般钢结构 防锈漆 第一遍","100kg","0.9693",55.62,19.84,2.21,{"v":13.8,"d":"13.80"},10.01,6.81,2.95]
[null,"B11-0120","金属结构刷油 一般钢结构 防锈漆 第二遍","100kg","0.9693",53.29,19.84,1.98,{"v":11.7,"d":"11.70"},10.01,6.81,2.95]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第27页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,"B11-0126","金属结构刷油 一般钢结构 调和漆 第一遍","100kg","0.9693",53.17,20.49,0.71,{"v":12,"d":"12.00"},10.01,6.95,3.01]
[null,"B11-0127","金属结构刷油 一般钢结构 调和漆 第二遍","100kg","0.9693",50.74,19.84,0.63,{"v":10.5,"d":"10.50"},10.01,6.81,2.95]
["121","030901010001","室内消火栓","套","6",859.59,148.14,5.71,{"v":638,"d":"638.00"},0.57,45.77,{"v":21.4,"d":"21.40"}]
[null,null,"安装方式：半暗装型"]
[null,null,"规格型号：箱子尺寸1000X700X240mm"]
[null,null,"配直流水枪1支,规格为:65mmX19mm;消防龙带:材质用衬胶。口径65mm 长度及条数:25m长配1条。"]
[null,"B9-0832换","甲型单栓带消防软管卷盘消火栓 箱子尺寸1000X700X240mm","套","6",859.59,148.14,5.71,{"v":638,"d":"638.00"},0.57,45.77,{"v":21.4,"d":"21.40"}]
[null,null,"自动喷淋系统"]
["122","030901001001","喷淋热镀锌钢管及管件安装","m","31.00",219.21,31.35,4.24,169.08,0.26,9.73,4.55]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：沟槽连接"]
[null,null,"规格型号：DN150"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B9-0040换","喷淋热镀锌钢管(沟槽连接)安装 DN150","10m","3.100",2191.99,313.48,{"v":42.4,"d":"42.40"},1690.75,2.59,97.29,45.48]
["123","030901001002","喷淋热镀锌钢管及管件安装","m","4.25",202.52,28.57,3.26,157.56,0.16,8.84,4.13]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：沟槽连接"]
[null,null,"规格型号：DN125"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B9-0039换","喷淋热镀锌钢管(沟槽连接)安装 DN125","10m","0.425",{"v":2025.1,"d":"2025.10"},285.66,32.57,1575.56,1.57,88.41,41.33]
["124","030901001003","喷淋热镀锌钢管及管件安装","m","8.59",{"v":138.5,"d":"138.50"},25.78,1.41,99.18,0.33,8.04,3.76]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：沟槽连接"]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第28页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,null,"规格型号：DN100"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B9-0038换","喷淋热镀锌钢管(沟槽连接)安装 DN100","10m","0.859",1385.02,257.83,14.14,991.81,3.29,80.37,37.58]
["125","030901001004","喷淋热镀锌钢管及管件安装","m","35.26",108.08,23.56,1.17,72.02,0.47,{"v":7.4,"d":"7.40"},3.46]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：沟槽连接"]
[null,null,"规格型号：DN80"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B9-0037换","喷淋热镀锌钢管(沟槽连接)安装 DN80","10m","3.526",1080.82,235.62,11.73,720.17,4.73,73.98,34.59]
["126","030901001005","喷淋热镀锌钢管及管件安装","m","10.65",108.08,23.56,1.17,72.02,0.47,{"v":7.4,"d":"7.40"},3.46]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：沟槽连接"]
[null,null,"规格型号：DN65"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B9-0037换","喷淋热镀锌钢管(沟槽连接)安装 DN80","10m","1.065",1080.82,235.62,11.73,720.17,4.73,73.98,34.59]
["127","030901001006","喷淋热镀锌钢管及管件安装","m","27.81",73.08,{"v":23.1,"d":"23.10"},2.58,35.99,0.67,7.32,3.42]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：螺纹连接"]
[null,null,"规格型号：DN50"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B9-0005换","喷淋热镀锌钢管(螺纹连接)安装 DN50","10m","2.781",730.69,230.97,25.75,359.93,6.69,73.15,{"v":34.2,"d":"34.20"}]
["128","030901001007","喷淋热镀锌钢管及管件安装","m","36.33",62.97,22.26,1.98,27.83,0.58,7.03,3.29]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：螺纹连接"]
[null,null,"规格型号：DN40"]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第29页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B9-0004换","喷淋热镀锌钢管(螺纹连接)安装 DN40","10m","3.633",629.71,{"v":222.6,"d":"222.60"},{"v":19.8,"d":"19.80"},278.29,5.84,70.31,32.87]
["129","030901001008","喷淋热镀锌钢管及管件安装","m","201.75",54.15,19.85,1.86,22.72,0.52,6.27,2.93]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：螺纹连接"]
[null,null,"规格型号：DN32"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B9-0003换","喷淋热镀锌钢管(螺纹连接)安装 DN32","10m","20.175",541.49,198.51,18.59,227.23,5.16,62.69,29.31]
["130","030901001009","喷淋热镀锌钢管及管件安装","m","190.09",50.05,19.21,1.58,20.04,0.37,6.03,2.82]
[null,null,"公称压力1.6MPa"]
[null,null,"连接方式：螺纹连接"]
[null,null,"规格型号：DN25"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B9-0002换","喷淋热镀锌钢管(螺纹连接)安装 DN25","10m","19.009",500.39,192.07,15.82,{"v":200.4,"d":"200.40"},3.68,60.25,28.17]
["131","031002001002","管道支架","kg","290.33",{"v":20.6,"d":"20.60"},5.79,3.79,7.26,0.89,1.96,0.91]
[null,null,"管道支架制作安装"]
[null,null,"面刷防锈漆二道，红色调和漆二道"]
[null,"B4-2001换","一般铁构件制作安装","100kg","2.9033",{"v":1846.2,"d":"1846.20"},498.53,373.38,{"v":678.4,"d":"678.40"},{"v":48.7,"d":"48.70"},168.44,78.75]
[null,"B11-0119","金属结构刷油 一般钢结构 防锈漆 第一遍","100kg","2.9033",55.62,19.84,2.21,{"v":13.8,"d":"13.80"},10.01,6.81,2.95]
[null,"B11-0120","金属结构刷油 一般钢结构 防锈漆 第二遍","100kg","2.9033",53.29,19.84,1.98,{"v":11.7,"d":"11.70"},10.01,6.81,2.95]
[null,"B11-0126","金属结构刷油 一般钢结构 调和漆 第一遍","100kg","2.9033",53.17,20.49,0.71,{"v":12,"d":"12.00"},10.01,6.95,3.01]
[null,"B11-0127","金属结构刷油 一般钢结构 调和漆 第二遍","100kg","2.9033",50.74,19.84,0.63,{"v":10.5,"d":"10.50"},10.01,6.81,2.95]
["132","030901003001","玻璃球闭式喷头DN15,喷头动作温度68℃","个","159",30.23,{"v":12.5,"d":"12.50"},4.51,6.62,0.66,4.05,1.89]
[null,null,"安装方式  有吊顶"]
[null,"B9-0800换","闭式喷头安装 公称直径15mm以内 有吊顶","10个","15.9",302.17,124.96,45.05,66.16,6.58,40.49,18.93]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第30页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
["133","030901008001","末端试水阀","组","1",{"v":40.4,"d":"40.40"},7.73,3.93,25.25,null,2.38,1.11]
[null,null,"规格型号 DN25"]
[null,"B9-0315换","螺纹阀门安装 螺纹阀 公称直径(mm以内) 25","个","1",{"v":40.4,"d":"40.40"},7.73,3.93,25.25,null,2.38,1.11]
["134","030901008002","末端试水装置","组","1",296.23,97.26,61.15,{"v":90.9,"d":"90.90"},2.06,30.57,14.29]
[null,null,"规格型号 DN25"]
[null,"B9-0827换","末端试水装置安装 DN25","组","1",296.23,97.26,61.15,{"v":90.9,"d":"90.90"},2.06,30.57,14.29]
["135","030905002001","水灭火控制装置调试","点","1",139.62,78.31,{"v":2.6,"d":"2.60"},null,16.08,29.05,13.58]
[null,"B5-1391","水灭火控制装置调试 自动喷水灭火系统","点","1",139.62,78.31,{"v":2.6,"d":"2.60"},null,16.08,29.05,13.58]
[null,null,"火灾自动报警系统"]
["136","030904001001","编码型感烟探测器","个","32",262.66,38.93,3.36,{"v":202,"d":"202.00"},0.54,12.15,5.68]
[null,null,"安装方式 吸顶"]
[null,"B5-1308换","编码型感烟探测器","个","32",262.66,38.93,3.36,{"v":202,"d":"202.00"},0.54,12.15,5.68]
["137","030904003001","编码型手动报警按钮 带电话插孔","个","4",277.82,57.72,2.05,{"v":191.9,"d":"191.90"},0.06,17.78,8.31]
[null,null,"1.安装方式:距地1.4m安装"]
[null,"B5-1316换","编码型手动报警按钮 带电话插孔","个","4",277.82,57.72,2.05,{"v":191.9,"d":"191.90"},0.06,17.78,8.31]
["138","030904008001","短路隔离器","个","2",271.86,92.03,5.49,{"v":130.9,"d":"130.90"},1.29,28.72,13.43]
[null,"B5-1329换","短路隔离器","个","2",271.86,92.03,5.49,{"v":130.9,"d":"130.90"},1.29,28.72,13.43]
["139","030904007001","火灾警报扬声器","个","10",101.75,21.26,{"v":4,"d":"4.00"},66.09,0.55,6.71,3.14]
[null,null,"1.功率:12V 3W"]
[null,null,"2.安装方式:吸顶"]
[null,"B5-1327换","火灾警报扬声器","个","10",101.75,21.26,{"v":4,"d":"4.00"},66.09,0.55,6.71,3.14]
["140","030904005001","火灾声光警报器","个","4",307.36,44.67,1.71,{"v":240,"d":"240.00"},0.55,13.92,6.51]
[null,null,"1.安装方式:距地2.4m安装"]
[null,"B5-1318换","火灾声光警报器","个","4",307.36,44.67,1.71,{"v":240,"d":"240.00"},0.55,13.92,6.51]
["141","030904003002","消防栓起泵按钮","个","6",237.42,57.72,2.05,{"v":151.5,"d":"151.50"},0.06,17.78,8.31]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第31页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,"B5-1316换","按钮安装 消防栓起泵按钮","个","6",237.42,57.72,2.05,{"v":151.5,"d":"151.50"},0.06,17.78,8.31]
["142","030411004008","管内穿报警线 ZR-RVS-2x1.0","m","597.97",4.33,0.59,0.23,3.24,null,0.18,0.09]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B4-1611换","报警线 ZR-RVS-2x1.0","100m束","5.9797",432.66,59.19,22.73,{"v":324,"d":"324.00"},null,18.22,8.52]
["143","030411004009","管内穿电源线 NH-BV-750V-4","m","1722.16",4.23,{"v":0.5,"d":"0.50"},0.17,3.34,null,0.15,0.07]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B4-1582换","电源线回路  NH-BV-750V-4","100m单线","17.2216",423.27,49.92,{"v":16.9,"d":"16.90"},{"v":333.9,"d":"333.90"},null,15.37,7.18]
["144","030411004010","管内穿消防广播回路 NH-RVVP-250V-2x1.5","m","263.11",{"v":5.4,"d":"5.40"},0.59,0.09,4.42,0.02,0.19,0.09]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B5-0257换","消防广播回路 NH-RVVP-250V-2x1.5","100m","2.6311",540.03,58.92,9.23,441.74,2.43,18.88,8.83]
["145","030411001005","配管","m","1459.05",14.31,{"v":4.9,"d":"4.90"},0.39,6.49,0.22,1.57,0.74]
[null,null,"材质 钢管"]
[null,null,"规格 SC15"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B4-1417换","电线管敷设 砖、混凝土结构暗配 电线管公称口径(mm以内)15","100m","14.5905",{"v":1430.6,"d":"1430.60"},489.58,39.19,{"v":648.9,"d":"648.90"},{"v":21.9,"d":"21.90"},157.43,{"v":73.6,"d":"73.60"}]
["146","030413002002","管道DN25 凿槽及恢复","m","44.00",17.11,9.18,3.31,null,0.32,2.93,1.37]
[null,"B4-2012","凿槽、刨沟  混凝土结构（公称管径15mm以内）","10m","4.400",121.89,73.81,{"v":11.2,"d":"11.20"},null,2.44,23.47,10.97]
[null,"B4-2018","所凿沟槽恢复  沟槽尺寸（公称管径20mm以内）{水泥砂浆 1∶2.5}","10m","4.400",49.18,18.03,21.86,null,0.79,5.79,2.71]
["147","030905001001","自动报警系统调试","系统","1",16399.49,10560.01,289.11,null,537.59,3415.84,1596.94]
[null,"B5-1383","自动报警系统调试 500点以下","系统","1",16399.49,10560.01,289.11,null,537.59,3415.84,1596.94]
[null,null,"应急照明"]
["148","030412001010","带蓄电池应急双头灯","套","13",147.22,15.88,2.75,{"v":121.2,"d":"121.20"},0.15,4.93,2.31]
[null,null,"型号规格 2x5W LED灯 ~220V A型灯具"]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第32页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
[null,null,"距地2.5米安装,5W,90min"]
[null,null,"无墙体位置吊装,距地大于2.2m"]
[null,"B4-1846换","自带电源事故照明灯","10套","1.3",1472.12,158.78,27.47,{"v":1212,"d":"1212.00"},1.48,49.33,23.06]
["149","030412001011","安全出口标志灯","套","6",{"v":165.4,"d":"165.40"},15.88,2.75,139.38,0.15,4.93,2.31]
[null,null,"型号规格  1x3W LED灯 ~220V A型灯具"]
[null,null,"门上0.2米安装,3W,90min"]
[null,"B4-1846换","安全出口标志灯","10套","0.6",1653.92,158.78,27.47,{"v":1393.8,"d":"1393.80"},1.48,49.33,23.06]
["150","030412001012","单向疏散指示灯","套","10",101.77,15.88,2.75,75.75,0.15,4.93,2.31]
[null,null,"型号规格 1x3W LED灯 ~220V A型灯具"]
[null,null,"距地0.5米安装,5W,90min"]
[null,"B4-1846换","单向疏散指示灯","10套","1",1017.62,158.78,27.47,{"v":757.5,"d":"757.50"},1.48,49.33,23.06]
["151","030412001013","双向疏散指示灯","套","1",101.77,15.88,2.75,75.75,0.15,4.93,2.31]
[null,null,"型号规格 1x3W LED灯 ~220V A型灯具"]
[null,null,"安装方式  距地0.5m壁装"]
[null,"B4-1846换","双向疏散指示灯","10套","0.1",1017.62,158.78,27.47,{"v":757.5,"d":"757.50"},1.48,49.33,23.06]
["152","030411004011","管内穿线NH-BV-2.5","m","609.30",4.05,{"v":0.5,"d":"0.50"},0.17,3.16,null,0.15,0.07]
[null,null,"品牌相当于或优于“银杉”"]
[null,"B4-1582换","管内穿线 动力线路 铜芯 导线截面(m㎡以内) 2.5","100m单线","6.093",405.42,49.92,{"v":16.9,"d":"16.90"},316.05,null,15.37,7.18]
["153","030411001006","配管","m","203.10",16.98,5.38,0.46,8.39,0.22,1.72,0.81]
[null,null,"材质 钢管"]
[null,null,"规格 SC20"]
[null,null,"品牌相当于或优于“雄塑”"]
[null,"B4-1418换","电线管敷设 砖、混凝土结构暗配 电线管公称口径(mm以内)20","100m","2.0310",1698.89,538.47,45.95,839.45,{"v":21.9,"d":"21.90"},172.48,80.64]
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]
["工程量清单综合单价分析表"]
["工程名称：广西中医药大学教师教学发展中心装修工程",{"$nulls":8},"第33页 共33页"]
["序号","项目编码","项目名称及项目\r\n特征描述","单位","工程量","综合单价\r\n(元)","综合单价"]
[{"$nulls":6},"人工费","材料费",null,"机械费","管理费","利润","其中:\r\n暂估价"]
[{"$nulls":7},"附材费","主材费"]
["154","030413002003","管道DN20 凿(压)槽及恢复","m","54.00",17.11,9.18,3.31,null,0.32,2.93,1.37]
[null,"B4-2012","凿槽、刨沟  混凝土结构（公称管径20mm以内）","10m","5.400",121.89,73.81,{"v":11.2,"d":"11.20"},null,2.44,23.47,10.97]
[null,"B4-2018","所凿沟槽恢复  沟槽尺寸（公称管径20mm以内）{水泥砂浆 1∶2.5}","10m","5.400",49.18,18.03,21.86,null,0.79,5.79,2.71]
[null,null,"单价措施项目"]
{"$rows_empty":20}
[" ",null,null," ",null,null," ",null,null," "," ",null,"表－09"]